  +------------------------------------------------------------------------+
  |    This report is created by ASTRA32 v.4.20     03-Feb-2025 09:14:49   |
  +------------------------------------------------------------------------+
                                       DESKTOP-O18FSDF
                                       
    Version:                           ASTRA32 - Advanced System Information Tool 4.20
    Registered To:                     Sysinfo Lab
    License Type:                      Professional for 1 computer
    Home Page:                         www.astra32.com
                                       
    Report Date:                       03-Feb-2025
    Report Time:                       09:14:49
    User Name:                         KKV1
                                       
    Disabled Tests:                    UDMA
                                       
                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor 
    Processor:                         AMD Ryzen 5 5600 3500 MHz
    CPU Clock:                         3500.0 MHz (35.0 x 100.0 MHz)
    Level 1 Cache:                     6 x 32 kB + 6 x 32 kB (data+instr.)
    Level 2 Cache:                     6 x 512 kB
    Level 3 Cache:                     1 x 32 MB
  Motherboard
    System Name:                       Micro-Star International Co., Ltd. MS-7A38
    Board Model:                       Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
    BIOS Version:                      American Megatrends International, LLC. B.L0
    BIOS Version:                      AMI BIOS 08.00.10
    Chipset Name:                      AMD B450 (Promontory)
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
    DMI/SMBIOS Version:                2.8
  Memory
    Memory Size:                       15.93 GB
    System Memory:                     16310 MB
    Memory Module:                     8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Memory Module:                     8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
  Storage
    Disk Model:                        Samsung SSD 860 EVO 250GB
    Disk Size:                         238475 MB (232.89 GB)
    Disk Model:                        WDC WD1001FALS-00J7B0
    Disk Size:                         953869 MB (931.51 GB)
    Disk Model:                        HGST HTS541010A9E680
    Disk Size:                         953869 MB (931.51 GB)
    Disk Model:                        Samsung SSD 970 EVO Plus 1TB            
    Disk Size:                         953869 MB (931.51 GB)
    CD/DVD Model:                      ATAPI   DVD W  DH16W1S
    CD/DVD Speed:                      48x (Write: 48x)
  Monitor
    Monitor Vendor:                    AOC International (TPV Technology)
    Monitor Model:                     Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5 (27.0")
  Video Card
    Video Chip Vendor:                 NVIDIA Corporation
    Video Chip:                        GeForce RTX 3060 Ti LHR [GA104]
    Bus Type:                          PCI Express 3.0 x16
    Video Memory Size:                 8 GB GDDR6 (Hynix)
  Sound
    Sound Chip Vendor:                 NVIDIA Corporation
    Sound Chip:                        GA104 High Definition Audio Controller
    Audio Codec Name:                  NVidia GPU GA104 HDMI/DP
  Sound 2
    Sound Chip Vendor:                 Advanced Micro Devices (AMD)
    Sound Chip:                        Starship/Matisse HD Audio Controller
    Audio Codec Name:                  Realtek ALC892
  Sound 3
    Sound Chip Vendor:                 FIFINE
    Sound Chip:                        PC Gaming Dynamic RGB Headset
  Sound 4
    Sound Chip Vendor:                 FIFINE
    Sound Chip:                        Microphone
  Sound 5
    Sound Chip Vendor:                 ASUSTek Computer
    Sound Chip:                        ASUS XONAR SC150 AUDIO DEVICE
  Printer
    Printer Vendor:                    Canon
    Printer Model:                     LaserBase MF3110 Scanner/Printer
  Operating System
    Operating System:                  MS Windows 11 Professional x64 Edition (Version 22H2, 10.0.22621.4317)
    Windows Folder:                    J:\Windows
  Network
    Network Name:                      DESKTOP-O18FSDF
    Network Chip Vendor:               Realtek Semiconductor
    Network Chip:                      RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
    Interface Description:             Realtek PCIe GbE Family Controller
    MAC Address:                       2C-F0-5D-D2-A7-22
  Ports
    LPT Ports:                         LPT1 (0378h) 
    COM Ports:                         COM1 (03F8h) 
                                       
                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
    System Vendor:                     Micro-Star International Co., Ltd.
    Product Name:                      MS-7A38
    Version:                           8.0
    Serial Number:                     To be filled by O.E.M.
    UUID:                              12983CA982A41496AAC82CF05DD2A722
    Wake-up Type:                      Power Switch
    SKU Number:                        To be filled by O.E.M.
    Family:                            To be filled by O.E.M.
  Motherboard
    Motherboard Vendor:                Unknown (0001)
    Vendor URL:                        Unknown
    Board Model:                       Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
    Motherboard ID:                    BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
    Version:                           8.0
    Serial Number:                     07A3880_KB1E018736
    Asset Tag:                         To be filled by O.E.M.
    BIOS Version:                      American Megatrends International, LLC. B.L0
    BIOS Version:                      AMI BIOS 08.00.10
    BIOS Date:                         10/26/2023
    Chipset Name:                      AMD B450 (Promontory)
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
  Onboard Device 1
    Description:                       Broadcom 5762
    Device Type:                       Ethernet
    Status:                            Disabled
  Configuration Options
    To be filled by O.E.M.
  System Enclosure
    Manufacturer:                      Micro-Star International Co., Ltd.
    Type:                              Desktop
    Version:                           8.0
    Serial Number:                     To be filled by O.E.M.
    Asset Tag:                         To be filled by O.E.M.
    Boot-up State:                     Safe
    Power Supply State:                Safe
    Thermal State:                     Safe
    Security Status:                   None
    OEM-defined:                       00000000h
    Height:                            0.0 sm
    Power Cords:                       1
    Contained Element:                 0
                                       
                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU 
    Processor:                         AMD Ryzen 5 5600 3500 MHz
    Coprocessor:                       Internal
    CPU Clock:                         3500.0 MHz
    Level 1 Cache:                     6 x 32 kB + 6 x 32 kB (data+instr.)
    Level 2 Cache:                     6 x 512 kB
    Level 3 Cache:                     1 x 32 MB
    Code Name:                         Vermeer (Zen 3)
    Manufacturing Process:             7 nm
    FSB Clock:                         100.0 MHz
    Multiplier:                        35.0
    Expected Clock:                    3500 MHz
    Overclocking Support:              Unlocked Multiplier
    AMD Core Performance Boost:        Supported (Enabled)
    Max Turbo Clock:                   4450.0 MHz
    Processor Topology:                Nodes: 1, CPU Complexes (CCX): 1, Cores: 6, Threads: 12
    Socket Type:                       Socket AM4
    Instruction Set:                   IA-32, AMD64, MMX, AMDMMX, SSE, SSE2, SSE3, SSSE3
    Instruction Set:                   SSE4.1, SSE4.2, SSE4A, AVX, AVX2, AES, FMA, SHA, AMD-V
    Maximum Temperature (Tjmax):       95 °C (203 °F)
    Core Voltage:                      1.125 V
    Infinity Fabric Clock (FCLK):      1800.0 MHz
    Vendor:                            AuthenticAMD
    Processor Name:                    AMD Ryzen 5 5600 6-Core Processor
    Processor Type:                    Original OEM Processor
    CPUID:                             Family: 15, Model: 1, Stepping: 2
    Ext. Family/Model:                 Family: 10, Model: 2
    CPU Signature:                     00A20F12h
    Number of Cores:                   6
    Logical Cores Count:               12
    Core Stepping:                     VMR-B2
    OPN Code:                          100-000000927, 100-100000927BOX
    Microcode Revision:                A20120Eh
    SMU Firmware Version:              56.76.00
    Power Table Version:               380905h
    Max TDP:                           65 Wattes
    Power Limit:                       76 Wattes
    Thermal Design Current (TDC):      60 Amps
    Electrical Design Current (EDC):   90 Amps
    Transistor Count:                  6240 million
    Die Size:                          81 mm2 + I/O 122 mm2
    Launch Date:                       April, 2022
    Recommended Price (USD):           $199
  Hardware Monitoring
    Core Voltage:                      1.119 V
    Core Voltage (SVI2 TFN):           1.113 V
    SoC Voltage (SVI2 TFN):            1.075 V
    Package Temperature:               53 °C (127 °F)
    CCD1 Temperature:                  53 °C (127 °F)
    SoC Temperature:                   45 °C (113 °F)
    L3 Cache Temperature:              43 °C (109 °F)
    Package Power:                     26.6 Wattes
    Cores Power:                       2.8 Wattes
    SoC Power:                         12.1 Wattes
    VDDIO Mem Power:                   9.2 Wattes
    VDD18 Power:                       0.9 Wattes
    FSB Clock:                         100.0 MHz
  Core 1
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.3 Wattes
    Core Clock:                        3560.0 MHz
    Multiplier:                        35.6
  Core 2
    Temperature Core:                  44 °C (111 °F)
    Core Power:                        0.6 Wattes
    Core Clock:                        3560.0 MHz
    Multiplier:                        35.6
  Core 3
    Temperature Core:                  44 °C (111 °F)
    Core Power:                        0.6 Wattes
    Core Clock:                        4450.0 MHz
    Multiplier:                        44.5
  Core 4
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.0 Wattes
    Core Clock:                        3560.0 MHz
    Multiplier:                        35.6
  Core 5
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.0 Wattes
    Core Clock:                        3560.0 MHz
    Multiplier:                        35.6
  Core 6
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.1 Wattes
    Core Clock:                        3560.0 MHz
    Multiplier:                        35.6
  Instruction Set
    Floating-Point Unit On-Chip:                  [X]
    IA MMX Technology:                            [X]
    SSE Instruction Set:                          [X]
    SSE2 Instruction Set:                         [X]
    SSE3 Instruction Set:                         [X]
    Supplemental SSE3 Instruction Set:            [X]
    SSE4.1 Instruction Set:                       [X]
    SSE4.2 Instruction Set:                       [X]
    Advanced Vector Extensions (AVX):             [X]
    Advanced Vector Extensions 2 (AVX2):          [X]
    AVX-512 Foundation Instructions:              [ ]
    AVX-512 Prefetch Instructions:                [ ]
    AVX-512 Exponential and Reciprocal:           [ ]
    AVX-512 Conflict Detection:                   [ ]
    AVX-512 Byte and Word Instructions:           [ ]
    AVX-512 Doubleword and Quadword:              [ ]
    AVX-512 Vector Length Extensions:             [ ]
    AVX-512 Integer Fused Multiply-Add:           [ ]
    AVX-512 Vector Bit Manipulation:              [ ]
    AVX-512 QVNNI Instructions:                   [ ]
    AVX-512 QFMA Instructions:                    [ ]
    AVX-512 VBMI2 Instructions:                   [ ]
    AVX-512 VNNI Instructions:                    [ ]
    AVX-512 BITALG Instructions:                  [ ]
    Galois Field NI/Affine Transformation:        [ ]
    VEX-encoded AES-NI (VAES):                    [X]
    VEX-encoded PCLMUL (VPCL):                    [X]
    PCOMMIT Instruction:                          [ ]
    CLWB Instruction:                             [X]
    PREFETCHWT1 Instruction:                      [ ]
    Software Guard Extensions (SGX):              [ ]
    SGX Launch Configuration:                     [ ]
    FMA Instructions Set:                         [X]
    AES Instructions Set:                         [X]
    Intel Extended Memory 64 Tech.:               [ ]
    Intel Architecture - 64 (IA-64):              [ ]
    AMD MMX Instruction Extensions:               [X]
    AMD 3DNow! Instructions:                      [ ]
    AMD 3DNow! Extensions:                        [ ]
    AMD 3DNow! Prefetch:                          [X]
    AMD SSE4A Extensions:                         [X]
    AMD eXtended OPeration (XOP):                 [ ]
    AMD Misaligned SSE:                           [X]
    AMD64 Architecture:                           [X]
    Cyrix Extended MMX:                           [ ]
    CMPXCHG8 Instruction Supported:               [X]
    CMPXCHG16 Instruction Supported:              [X]
    Fast System Call:                             [X]
    Conditional Move Instruction:                 [X]
    CLFLUSH Insruction Supported:                 [X]
    Fast Save and Restore:                        [X]
    Monitor/MWAIT Instructions:                   [X]
    SYSCALL/SYSRET Instructions:                  [X]
    LAHF/SAHF Instructions:                       [X]
    POPCNT Insruction Supported:                  [X]
    XSAVE Insructions Supported:                  [X]
    OS Supports XSAVE Instructions:               [X]
    PCLMULQDQ Instruction Supported:              [X]
    MOVBE Insruction Supported:                   [X]
    F16C Insruction Supported:                    [X]
    RDTSCP Insruction Supported:                  [X]
    RDRAND Insruction Supported:                  [X]
    (RD/WR)(FS/GS) BASE Instructions:             [X]
    Bit Manipulation 1 Instructions:              [X]
    Bit Manipulation 1 Instructions:              [X]
    Enhanced REP MOVSB/STOSB:                     [X]
    INVPCID Instruction:                          [X]
    XSAVEOPT Instruction:                         [X]
    RDSEED Instruction:                           [X]
    ADCX/ADOX Instructions:                       [X]
    CLAC/STAC Instructions:                       [X]
    SCLFLUSHOPT Instruction:                      [X]
    RDPID Instruction:                            [X]
    VPOPCNT[D/Q] Instructions:                    [ ]
    Fast Short REP MOV Instruction:               [X]
    PCONFIG Instruction:                          [ ]
    WBNOINVD Instruction:                         [X]
    WaitPKG Instructions:                         [ ]
    CLDEMOTE Instruction:                         [ ]
    MOVDIRI Instruction:                          [ ]
    MOVDIRI64B Instruction:                       [ ]
    RDPRU Instruction:                            [X]
    MCOMMIT Instruction:                          [ ]
    AMD Fast Save and Restore:                    [X]
    AMD SKINIT, STGI, DEV Supported:              [X]
    AMD Light Weight Profiling (LWP):             [ ]
    AMD FMA4 Insruction Supported:                [ ]
    AMD TBM Insruction Supported:                 [ ]
    AMD MONITORX/MWAITX Instructions:             [X]
    AMD CLZERO Instruction:                       [X]
  Processor Features
    Hypervisor Present:                           [ ]
    Virtual Mode Extension:                       [X]
    Debugging Extension:                          [X]
    Page Size Extension:                          [X]
    Time Stamp Counter:                           [X]
    Model Specific Registers:                     [X]
    Physical Address Extension:                   [X]
    Machine Check Exception:                      [X]
    On-chip APIC Hardware Supported:              [X]
    Memory Type Range Registers:                  [X]
    Page Global Enable:                           [X]
    Machine Check Architecture:                   [X]
    Page Attribute Table:                         [X]
    36-bit Page Size Extension:                   [X]
    Processor Serial Number:                      [ ]
    Debug Store:                                  [ ]
    64-bit Debug Store:                           [ ]
    Self-Snoop:                                   [ ]
    Hyper-Threading Technology:                   [X]
    Pending Break Enable:                         [ ]
    CPL-Qualified Debug Store:                    [ ]
    L1 Context ID:                                [ ]
    Send Task Priority Messages:                  [ ]
    Direct Cache Access:                          [ ]
    Performance Capabilities MSR:                 [ ]
    x2APIC Architecture:                          [X]
    Advanced Bit Manipulation:                    [X]
    OS Visible Workaround:                        [X]
    Instruction Based Sampling:                   [X]
    1-GB Large Page:                              [X]
    Process Context Identifiers:                  [ ]
    Time Stamp Counter Deadline:                  [ ]
    Time Stamp Counter Adjust:                    [ ]
    Intel Virtualization Technology:              [ ]
    Intel Trusted Execution Technology:           [ ]
    Supervisor Mode Execution Protection:         [X]
    Hardware Lock Elision:                        [ ]
    Restricted Transactional Memory:              [ ]
    Quality of Service Monitoring:                [X]
    Quality of Service Enforcement:               [X]
    Deprecated FPU CS and FPU DS:                 [ ]
    Memory Protection Extensions (MPX):           [ ]
    Processor Trace (PT):                         [ ]
    Secure Hash Algorithm Ext. (SHA):             [X]
    Debug Interface MSR:                          [ ]
    User-Mode Instruction Prevention:             [X]
    Protection Keys for User-Mode Pages:          [X] disabled
    5 Level Page Table:                           [ ]
    Total Memory Encryption (TME):                [ ]
    Speculation Control (IBRS and IBPB):          [ ]
    Single Thread Indirect Branch Predictors:     [ ]
    L1 Data Cache (L1D) Flush:                    [ ]
    ARCH_CAPABILITIES MSR:                        [ ]
    Speculative Store Bypass Disable (SSBD):      [ ]
    AMD Core Performance Boost:                   [X] enabled
    Intel Turbo Boost Max Technology 3.0:         [ ]
    AMD No-execute Page Protection:               [X]
    Hybrid Processor:                             [ ]
    AMD Secure Virtual Machine:                   [X]
    AMD Model-Specific Registers:                 [X]
    AMD Multiprocessing Capable:                  [ ]
    AMD CMP Legacy Mode:                          [X]
    AMD CR8 in Legacy Mode:                       [X]
    AMD Ext. APIC Register Space:                 [X]
    AMD Watchdog Timer:                           [X]
    AMD Translation Cache Extension:              [X]
    AMD NodeID MSR:                               [ ]
    AMD Topology Extensions:                      [X]
    AMD Core Performance Counter Ext.:            [X]
    AMD NB Performance Counter Ext.:              [X]
    AMD Streaming Performance Monitor:            [ ]
    AMD Data Breakpoint Extension:                [X]
    AMD Performance TSC:                          [ ]
    AMD L2I Performance Counter Ext.:             [X]
    AMD IRPERF Performance Counter:               [X]
    AMD Always Save/Restore FP Error Pointers:    [X]
    AMD Indirect Branch Prediction Barrier:       [X]
    AMD Indirect Branch Restricted Speculation:   [X]
    AMD IBRS Always On Mode:                      [ ]
    AMD IBRS Preferred:                           [X]
    AMD Single Thread Indirect Branch Predictor:  [X]
    AMD STIBP Always On Mode:                     [X]
    AMD Speculative Store Bypass Disable (SSBD):  [X]
    AMD SSBD Not Needed:                          [ ]
    AMD VIRT_SPEC_CTRL MSR:                       [ ]
  Power Management
    ACPI Supported:                               [ ]
    Thermal Monitor Supported:                    [ ]
    Thermal Monitor 2:                            [ ]
    Enhanced SpeedStep Technology:                [ ]
    Digital Thermal Sensor:                       [ ]
    Always Running APIC Timer:                    [X]
    Invariant TSC:                                [X]
    Power Limit Notification:                     [ ]
    Extended Clock Modulation Duty:               [ ]
    Package Thermal Management:                   [ ]
    Hardware Coordination Feedback:               [X]
    ACNT2 Capability:                             [ ]
    Performance-Energy Bias:                      [ ]
    Hardware-Managed P-State Base Support:        [ ]
    Hardware Duty Cycle Programming (HDC):        [ ]
    AMD Temperature Sensor:                       [X]
    AMD Frequency ID Control:                     [ ]
    AMD Voltage ID Control:                       [ ]
    AMD Thermal Trip:                             [X]
    AMD Thermal Monitoring:                       [X]
    AMD Software Thermal Control:                 [ ]
    AMD 100MHz Multiplier Steps:                  [ ]
    AMD Hardware P-State Control:                 [X]
    AMD Effective Frequency Interface:            [X]
    AMD Processor Feedback Interface:             [ ]
    AMD Processor Accumulator:                    [ ]
    AMD Connected Standby:                        [X]
    AMD Running Average Power Limit:              [X]
    AMD MCA Overflow Recovery:                    [X]
    AMD Software Uncorr. Error Containment/Recovery:[X]
    AMD Hardware Assert (HWA):                    [ ]
    AMD Scalable MCA:                             [X]
                                       
                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Data Cache
    Size:                              6 x 32 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    TLB 4K Pages:                      
      Number of Entries:               64
      Associativity:                   full
    TLB 2/4M Pages:                    
      Number of Entries:               64
      Associativity:                   full
  Level 1 Instruction Cache
    Size:                              6 x 32 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    TLB 4K Pages:                      
      Number of Entries:               64
      Associativity:                   full
    TLB 2/4M Pages:                    
      Number of Entries:               64
      Associativity:                   full
  Level 2 Cache
    Size:                              6 x 512 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    Data TLB 4K Pages:                 
      Number of Entries:               2048
      Associativity:                   8-way
    Instr. TLB 4K Pages:               
      Number of Entries:               512
      Associativity:                   4-way
    Data TLB 2/4M Pages:               
      Number of Entries:               2048
      Associativity:                   4-way
    Instr. TLB 2/4M Pages:             
      Number of Entries:               512
      Associativity:                   2-way
  Level 3 Cache
    Size:                              1 x 32 MB
    Associativity:                     16-way
    Lines per Tag:                     1
    Line Size:                         64 byte
                                       
                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor 
    Processor Vendor:                  Advanced Micro Devices, Inc.
    Processor Version:                 AMD Ryzen 5 5600 6-Core Processor
    Current Speed:                     3500 MHz
    External Clock:                    100 MHz
    Voltage:                           1.1 V
    Processor Upgrade:                 Socket AM4
    Processor Status:                  CPU Enabled
    Socket Designation:                AM4
    Processor Type:                    Central Processor
    Processor Family:                  AMD Zen
    Processor ID1:                     00A20F12h
    Processor ID2:                     178BFBFFh
    Max Speed:                         4450 MHz
    Socket Status:                     CPU Socket Populated
    Serial Number:                     Unknown
    Asset Tag:                         Unknown
    Part Number:                       Unknown
    CPU Core Count:                    6 (Enabled: 6)
    CPU Thread Count:                  12
    Structure Length:                  30h
                                       
                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
    Installed Size:                    384 kB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L1 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                384 kB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     8-way Set-Associative
    Structure Length:                  13h
  Level 2 Cache
    Installed Size:                    3 MB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L2 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                3 MB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     8-way Set-Associative
    Structure Length:                  13h
  Level 3 Cache
    Installed Size:                    32 MB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L3 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                32 MB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     16-way Set-Associative
    Structure Length:                  13h
                                       
                  +-----------------------------------------+
                  |                 Chipset                 |
                  +-----------------------------------------+
  Chipset
    Chipset Name:                      AMD B450
    Code Name:                         Promontory
    Chipset Type:                      Single Chip: Southbridge-only
    Manufacturing Process:             55 nm
    Launch Date:                       March, 2018
  Northbridge
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Code Name:                         Vermeer (Zen 3)
    Location:                          CPU Integrated
    Infinity Fabric Clock (FCLK):      1800.0 MHz
    Manufacturing Process:             7 nm
    Hardware ID:                       VEN_1022&DEV_1480
    Revision:                          00h
    Stepping:                          VMR-B2
  Memory Controller
    Current Memory Type:               DDR4-3600
    Supported Memory Types:            DDR4-2667, DDR4-2933, DDR4-3200
    Maximum Memory Amount:             128 GB
    Current Controller Mode:           Dual-channel (128-bit)
    Supported Controller Mode:         Dual-channel (128-bit)
    Channel 0 DIMM A:                  8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Channel 1 DIMM A:                  8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Current Memory Clock:              1800.0 MHz (Effective: 3600.0 MHz)
    FSB:DRAM Ratio:                    1:18
    Memory Bandwidth:                  56.3 GB/s
    Memory Controller Clock (UCLK):    1800.0 MHz
    ECC:                               [X] disabled
    ECC Scrubbing:                     [ ]
    Mirroring Mode (RAID):             [ ]
    ECC Chipkill:                      [ ]
  Timings
    CAS Latency (CL):                  16.0
    RAS to CAS Delay (tRCD):           20
    RAS Precharge Time (tRP):          20
    RAS Active Time (tRAS):            39
    Row Cycle Time (tRC):              83
    Row Refresh Cycle Time (tRFC):     631
    Command Rate (CR):                 1T
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Connected Device:                  Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x8 8.0 GT/s (Current: x4 8.0 GT/s)
    Bus Bandwidth:                     7.9 GB/sec (Current: 3.9 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Connected Device 1:                AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
    Connected Device 2:                AMD 400 Series Chipset SATA Controller
    Connected Device 3:                AMD 400 Series Chipset PCIe Bridge
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x16 8.0 GT/s (Current: x16 5.0 GT/s)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Connected Device 1:                NVIDIA GeForce RTX 3060 Ti LHR [GA104]
    Connected Device 2:                NVIDIA GA104 High Definition Audio Controller
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Bus Type:                          PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Connected Device:                  AMD Starship/Matisse PCIe Dummy Function
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Bus Type:                          PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Connected Device 1:                AMD Starship/Matisse Reserved SPP
    Connected Device 2:                AMD Starship/Matisse Cryptographic Coprocessor PSPCPP
    Connected Device 3:                AMD Matisse USB 3.0 Host Controller
    Connected Device 4:                AMD Starship/Matisse HD Audio Controller
    Connected Device 5:                Motherboard registers
  Southbridge
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
    Bus Type:                          PCI Express
    Manufacturing Process:             55 nm
    Hardware ID:                       VEN_1022&DEV_790E
    Revision:                          51h
    Top Marking:                       218-0891011
    Package Type:                      LFBGA-583
    Connected Device 1:                AT Interrupt Controller
    Connected Device 2:                Motherboard registers
    Connected Device 3:                Standard LPT printer port
    Connected Device 4:                AT DMA Controller
    Connected Device 5:                16550A-compatible COM port
    Connected Device 6:                AT standard speaker sound
    Connected Device 7:                AT Timer
    Connected Device 8:                AT Real-Time Clock
  Integrated Sound
    Audio Controller:                  AMD Starship/Matisse HD Audio Controller
    Audio Codec Name:                  Realtek ALC892
    Controller Type:                   High Definition Audio
    Hardware ID:                       VEN_1022&DEV_1487
    Revision:                          00h
  Integrated Storage
    Storage Controller:                AMD 400 Series Chipset SATA Controller
    Controller Type:                   Serial ATA
    Hardware ID:                       VEN_1022&DEV_43C8
    Revision:                          01h
                                       
                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
    BIOS Version:                      AMI BIOS 08.00.10
    BIOS Type:                         UEFI
    BIOS Date:                         12/24/18
    BIOS Copyright:                    12/24/18(C)2010 American Megatrends, Inc. All Rights Reserved
    Motherboard ID:                    BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
    BIOS ID:                           63-0100-000001-00101111-122418-Chipset
    AMI BIOS Tag:                      0AAAA000
    BIOS Size:                         512 kB
    Processor:                         686
    Chipset ID:                        Chipset
    BIOS Revision:                     0100
    PnP Version:                       1.0
    ACPI Version:                      2.0+ (ALASKA)
    MCFG Address:                      F0000000h
    MP Specification Ver.:             Not Supported
    DMI/SMBIOS Version:                2.8
    DMI/SMBIOS Structures:             62
  SMBIOS
    BIOS Vendor:                       American Megatrends International, LLC.
    BIOS Version:                      B.L0
    BIOS Date:                         10/26/2023
    BIOS ROM Size:                     16 MB
    System BIOS Version:               5.17
    Starting Segment:                  F000h
    Structure Length:                  1Ah
  Bus Supported
    PCI is Supported:                             [X]
    AGP is Supported:                             [ ]
    USB is Supported:                             [X]
    ISA is Supported:                             [ ]
    VLBus is Supported:                           [ ]
    MCA is Supported:                             [ ]
    EISA is Supported:                            [ ]
    PC Card is Supported:                         [ ]
  Boot Options
    Selectable Boot:                              [X]
    Boot From CD:                                 [X]
    ATAPI ZIP Drive Boot:                         [ ]
    LS-120 Boot:                                  [ ]
    BIOS Boot Specification:                      [X]
    Boot From PC Card:                            [ ]
    Network Service Boot Supported:               [ ]
    I2O Boot:                                     [ ]
    1394 Boot:                                    [ ]
  BIOS Features
    BIOS Characteristics:                         [X]
    ACPI Supported:                               [ ]
    PnP is Supported:                             [ ]
    APM is Supported:                             [ ]
    ESCD Support:                                 [ ]
    Enhanced Disk Drive (EDD):                    [X]
    BIOS is Upgradeable (Flash):                  [X]
    BIOS ROM is Socketed:                         [X]
    BIOS Shadowing is Allowed:                    [X]
    Smart Battery Supported:                      [ ]
    Targeted Content Distribution:                [X]
    UEFI Specification is Supported:              [X]
    Virtual Machine:                              [ ]
    Int 13h - 5.25"/360kB Floppy:                 [X]
    Int 13h - 5.25"/1.2MB Floppy:                 [X]
    Int 13h - 3.5"/720kB Floppy:                  [X]
    Int 13h - 3.5"/2.88MB Floppy:                 [X]
    Int 5h, Print Screen Service:                 [X]
    Int 9h, 8042 Keyboard Services:               [X]
    Int 14h, Serial Services:                     [X]
    Int 17h, Printer Services:                    [X]
    Int 10h, CGA/Mono Video Services:             [X]
    Int 13h - Floppy for NEC 9800:                [X]
    Int 13h - Floppy for Toshiba:                 [X]
    NEC PC-98:                                    [ ]
  ROM Extension
    Adapter Vendor:                    Intel Corporation
    Adapter Name:                      Realtek PXE B25 D00
    BIOS Version:                      PXE-EC6: UNDI driver image is invalid.
    BIOS Copyright:                    Copyright (C) 1997-2000  Intel Corporation
    Device Class:                      Network
    ROM Address:                       CF80h
    BIOS ROM Size:                     4 kB
  ROM Extension
    Device Name:                       NVIDIA GeForce RTX 3060 Ti LHR [GA104]
    BIOS Version:                      Version 94.04.46.00.D2
    BIOS Copyright:                    Copyright (C) 1996-2021 NVIDIA Corp.
    Device Class:                      Display
    ROM Address:                       C000h
    BIOS ROM Size:                     61 kB
  OEM SMBIOS Strings
    To be filled by O.E.M.
  Other SMBIOS Structures
    System Boot Information (32)
    Unknown (44)
    TPM Device (43)
    32-bit Memory Error Information (18)
    Memory Array Mapped Address (19)
    Memory Array Mapped Address (19)
    32-bit Memory Error Information (18)
    32-bit Memory Error Information (18)
    Memory Device Mapped Address (20)
    32-bit Memory Error Information (18)
    32-bit Memory Error Information (18)
    Memory Device Mapped Address (20)
    Unknown (143)
                                       
                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  Bus: 00h, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1480h):                    Starship/Matisse Root Complex
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1480
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 0, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1480&SUBSYS_7A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1480&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 00h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1481h):                    Starship/Matisse IOMMU
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (08h):                       System Peripheral
    SubClass (06h):                    IOMMU
    Hardware ID:                       VEN_1022&DEV_1481
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 01h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 1, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 01h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device:                            Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FC800000h - FC8FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  1
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Port
    Device Class:                      System
    Device Location:                   PCI bus 0, device 1, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1483&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 01h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device 1:                          AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
    Device 2:                          AMD 400 Series Chipset SATA Controller
    Device 3:                          AMD 400 Series Chipset PCIe Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC500000h - FC7FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x8 (Current: x4)
    Bus Bandwidth:                     7.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Port
    Device Class:                      System
    Device Location:                   PCI bus 0, device 1, function 3
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1483&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 02h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 2, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 03h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 3, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 03h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device 1:                          NVIDIA GeForce RTX 3060 Ti LHR [GA104]
    Device 2:                          NVIDIA GA104 High Definition Audio Controller
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     E000h - EFFFh
    Memory Address:                    FB000000h - FC0FFFFFh
    Memory Address:                    D0000000h - E1FFFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Port
    Device Class:                      System
    Device Location:                   PCI bus 0, device 3, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1483&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 04h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 4, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 05h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 5, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 07h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 7, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 07h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1484h):                    Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device:                            AMD Starship/Matisse PCIe Dummy Function
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Port
    Device Class:                      System
    Device Location:                   PCI bus 0, device 7, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1484&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 08h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 8, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 08h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1484h):                    Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device 1:                          AMD Starship/Matisse Reserved SPP
    Device 2:                          AMD Starship/Matisse Cryptographic Coprocessor PSPCPP
    Device 3:                          AMD Matisse USB 3.0 Host Controller
    Device 4:                          AMD Starship/Matisse HD Audio Controller
    Device 5:                          Motherboard registers
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FC200000h - FC4FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Port
    Device Class:                      System
    Device Location:                   PCI bus 0, device 8, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1484&REV_00
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 14h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (790Bh):                    Hudson SMBus Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (0Ch):                       Serial
    SubClass (05h):                    SMBus Controller
    Hardware ID:                       VEN_1022&DEV_790B
    Revision:                          61h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Medium
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [X]
  Device Resources
    SMBus Port:                        0B00h
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices, Inc
    Device Description:                AMD SMBus
    Device Class:                      System
    Device Location:                   PCI bus 0, device 20, function 0
    Driver Provider:                   Advanced Micro Devices, Inc
    Driver Version:                    5.12.0.38
    Driver Date:                       9-15-2022
    Inf File:                          oem3.inf
    Hardware ID:                       PCI\VEN_1022&DEV_790B&SUBSYS_7A381462&REV_61
    Compatible ID:                     PCI\VEN_1022&DEV_790B&REV_61
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 14h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (790Eh):                    B450 Fusion Controller Hub (FCH)
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (06h):                       Bridge
    SubClass (01h):                    PCI/ISA
    Hardware ID:                       VEN_1022&DEV_790E
    Revision:                          51h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Connected Devices
    Device 1:                          AT Interrupt Controller
    Device 2:                          Motherboard registers
    Device 3:                          Standard LPT printer port
    Device 4:                          AT DMA Controller
    Device 5:                          16550A-compatible COM port
    Device 6:                          AT standard speaker sound
    Device 7:                          AT Timer
    Device 8:                          AT Real-Time Clock
  Device Properties
    Device Timing:                     Medium
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [X]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard ISA bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 20, function 3
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Service Name:                      msisadrv
    Hardware ID:                       PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
    Compatible ID:                     PCI\VEN_1022&DEV_790E&REV_51
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1440h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 0
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1440
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1440&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1441h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 1
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1441
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1441&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1442h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 2
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1442
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 2
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1442&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1443h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 3
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1443
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 3
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1443&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 04h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1444h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 4
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1444
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 4
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1444&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 05h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1445h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 5
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1445
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 5
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1445&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 06h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1446h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 6
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1446
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 6
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1446&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 00h, Device: 18h, Function: 07h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1447h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 7
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1447
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     PCI Bus Host Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI standard host CPU bridge
    Device Class:                      System
    Device Location:                   PCI bus 0, device 24, function 7
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       PCI\VEN_1022&DEV_1447&SUBSYS_00000000&REV_00
    Compatible ID:                     PCI\VEN_1022&CC_060000
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  Bus: 01h, Device: 00h, Function: 00h         
    Vendor (144Dh):                    Samsung Electronics Co Ltd
    Device (A808h):                    NVMe SSD Controller SM981/PM981/PM983
    Subsys Vendor (144Dh):             Samsung Electronics Co Ltd
    Subsystem ID (A801h):              SSD 970 EVO/PRO
    Class (01h):                       Storage
    SubClass (08h):                    Non-Volatile memory controller
    Hardware ID:                       VEN_144D&DEV_A808
    Revision:                          00h
    Interface:                         02h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Connected Devices
    Device:                            Samsung SSD 970 EVO Plus 1TB
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC800000h - FC803FFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Standard NVM Express Controller
    Device Description:                Standard NVM Express Controller
    Device Class:                      SCSIAdapter
    Device Location:                   PCI bus 1, device 0, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          stornvme.inf
    Service Name:                      stornvme
    Hardware ID:                       PCI\VEN_144D&DEV_A808&SUBSYS_A801144D&REV_00
    Compatible ID:                     PCI\VEN_144D&DEV_A808&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 03h, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43D5h):                    400 Series Chipset USB 3.1 xHCI Compliant Host Controller
    Subsys Vendor (1B21h):             ASMedia Technology Inc.
    Subsystem ID (1142h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1022&DEV_43D5
    Revision:                          01h
    Interface:                         30h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Connected Devices
    Device 1:                          Logitech G102 LIGHTSYNC Gaming Mouse
    Device 2:                          FIFINE PC Gaming Dynamic RGB Headset
    Device 3:                          FIFINE Microphone
    Device 4:                          Canon LaserBase MF3110 Scanner/Printer
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC7A0000h - FC7A7FFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Generic USB xHCI Host Controller
    Device Description:                USB xHCI Compliant Host Controller
    Friendly Name:                     AMD USB 3.10 eXtensible Host Controller - 1.10 (Microsoft)
    Device Class:                      USB
    Device Location:                   PCI bus 3, device 0, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       5-21-2024
    Inf File:                          usbxhci.inf
    Service Name:                      USBXHCI
    Hardware ID:                       PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43D5&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 03h, Device: 00h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C8h):                    400 Series Chipset SATA Controller
    Subsys Vendor (1B21h):             ASMedia Technology Inc.
    Subsystem ID (1062h):              Unknown
    Class (01h):                       Storage
    SubClass (06h):                    Serial ATA
    Hardware ID:                       VEN_1022&DEV_43C8
    Revision:                          01h
    Interface:                         01h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Connected Devices
    Device 1:                          Samsung SSD 860 EVO 250GB
    Device 2:                          WDC WD1001FALS-00J7B0
    Device 3:                          HGST HTS541010A9E680
    Device 4:                          ATAPI   DVD W  DH16W1S
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC780000h - FC79FFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Standard SATA AHCI Controller
    Device Description:                Standard SATA AHCI Controller
    Device Class:                      HDC
    Device Location:                   PCI bus 3, device 0, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.2506
    Driver Date:                       6-21-2006
    Inf File:                          mshdc.inf
    Service Name:                      storahci
    Hardware ID:                       PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C8&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 03h, Device: 00h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C6h):                    400 Series Chipset PCIe Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C6
    Revision:                          01h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Connected Devices
    Device 1:                          AMD 400 Series Chipset PCIe Port
    Device 2:                          AMD 400 Series Chipset PCIe Port
    Device 3:                          AMD 400 Series Chipset PCIe Port
    Device 4:                          AMD 400 Series Chipset PCIe Port
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC500000h - FC6FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTC#
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Upstream Port of PCI-E Switch
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Upstream Switch Port
    Device Class:                      System
    Device Location:                   PCI bus 3, device 0, function 2
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C6&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 20h, Device: 04h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
    Parent Device:                     AMD 400 Series Chipset PCIe Bridge
  Connected Devices
    Device:                            Realtek Semiconductor RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC600000h - FC6FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  4
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Downstream Switch Port
    Device Class:                      System
    Device Location:                   PCI bus 32, device 4, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C7&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
                                       
  Bus: 20h, Device: 05h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
    Parent Device:                     AMD 400 Series Chipset PCIe Bridge
  Connected Devices
    Device:                            ASMedia Technology Inc. ASM1042A USB 3.0 Host Controller
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  5
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Downstream Switch Port
    Device Class:                      System
    Device Location:                   PCI bus 32, device 6, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C7&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
                                       
  Bus: 20h, Device: 06h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
    Parent Device:                     AMD 400 Series Chipset PCIe Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FC500000h - FC5FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.5 GB/sec)
    Link Port Number:                  6
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Downstream Switch Port
    Device Class:                      System
    Device Location:                   PCI bus 32, device 5, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C7&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
                                       
  Bus: 20h, Device: 07h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
    Parent Device:                     AMD 400 Series Chipset PCIe Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  7
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Downstream Switch Port
    Device Class:                      System
    Device Location:                   PCI bus 32, device 7, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
    Compatible ID:                     PCI\VEN_1022&DEV_43C7&REV_01
    Parent ID:                         PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
                                       
  Bus: 25h, Device: 00h, Function: 00h         
    Vendor (10ECh):                    Realtek Semiconductor
    Device (8168h):                    RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (02h):                       Network
    SubClass (00h):                    Ethernet
    Hardware ID:                       VEN_10EC&DEV_8168
    Revision:                          15h
    Interface:                         00h
    Parent Device:                     AMD 400 Series Chipset PCIe Port
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC604000h - FC604FFFh
    Memory Address:                    FC600000h - FC603FFFh
  PCI-E Capabilities
    PCI Express Version:               1.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        2.5 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.25 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Realtek
    Device Description:                Realtek PCIe GbE Family Controller
    Friendly Name:                     Realtek PCIe GbE Family Controller
    Device Class:                      Net
    Device Location:                   PCI bus 37, device 0, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    1.0.0.14
    Driver Date:                       2-1-2021
    Inf File:                          rtcx21x64.inf
    Service Name:                      rtcx21
    Hardware ID:                       PCI\VEN_10EC&DEV_8168&SUBSYS_7A381462&REV_15
    Compatible ID:                     PCI\VEN_10EC&DEV_8168&REV_15
    Parent ID:                         PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
                                       
  Bus: 27h, Device: 00h, Function: 00h         
    Vendor (1B21h):                    ASMedia Technology Inc.
    Device (1142h):                    ASM1042A USB 3.0 Host Controller
    Subsys Vendor (1043h):             ASUSTeK Computer Inc
    Subsystem ID (86A0h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1B21&DEV_1142
    Revision:                          00h
    Interface:                         30h
    Parent Device:                     AMD 400 Series Chipset PCIe Port
  Connected Devices
    Device:                            ASUSTek Computer ASUS XONAR SC150 AUDIO DEVICE
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC500000h - FC507FFFh
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        5.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.5 GB/sec)
    Link Port Number:                  1
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Generic USB xHCI Host Controller
    Device Description:                USB xHCI Compliant Host Controller
    Friendly Name:                     ASMedia USB 3.0 eXtensible Host Controller - 1.0 (Microsoft)
    Device Class:                      USB
    Device Location:                   PCI bus 39, device 0, function 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       5-21-2024
    Inf File:                          usbxhci.inf
    Service Name:                      USBXHCI
    Hardware ID:                       PCI\VEN_1B21&DEV_1142&SUBSYS_86A01043&REV_00
    Compatible ID:                     PCI\VEN_1B21&DEV_1142&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
                                       
  Bus: 29h, Device: 00h, Function: 00h         
    Vendor (10DEh):                    NVIDIA Corporation
    Device (2489h):                    GeForce RTX 3060 Ti LHR [GA104]
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (3972h):              MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
    Class (03h):                       Display
    SubClass (00h):                    VGA
    Hardware ID:                       VEN_10DE&DEV_2489
    Revision:                          A1h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Connected Devices
    Device:                            AOC International (TPV Technology) Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FB000000h - FBFFFFFFh
    Memory Address:                    D0000000h - DFFFFFFFh
    Memory Address:                    E0000000h - E1FFFFFFh
    Base I/O Port:                     0000E000h - 0000E07Fh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      NVIDIA
    Device Description:                NVIDIA GeForce RTX 3060 Ti
    Device Class:                      Display
    Device Location:                   PCI bus 41, device 0, function 0
    Driver Provider:                   NVIDIA
    Driver Version:                    32.0.15.7216
    Driver Date:                       1-26-2025
    Inf File:                          oem13.inf
    Service Name:                      nvlddmkm
    Hardware ID:                       PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
    Compatible ID:                     PCI\VEN_10DE&DEV_2489&REV_A1
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 29h, Device: 00h, Function: 01h         
    Vendor (10DEh):                    NVIDIA Corporation
    Device (228Bh):                    GA104 High Definition Audio Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (3972h):              Unknown
    Class (04h):                       Multimedia
    SubClass (03h):                    High Definition Audio
    Hardware ID:                       VEN_10DE&DEV_228B
    Revision:                          A1h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse GPP Bridge
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC080000h - FC083FFFh
  Sound
    Audio Codec Name:                  NVidia GPU GA104 HDMI/DP
    Controller Type:                   High Definition Audio
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                High Definition Audio Controller
    Device Class:                      System
    Device Location:                   PCI bus 41, device 0, function 1
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3810
    Driver Date:                       6-18-2024
    Inf File:                          hdaudbus.inf
    Service Name:                      HDAudBus
    Hardware ID:                       PCI\VEN_10DE&DEV_228B&SUBSYS_39721462&REV_A1
    Compatible ID:                     PCI\VEN_10DE&DEV_228B&REV_A1
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
  Bus: 2Ah, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (148Ah):                    Starship/Matisse PCIe Dummy Function
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (13h):                       Non-Essential Instrumentation
    SubClass (00h):                    Unknown
    Hardware ID:                       VEN_1022&DEV_148A
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices
    Device Description:                AMD PCI
    Device Class:                      System
    Device Location:                   PCI bus 42, device 0, function 0
    Driver Provider:                   Advanced Micro Devices
    Driver Version:                    1.0.0.90
    Driver Date:                       10-27-2022
    Inf File:                          oem1.inf
    Service Name:                      AMDPCIDev
    Hardware ID:                       PCI\VEN_1022&DEV_148A&SUBSYS_7A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_148A&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
  Bus: 2Bh, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1485h):                    Starship/Matisse Reserved SPP
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (13h):                       Non-Essential Instrumentation
    SubClass (00h):                    Unknown
    Hardware ID:                       VEN_1022&DEV_1485
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices
    Device Description:                AMD PCI
    Device Class:                      System
    Device Location:                   PCI bus 43, device 0, function 0
    Driver Provider:                   Advanced Micro Devices
    Driver Version:                    1.0.0.90
    Driver Date:                       10-27-2022
    Inf File:                          oem1.inf
    Service Name:                      AMDPCIDev
    Hardware ID:                       PCI\VEN_1022&DEV_1485&SUBSYS_7A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1485&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
  Bus: 2Bh, Device: 00h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1486h):                    Starship/Matisse Cryptographic Coprocessor PSPCPP
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (10h):                       En/Decryption
    SubClass (80h):                    Other
    Hardware ID:                       VEN_1022&DEV_1486
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC300000h - FC3FFFFFh
    Memory Address:                    FC408000h - FC409FFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices Inc.
    Device Description:                AMD PSP 11.0 Device
    Device Class:                      SecurityDevices
    Device Location:                   PCI bus 43, device 0, function 1
    Driver Provider:                   Advanced Micro Devices Inc.
    Driver Version:                    4.13.0.0
    Driver Date:                       3-6-2020
    Inf File:                          oem16.inf
    Service Name:                      amdpsp
    Hardware ID:                       PCI\VEN_1022&DEV_1486&SUBSYS_7A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1486&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
  Bus: 2Bh, Device: 00h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (149Ch):                    Matisse USB 3.0 Host Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1022&DEV_149C
    Revision:                          00h
    Interface:                         30h
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Connected Devices
    Device:                            Evision RGB Gaming Mechanical Keyboard
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC200000h - FC2FFFFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Generic USB xHCI Host Controller
    Device Description:                USB xHCI Compliant Host Controller
    Friendly Name:                     AMD USB 3.10 eXtensible Host Controller - 1.10 (Microsoft)
    Device Class:                      USB
    Device Location:                   PCI bus 43, device 0, function 3
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       5-21-2024
    Inf File:                          usbxhci.inf
    Service Name:                      USBXHCI
    Hardware ID:                       PCI\VEN_1022&DEV_149C&SUBSYS_7A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_149C&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
  Bus: 2Bh, Device: 00h, Function: 04h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1487h):                    Starship/Matisse HD Audio Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (9A38h):              Unknown
    Class (04h):                       Multimedia
    SubClass (03h):                    High Definition Audio
    Hardware ID:                       VEN_1022&DEV_1487
    Revision:                          00h
    Interface:                         00h
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC400000h - FC407FFFh
  Sound
    Audio Codec Name:                  Realtek ALC892
    Controller Type:                   High Definition Audio
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                High Definition Audio Controller
    Device Class:                      System
    Device Location:                   PCI bus 43, device 0, function 4
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3810
    Driver Date:                       6-18-2024
    Inf File:                          hdaudbus.inf
    Service Name:                      HDAudBus
    Hardware ID:                       PCI\VEN_1022&DEV_1487&SUBSYS_9A381462&REV_00
    Compatible ID:                     PCI\VEN_1022&DEV_1487&REV_00
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 3
    Memory Type:                       8 GB DDR4-3602 (1801 MHz) SDRAM
    Manufacturer:                      Kingston
    DRAM Manufacturer:                 SK Hynix
    Module Type:                       Unbuffered DIMM
    Number of Ranks/Banks:             1 Ranks, 16 Banks
    Module Attributes:                 Unbuffered
    Error Checking:                    None
    JEDEC Timings:                     CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
    JEDEC Profile @ 1200 MHz:          18.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1200 MHz:          17.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1163 MHz:          16.0-16-16-38-54-408-303-187
    JEDEC Profile @ 1090 MHz:          15.0-15-15-35-50-382-284-175
    JEDEC Profile @ 1018 MHz:          14.0-14-14-33-47-357-265-163
    JEDEC Profile @ 945 MHz:           13.0-13-13-31-44-331-246-152
    JEDEC Profile @ 872 MHz:           12.0-12-12-28-40-306-227-140
    JEDEC Profile @ 799 MHz:           11.0-11-11-26-37-280-208-128
    JEDEC Profile @ 727 MHz:           10.0-10-10-24-34-255-190-117
    Data Width:                        64 bits
    SDRAM Width:                       x8
    Voltage Interface:                 1.20 V
    SPD Revision:                      1.1
    Part Number:                       KF3600C16D4/8GX   
    Manufacturing Location:            7
    Manufacture Date:                  September 2023 (2338h)
    Serial Number:                     211C9E38h
    Revision Code:                     None
    EPP Support:                       [ ]
    XMP Support:                       [X]
    XMP Revision:                      2.0
  XMP Profile 1
    Profile Name:                      XMP-3602 (1801 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1801 MHz:            18.0-20-20-39-85
    XMP Profile @ 1801 MHz:            17.0-20-20-39-85
    XMP Profile @ 1801 MHz:            16.0-20-20-39-85 (Active)
    XMP Profile @ 1689 MHz:            15.0-19-19-37-80
    XMP Profile @ 1576 MHz:            14.0-18-18-35-75
    XMP Profile @ 1463 MHz:            13.0-17-17-32-69
    XMP Profile @ 1351 MHz:            12.0-15-15-30-64
    XMP Profile @ 1238 MHz:            11.0-14-14-27-59
    XMP Profile @ 1126 MHz:            10.0-13-13-25-53
  XMP Profile 2
    Profile Name:                      XMP-2998 (1499 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1499 MHz:            17.0-17-17-36-64
    XMP Profile @ 1499 MHz:            16.0-17-17-36-64
    XMP Profile @ 1499 MHz:            15.0-17-17-36-64
    XMP Profile @ 1399 MHz:            14.0-16-16-34-60
    XMP Profile @ 1299 MHz:            13.0-15-15-32-56
    XMP Profile @ 1199 MHz:            12.0-14-14-29-52
    XMP Profile @ 1099 MHz:            11.0-13-13-27-47
    XMP Profile @ 899 MHz:             9.0-11-11-22-39
                                       
  Memory Slot 4
    Memory Type:                       8 GB DDR4-3602 (1801 MHz) SDRAM
    Manufacturer:                      Kingston
    DRAM Manufacturer:                 SK Hynix
    Module Type:                       Unbuffered DIMM
    Number of Ranks/Banks:             1 Ranks, 16 Banks
    Module Attributes:                 Unbuffered
    Error Checking:                    None
    JEDEC Timings:                     CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
    JEDEC Profile @ 1200 MHz:          18.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1200 MHz:          17.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1163 MHz:          16.0-16-16-38-54-408-303-187
    JEDEC Profile @ 1090 MHz:          15.0-15-15-35-50-382-284-175
    JEDEC Profile @ 1018 MHz:          14.0-14-14-33-47-357-265-163
    JEDEC Profile @ 945 MHz:           13.0-13-13-31-44-331-246-152
    JEDEC Profile @ 872 MHz:           12.0-12-12-28-40-306-227-140
    JEDEC Profile @ 799 MHz:           11.0-11-11-26-37-280-208-128
    JEDEC Profile @ 727 MHz:           10.0-10-10-24-34-255-190-117
    Data Width:                        64 bits
    SDRAM Width:                       x8
    Voltage Interface:                 1.20 V
    SPD Revision:                      1.1
    Part Number:                       KF3600C16D4/8GX   
    Manufacturing Location:            7
    Manufacture Date:                  November 2023 (2346h)
    Serial Number:                     804C34DDh
    Revision Code:                     None
    EPP Support:                       [ ]
    XMP Support:                       [X]
    XMP Revision:                      2.0
  XMP Profile 1
    Profile Name:                      XMP-3602 (1801 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1801 MHz:            18.0-20-20-39-85
    XMP Profile @ 1801 MHz:            17.0-20-20-39-85
    XMP Profile @ 1801 MHz:            16.0-20-20-39-85 (Active)
    XMP Profile @ 1689 MHz:            15.0-19-19-37-80
    XMP Profile @ 1576 MHz:            14.0-18-18-35-75
    XMP Profile @ 1463 MHz:            13.0-17-17-32-69
    XMP Profile @ 1351 MHz:            12.0-15-15-30-64
    XMP Profile @ 1238 MHz:            11.0-14-14-27-59
    XMP Profile @ 1126 MHz:            10.0-13-13-25-53
  XMP Profile 2
    Profile Name:                      XMP-2998 (1499 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1499 MHz:            17.0-17-17-36-64
    XMP Profile @ 1499 MHz:            16.0-17-17-36-64
    XMP Profile @ 1499 MHz:            15.0-17-17-36-64
    XMP Profile @ 1399 MHz:            14.0-16-16-34-60
    XMP Profile @ 1299 MHz:            13.0-15-15-32-56
    XMP Profile @ 1199 MHz:            12.0-14-14-29-52
    XMP Profile @ 1099 MHz:            11.0-13-13-27-47
    XMP Profile @ 899 MHz:             9.0-11-11-22-39
                                       
                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
    Maximum Capacity:                  131072 MB
    Location:                          System Board or Motherboard
    Use:                               System Memory
    Memory Error Correct.:             None
    Memory Devices:                    4
    Structure Length:                  17h
  Memory Device 1
    Size:                              Not Installed
    Form Factor:                       Unknown
    Memory Type:                       Unknown
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                Unknown
    Maximum Voltage:                   Unknown
    Minimum Voltage:                   Unknown
    Device Locator:                    DIMM 0
    Bank Locator:                      P0 CHANNEL A
    Total Width:                       Unknown
    Data Width:                        Unknown
    Device Set:                        00h
    Type Detail:                       Unknown
    Manufacturer:                      Unknown
    Serial Number:                     Unknown
    Asset Tag:                         
    Part Number:                       Unknown
    Structure Length:                  28h
  Memory Device 2
    Size:                              8192 MB
    Form Factor:                       DIMM
    Memory Type:                       DDR4
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                1.2 V
    Maximum Voltage:                   1.2 V
    Minimum Voltage:                   1.2 V
    Device Locator:                    DIMM 1
    Bank Locator:                      P0 CHANNEL A
    Total Width:                       64 bits
    Data Width:                        64 bits
    Device Set:                        00h
    Type Detail:                       Synchronous, Unbuffered (Unregistered)
    Manufacturer:                      Kingston
    Serial Number:                     211C9E38
    Asset Tag:                         
    Part Number:                       KF3600C16D4/8GX
    Structure Length:                  28h
  Memory Device 3
    Size:                              Not Installed
    Form Factor:                       Unknown
    Memory Type:                       Unknown
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                Unknown
    Maximum Voltage:                   Unknown
    Minimum Voltage:                   Unknown
    Device Locator:                    DIMM 0
    Bank Locator:                      P0 CHANNEL B
    Total Width:                       Unknown
    Data Width:                        Unknown
    Device Set:                        00h
    Type Detail:                       Unknown
    Manufacturer:                      Unknown
    Serial Number:                     Unknown
    Asset Tag:                         
    Part Number:                       Unknown
    Structure Length:                  28h
  Memory Device 4
    Size:                              8192 MB
    Form Factor:                       DIMM
    Memory Type:                       DDR4
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                1.2 V
    Maximum Voltage:                   1.2 V
    Minimum Voltage:                   1.2 V
    Device Locator:                    DIMM 1
    Bank Locator:                      P0 CHANNEL B
    Total Width:                       64 bits
    Data Width:                        64 bits
    Device Set:                        00h
    Type Detail:                       Synchronous, Unbuffered (Unregistered)
    Manufacturer:                      Kingston
    Serial Number:                     804C34DD
    Asset Tag:                         
    Part Number:                       KF3600C16D4/8GX
    Structure Length:                  28h
                                       
                  +-----------------------------------------+
                  |                  Disk                   |
                  +-----------------------------------------+
  Disk
    Disk Model:                        Samsung SSD 860 EVO 250GB
    Disk Size:                         238475 MB (232.89 GB)
    Interface Type:                    Serial ATA III (SATA/600)
    Form Factor:                       2.5"
    Rotation Rate:                     SSD
    Geometry:                          Heads: 16, Sectors: 63, Tracks: 16383
    Compatibility:                     ACS-4 revision 94
    Serial Number:                     S3Y9NB0K275545B
    Controller Revision:               RVT01B6Q
    Disk Marketing Size:               250059 MB (250.06 GB)
    Buffer Size:                       Unknown
    Buffer Type:                       Not Specified
    Disk Temperature:                  37 °C (99 °F)
    Reallocated Sectors:               0
    Disk Health Status:                Good
    SSD Remaining Life:                83 %
    Power On Hours Count:              27117 Hour(s)
    Drive Power Cycle Count:           13919
    Total Host Writes:                 63.98 TB
    Logical Drives:                    K:
    ECC bytes:                         None
    Security Erase Time:               4 min
    Enh. Security Erase:               8 min
    Current APM Value:                 None
    Acoustic Management:               None
    Location:                          AMD 400 Series Chipset SATA Controller
  Transfer Modes
    SATA Speed:                        600 MB/s, Active: 600 MB/s
    PIO Mode Support:                  4
    SW DMA Mode Support:               Not Supported
    MW DMA Mode Support:               2, Active: None
    UDMA Mode Support:                 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
    Sectors per Interrupt:             1, Active: 1
  Disk Features
    SATA NCQ Command:                             [X]
    SSD TRIM Command:                             [X]
    DMA Transfer:                                 [X]
    LBA Supported:                                [X]
    Block Mode:                                   [X]
    Double Word I/O:                              [X]
    Standard Standby Timer:                       [X]
    IORDY Supported:                              [X]
    IORDY may be Disabled:                        [X]
    S.M.A.R.T.:                                   [X] enabled
    S.M.A.R.T. Self-test:                         [X] enabled
    S.M.A.R.T. Error Logging:                     [X] enabled
    Security Mode Feature Set:                    [X] disabled
    Removable Media:                              [ ]
    Power Management:                             [X] enabled
    PACKET Command:                               [ ]
    Write Cache:                                  [X] enabled
    Look-ahead:                                   [X] enabled
    Release Interrupt:                            [ ]
    Service Interrupt:                            [ ]
    Device Reset Command:                         [ ]
    Host Protected Area:                          [X] enabled
    Write Verify Command:                         [ ]
    Write Buffer Command:                         [X] enabled
    Read Buffer Command:                          [X] enabled
    NOP Command:                                  [X] enabled
    Identify Device DMA Command:                  [ ]
    Download Microcode Command:                   [X] enabled
    Read/Write DMA Queued:                        [ ]
    CFA Feature Set:                              [ ]
    Advanced Power Management:                    [ ]
    Removable Media Status:                       [ ]
    Power-up in Standby:                          [ ]
    Set Features Req. to Spinup:                  [ ]
    Set Max Security Extension:                   [X] disabled
    Automatic Acoustic Management:                [ ]
    48-bit Address:                               [X] enabled
    Device Configuration Overlay:                 [X] enabled
    Flush Cache Command:                          [X] enabled
    Flush Cache Ext Command:                      [X] enabled
    Media Serial Number:                          [ ]
    Media Card Pass Through:                      [ ]
    Streaming Feature Set:                        [ ]
    General Purpose Logging:                      [X] enabled
    Write DMA/Multiple FUA EXT:                   [X] enabled
    Write DMA Queued FUA EXT:                     [ ]
    World Wide Name:                              [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name                    |Threshold|Worst|Value| Raw Value
     ----+-----------------------------------+---------+-----+-----+-----------
     5   | Reallocated Sectors Count         |       10|  100|  100|     0
     9   | Power On Hours Count              |        0|   94|   94| 27117
     12  | Drive Power Cycle Count           |        0|   86|   86| 13919
     177 | Wear Leveling Count               |        0|   83|   83|   301
     179 | Used Reserved Block Count (Total) |       10|  100|  100|     0
     181 | Program Fail Count                |       10|  100|  100|     0
     182 | Erase Fail Count                  |       10|  100|  100|     0
     183 | Runtime Bad Block                 |       10|  100|  100|     0
     187 | Uncorrectable Errors              |        0|  100|  100|     0
     190 | Airflow Temperature               |        0|   40|   63|    37
     195 | Hardware ECC Recovered            |        0|  200|  200|     0
     199 | UltraDMA CRC Error Rate           |        0|   99|   99|     3
     235 | POR Recovery Count                |        0|   99|   99|  1482
     241 | Total Host Writes                 |        0|   99|   99| 137403892115
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard disk drives)
    Device Description:                Disk drive
    Friendly Name:                     Samsung SSD 860 EVO 250GB
    Device Class:                      DiskDrive
    Device Location:                   Bus Number 0, Target Id 0, LUN 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          disk.inf
    Service Name:                      disk
    Hardware ID:                       SCSI\DiskSamsung_SSD_860_EVO_250GRVT0
    Compatible ID:                     SCSI\Disk
    Parent ID:                         PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
                                       
  Disk
    Disk Model:                        WDC WD1001FALS-00J7B0
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    Serial ATA II (SATA/300)
    Geometry:                          Heads: 16, Sectors: 63, Tracks: 16383
    Compatibility:                     ATA8-ACS
    Serial Number:                     WD-WMATV0357962
    Controller Revision:               05.00K05
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Buffer Size:                       32 MB
    Buffer Type:                       Not Specified
    Disk Temperature:                  42 °C (108 °F)
    Reallocated Sectors:               2
    Disk Health Status:                Poor
    Power On Hours Count:              12757 Hour(s)
    Drive Power Cycle Count:           6419
    Logical Drives:                    E:, F:, H:
    ECC bytes:                         50
    Security Erase Time:               194 min
    Enh. Security Erase:               194 min
    Current APM Value:                 None
    Acoustic Management:               80h (80h Recommended) - Enabled
    Location:                          AMD 400 Series Chipset SATA Controller
  Transfer Modes
    SATA Speed:                        300 MB/s
    PIO Mode Support:                  4
    SW DMA Mode Support:               Not Supported
    MW DMA Mode Support:               2, Active: None
    UDMA Mode Support:                 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
    Sectors per Interrupt:             16, Active: 16
  Disk Features
    SATA NCQ Command:                             [X]
    SSD TRIM Command:                             [ ]
    DMA Transfer:                                 [X]
    LBA Supported:                                [X]
    Block Mode:                                   [X]
    Double Word I/O:                              [ ]
    Standard Standby Timer:                       [X]
    IORDY Supported:                              [X]
    IORDY may be Disabled:                        [X]
    S.M.A.R.T.:                                   [X] enabled
    S.M.A.R.T. Self-test:                         [X] enabled
    S.M.A.R.T. Error Logging:                     [X] enabled
    Security Mode Feature Set:                    [X] disabled
    Removable Media:                              [ ]
    Power Management:                             [X] enabled
    PACKET Command:                               [ ]
    Write Cache:                                  [X] enabled
    Look-ahead:                                   [X] enabled
    Release Interrupt:                            [ ]
    Service Interrupt:                            [ ]
    Device Reset Command:                         [ ]
    Host Protected Area:                          [X] enabled
    Write Verify Command:                         [ ]
    Write Buffer Command:                         [X] enabled
    Read Buffer Command:                          [X] enabled
    NOP Command:                                  [X] enabled
    Identify Device DMA Command:                  [ ]
    Download Microcode Command:                   [X] enabled
    Read/Write DMA Queued:                        [ ]
    CFA Feature Set:                              [ ]
    Advanced Power Management:                    [ ]
    Removable Media Status:                       [ ]
    Power-up in Standby:                          [X] disabled
    Set Features Req. to Spinup:                  [X] enabled
    Set Max Security Extension:                   [X] disabled
    Automatic Acoustic Management:                [X] enabled
    48-bit Address:                               [X] enabled
    Device Configuration Overlay:                 [X] enabled
    Flush Cache Command:                          [X] enabled
    Flush Cache Ext Command:                      [X] enabled
    Media Serial Number:                          [ ]
    Media Card Pass Through:                      [ ]
    Streaming Feature Set:                        [ ]
    General Purpose Logging:                      [X] enabled
    Write DMA/Multiple FUA EXT:                   [ ]
    Write DMA Queued FUA EXT:                     [ ]
    World Wide Name:                              [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       51|  190|  200|    42
     3   | Spin-up Time              |       21|  253|  253|  6275
     4   | Start/Stop Count          |        0|   86|   86| 14933
     5   | Reallocated Sectors Count |      140|  199|  199|     2
     7   | Seek Error Rate           |       51|  253|  100|     0
     9   | Power On Hours Count      |        0|   83|   83| 12757
     10  | Spin-up Retry Count       |       51|  100|  100|     0
     11  | Recalibration Retries     |       51|  100|  100|     0
     12  | Drive Power Cycle Count   |        0|   94|   94|  6419
     192 | Power-Off Retract Count   |        0|  199|  199|  1203
     193 | Load/Unload Cycle Count   |        0|  196|  196| 14919
     194 | Drive Temperature         |        0|   97|  108|    42
     196 | Reallocation Event Count  |        0|  198|  198|     2
     197 |!Current Pending Sectors   |        0|  200|  200|     1
     198 | Uncorrectable Sectors     |        0|  200|  200|     0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|     0
     200 | Write Error Rate          |       51|  197|  200|     0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard disk drives)
    Device Description:                Disk drive
    Friendly Name:                     WDC WD1001FALS-00J7B0
    Device Class:                      DiskDrive
    Device Location:                   Bus Number 1, Target Id 0, LUN 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          disk.inf
    Service Name:                      disk
    Hardware ID:                       SCSI\DiskWDC_____WD1001FALS-00J7B05.0
    Compatible ID:                     SCSI\Disk
    Parent ID:                         PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
                                       
  Disk
    Disk Model:                        HGST HTS541010A9E680
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    Serial ATA III (SATA/600)
    Form Factor:                       2.5"
    Rotation Rate:                     5400 rpm
    Geometry:                          Heads: 16, Sectors: 63, Tracks: 16383
    Compatibility:                     ATA8-ACS revision 40
    Serial Number:                     JDA0001V16XKSH
    Controller Revision:               JA0OA560
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Buffer Size:                       8 MB
    Buffer Type:                       Dual ported multi-sector buffer with a read caching
    Disk Temperature:                  30 °C (86 °F)
    Reallocated Sectors:               0
    Disk Health Status:                Poor
    Power On Hours Count:              16657 Hour(s)
    Drive Power Cycle Count:           4911
    Logical Drives:                    L:
    ECC bytes:                         4
    Security Erase Time:               218 min
    Enh. Security Erase:               220 min
    Current APM Value:                 01h
    Acoustic Management:               None
    Location:                          AMD 400 Series Chipset SATA Controller
  Transfer Modes
    SATA Speed:                        600 MB/s, Active: 600 MB/s
    PIO Mode Support:                  4
    SW DMA Mode Support:               Not Supported
    MW DMA Mode Support:               2, Active: None
    UDMA Mode Support:                 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
    Sectors per Interrupt:             16, Active: 16
  Disk Features
    SATA NCQ Command:                             [X]
    SSD TRIM Command:                             [ ]
    DMA Transfer:                                 [X]
    LBA Supported:                                [X]
    Block Mode:                                   [X]
    Double Word I/O:                              [X]
    Standard Standby Timer:                       [X]
    IORDY Supported:                              [X]
    IORDY may be Disabled:                        [X]
    S.M.A.R.T.:                                   [X] enabled
    S.M.A.R.T. Self-test:                         [X] enabled
    S.M.A.R.T. Error Logging:                     [X] enabled
    Security Mode Feature Set:                    [X] disabled
    Removable Media:                              [ ]
    Power Management:                             [X] enabled
    PACKET Command:                               [ ]
    Write Cache:                                  [X] enabled
    Look-ahead:                                   [X] enabled
    Release Interrupt:                            [ ]
    Service Interrupt:                            [ ]
    Device Reset Command:                         [ ]
    Host Protected Area:                          [X] enabled
    Write Verify Command:                         [ ]
    Write Buffer Command:                         [X] enabled
    Read Buffer Command:                          [X] enabled
    NOP Command:                                  [X] enabled
    Identify Device DMA Command:                  [ ]
    Download Microcode Command:                   [X] enabled
    Read/Write DMA Queued:                        [ ]
    CFA Feature Set:                              [ ]
    Advanced Power Management:                    [X] enabled
    Removable Media Status:                       [ ]
    Power-up in Standby:                          [X] disabled
    Set Features Req. to Spinup:                  [X] enabled
    Set Max Security Extension:                   [X] disabled
    Automatic Acoustic Management:                [ ]
    48-bit Address:                               [X] enabled
    Device Configuration Overlay:                 [X] enabled
    Flush Cache Command:                          [X] enabled
    Flush Cache Ext Command:                      [X] enabled
    Media Serial Number:                          [ ]
    Media Card Pass Through:                      [ ]
    Streaming Feature Set:                        [ ]
    General Purpose Logging:                      [X] enabled
    Write DMA/Multiple FUA EXT:                   [X] enabled
    Write DMA Queued FUA EXT:                     [ ]
    World Wide Name:                              [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       62|  100|  100|     0
     2   | Throughput Performance    |       40|  100|  100|     0
     3   | Spin-up Time              |       33|  223|  223| 60129542145
     4   | Start/Stop Count          |        0|   57|   57| 68110
     5   | Reallocated Sectors Count |        5|   59|   59|     0
     7   | Seek Error Rate           |       67|  100|  100|     0
     8   | Seek Time Performance     |       40|  100|  100|     0
     9   | Power On Hours Count      |        0|   62|   62| 16657
     10  | Spin-up Retry Count       |       60|  100|  100|     0
     12  | Drive Power Cycle Count   |        0|   97|   97|  4911
     191 | G-Sense Error Rate        |        0|  100|  100|     0
     192 | Power-Off Retract Count   |        0|  100|  100|   130
     193 | Load/Unload Cycle Count   |        0|   80|   80| 208413
     194 | Drive Temperature         |        0|  200|  200| 219043856414
     196 | Reallocation Event Count  |        0|   56|   56|  1199
     197 |!Current Pending Sectors   |        0|  100|  100|    32
     198 | Uncorrectable Sectors     |        0|  100|  100|     0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|     0
     223 | Load/Unload Retry Count   |        0|  100|  100|     0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard disk drives)
    Device Description:                Disk drive
    Friendly Name:                     HGST HTS541010A9E680
    Device Class:                      DiskDrive
    Device Location:                   Bus Number 4, Target Id 0, LUN 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          disk.inf
    Service Name:                      disk
    Hardware ID:                       SCSI\DiskHGST_____HTS541010A9E680JA0O
    Compatible ID:                     SCSI\Disk
    Parent ID:                         PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
                                       
  Disk
    Disk Model:                        Samsung SSD 970 EVO Plus 1TB            
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    NVMe 1.3.0
    Serial Number:                     S6P7NF0T435103B     
    Controller Revision:               4B2QEXM7
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Disk Temperature:                  47 °C (117 °F)
    Disk Health Status:                Good
    SSD Remaining Life:                100 %
    Power On Hours Count:              4550 Hour(s)
    Drive Power Cycle Count:           3581
    Total Host Writes:                 9.18 TB
    Total Host Reads:                  15.06 TB
    Logical Drives:                    C:, D:, G:, I:, J:
    Controller Manufacturer:           Samsung Electronics Co., Ltd., Memory Division
    IEEE OUI Identifier:               00-25-38
    Controller ID:                     6
    Number of Namespaces:              1
    Power Consumption:                 0.005-7.5 Wattes
    Number of Power States:            5
    Warning Temperature Threshold:     82 °C (180 °F)
    Critical Temperature Threshold:    85 °C (185 °F)
    Max Data Transfer Size:            128 Pages
    Abort Command Limit:               8
    Asynchronous Event Request Limit:  4
    Firmware Slots:                    3
    Time for Firmware Activation:      0 sec
    Max Error Log Page Entries:        64
    Host Memory Buffer Preferred Size: 0 kB
    Host Memory Buffer Minimum Size:   0 kB
    Extended Self-Test Time:           35 min
    Submission Queue Entry Size:       Minimum: 64 bytes, Maximum: 64 bytes
    Completion Queue Entry Size:       Minimum: 16 bytes, Maximum: 16 bytes
    Subsystem Name:                    nqn.1994-11.com.samsung:nvme:980PRO:M.2:S6P7NF0T435103B
    Location:                          Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
  Transfer Modes
    Bus Type:                          PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
  NVMe Commands
    Security Send/Receive:                        [X]
    Format NVM:                                   [X]
    Firmware Commit:                              [X]
    Firmware Image Download:                      [X]
    Namespace Management:                         [ ]
    Device Self-test:                             [X]
    Directive Send/Receive:                       [ ]
    NVMe-MI Send/Receive:                         [ ]
    Virtualization Management:                    [ ]
    Doorbell Buffer Config:                       [ ]
    Compare:                                      [X]
    Write Uncorrectable:                          [X]
    Dataset Management:                           [X]
    Write Zeroes:                                 [ ]
    Reservations:                                 [ ]
    Verify:                                       [ ]
  NVMe Features
    Volatile Write Cache:                         [X]
    Get LBA Status:                               [ ]
    SMART Info Per Namespace:                     [X]
    Command Effects Log Page:                     [X]
    Get Log Page Extended Data:                   [X]
    Telemetry Host-Initiated:                     [X]
    Telemetry Controller-Initiated:               [X]
    Persistent Event Log:                         [ ]
    Autonomous Power State Transition:            [X]
    Keep Alive Support:                           [ ]
    Thermal Management:                           [X]
    Crypto Erase Support:                         [X]
    Block Erase Support:                          [X]
    Overwrite Support:                            [ ]
    Save Select Field:                            [X]
    Timestamp Feature:                            [X]
    Compare/Write Fused Operation:                [ ]
    NVM Sets:                                     [ ]
    Endurance Groups:                             [X]
  S.M.A.R.T.
     ID  | Attribute Name                      |Raw Value
     ----+-------------------------------------+---------+--------
     0   | Critical Warning                    |        0
     1   | Composite Temperature               |      320
     3   | Available Spare                     |      100
     4   | Available Spare Threshold           |       10
     5   | Percentage Used                     |        0
     6   | Endurance Group Critical Warning    |        0
     32  | Data Units Read                     | 32342667
     48  | Data Units Written                  | 19721145
     64  | Host Read Commands                  |520124208
     80  | Host Write Commands                 |319779233
     96  | Controller Busy Time                |     2257
     112 | Drive Power Cycle Count             |     3581
     128 | Power On Hours Count                |     4550
     144 | Unsafe Shutdown Count               |     1169
     160 | Media and Data Integrity Errors     |        0
     176 | Error Information Log Entries       |        0
     192 | Warning Composite Temperature Time  |        0
     196 | Critical Composite Temperature Time |        0
     200 | Temperature Sensor 1                |      320
     202 | Temperature Sensor 2                |      327
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard disk drives)
    Device Description:                Disk drive
    Friendly Name:                     Samsung SSD 970 EVO Plus 1TB
    Device Class:                      DiskDrive
    Device Location:                   Bus Number 0, Target Id 0, LUN 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          disk.inf
    Service Name:                      disk
    Hardware ID:                       SCSI\DiskNVMe________________Samsung_SSD_970_EVO_Plus_1TB4B2QEXM7
    Compatible ID:                     SCSI\Disk
    Parent ID:                         PCI\VEN_144D&DEV_A808&SUBSYS_A801144D&REV_00
                                       
                  +-----------------------------------------+
                  |                  ATAPI                  |
                  +-----------------------------------------+
   ATAPI
    ATAPI Model:                       ATAPI   DVD W  DH16W1S
    ATAPI Type:                        DVD+-RW DL/CD-RW
    Interface Type:                    Serial ATA I
    Physical Interface:                Serial ATAPI
    ATAPI Name:                        ATAPI DVD W  DH16W1S
    Vendor Specific:                   2006/10/27 19:00
    CD Read Speed:                     48x (Current: 48x)
    CD Write Speed:                    48x (Current: 48x)
    DVD Read Speed:                    Current: 5x
    DVD Write Speed:                   Current: 5x
    Buffer Size:                       2 MB
    Loading Mechanism:                 Tray Type
    Rotation Control:                  CLV
    Read Retry Count:                  48
    Write Retry Count:                 0
    Compatibility:                     ATA/ATAPI-7
    Serial Number:                                         
    Controller Revision:               2A11
    Logical Drives:                    M:
    Command DRQ Type:                  Accelerated DRQ
    Command Packet Size:               12 bytes
    Location:                          AMD 400 Series Chipset SATA Controller
  Transfer Modes
    PIO Mode Support:                  4
    SW DMA Mode Support:               7, Active: 2
    MW DMA Mode Support:               2, Active: None
    UDMA Mode Support:                 5 (UltraDMA/100), Active: 2 (UltraDMA/33)
  Reading Features
    CD-R Disk Read:                               [X]
    CD-RW Disk Read:                              [X]
    DVD-ROM Disk Read:                            [X]
    DVD-RAM Disk Read:                            [ ]
    DVD-R Disk Read:                              [X]
    DVD-R DL Disk Read:                           [X]
    DVD-RW Disk Read:                             [X]
    DVD-RW DL Disk Read:                          [ ]
    DVD+R Disk Read:                              [X]
    DVD+R DL Disk Read:                           [X]
    DVD+RW Disk Read:                             [X]
    DVD+RW DL Disk Read:                          [ ]
    BD-ROM Disk Read:                             [ ]
    BD-R Disk Read:                               [ ]
    BD-RE Disk Read:                              [ ]
    HD DVD-ROM Disk Read:                         [ ]
    HD DVD-RAM Disk Read:                         [ ]
    HD DVD-R Disk Read:                           [ ]
    HD DVD-R DL Disk Read:                        [ ]
    HD DVD-RW Disk Read:                          [ ]
    HD DVD-RW DL Disk Read:                       [ ]
    Read Packet Using Method 2:                   [X]
    Read Mode2 Form1 Sectors:                     [X]
    Read Mode2 Form2 Sectors:                     [X]
    Multisession Disk Read:                       [X]
    READ-CD Command on AudioCD:                   [X]
    Read Bar Code Capable:                        [ ]
    Read Lead-in (CD-Text):                       [X]
  Writing Features
    CD-R Disk Write:                              [X]
    CD-RW Disk Write:                             [X]
    DVD-RAM Disk Write:                           [ ]
    DVD-R Disk Write:                             [X]
    DVD-R DL Disk Write:                          [ ]
    DVD-RW Disk Write:                            [X]
    DVD+R Disk Write:                             [X]
    DVD+R DL Disk Write:                          [X]
    DVD+RW Disk Write:                            [X]
    DVD+RW DL Disk Write:                         [ ]
    BD-R Disk Write:                              [ ]
    BD-RE Disk Write:                             [ ]
    HD DVD-R Disk Write:                          [ ]
    HD DVD-R DL Disk Write:                       [ ]
    HD DVD-RAM Disk Write:                        [ ]
    HD DVD-RW Disk Write:                         [ ]
    HD DVD-RW DL Disk Write:                      [ ]
    Test Write Mode Support:                      [X]
    Buffer Underrun Protection:                   [X]
  Other Features
    Audio Play Support:                           [X]
    CD-DA Stream is Accurate:                     [X]
    Composite Audio/Video:                        [ ]
    Digital Output on Port 1:                     [X]
    Digital Output on Port 2:                     [ ]
    Support Subcode R-W:                          [ ]
    Support Subcode R-W D&C:                      [ ]
    C2 Pointers Supported:                        [X]
    ISRC Supported:                               [X]
    UPC Supported:                                [X]
  ATAPI Features
    DMA Transfer:                                 [X]
    LBA Supported:                                [X]
    Block Mode:                                   [ ]
    IORDY Supported:                              [X]
    IORDY may be Disabled:                        [X]
    ATA Software Reset:                           [ ]
    Overlap Operation:                            [ ]
    Command Queuing:                              [ ]
    Interleaving DMA:                             [ ]
    S.M.A.R.T.:                                   [ ]
    S.M.A.R.T. Self-test:                         [ ]
    S.M.A.R.T. Error Logging:                     [ ]
    Security Mode Feature Set:                    [ ]
    Removable Media:                              [ ]
    Power Management:                             [ ]
    PACKET Command:                               [X] enabled
    Write Cache:                                  [ ]
    Look-ahead:                                   [ ]
    Release Interrupt:                            [ ]
    Service Interrupt:                            [ ]
    Device Reset Command:                         [X] enabled
    Host Protected Area:                          [ ]
    Write Verify Command:                         [ ]
    Write Buffer Command:                         [ ]
    Read Buffer Command:                          [ ]
    NOP Command:                                  [ ]
    Identify Device DMA Command:                  [ ]
    Download Microcode Command:                   [ ]
    Read/Write DMA Queued:                        [ ]
    CFA Feature Set:                              [ ]
    Advanced Power Management:                    [ ]
    Removable Media Status:                       [ ]
    Power-up in Standby:                          [ ]
    Set Features Req. to Spinup:                  [ ]
    Set Max Security Extension:                   [ ]
    Automatic Acoustic Management:                [ ]
    48-bit Address:                               [ ]
    Device Configuration Overlay:                 [ ]
    Flush Cache Command:                          [X] enabled
    Flush Cache Ext Command:                      [ ]
    Media Serial Number:                          [ ]
    Media Card Pass Through:                      [ ]
    Streaming Feature Set:                        [ ]
    General Purpose Logging:                      [ ]
    Write DMA/Multiple FUA EXT:                   [ ]
    Write DMA Queued FUA EXT:                     [ ]
    World Wide Name:                              [ ]
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard CD-ROM drives)
    Device Description:                CD-ROM Drive
    Friendly Name:                     ATAPI DVD W  DH16W1S
    Device Class:                      CDROM
    Device Location:                   Bus Number 5, Target Id 0, LUN 0
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          cdrom.inf
    Service Name:                      cdrom
    Hardware ID:                       SCSI\CdRomATAPI___DVD_W__DH16W1S__2A11
    Compatible ID:                     SCSI\CdRom
    Parent ID:                         PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
                                       
                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
    ASPI devices not found
                                       
                  +-----------------------------------------+
                  |              Logical Drives             |
                  +-----------------------------------------+
  Local Drives
  C:[SYSTEM]
    Drive Letter:                      C:
    Drive Type:                        Fixed Disk
    Volume Label:                      SYSTEM
    File System:                       FAT
    Volume Serial Number:              0805-FB80
    Total Size:                        1.99 GB
    Free Space:                        747.5 MB (36.6%)
    Location:                          Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
  D:[UTILITIES]
    Drive Letter:                      D:
    Drive Type:                        Fixed Disk
    Volume Label:                      UTILITIES
    File System:                       FAT32
    Volume Serial Number:              089E-9200
    Total Size:                        29.99 GB
    Free Space:                        8.73 GB (29.1%)
    Location:                          Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
  E:[WIN2K]
    Drive Letter:                      E:
    Drive Type:                        Fixed Disk
    Volume Label:                      WIN2K
    File System:                       NTFS
    Volume Serial Number:              A4B5-2192
    Total Size:                        30.0 GB
    Free Space:                        20.35 GB (67.8%)
    Location:                          WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  F:[WINXP]
    Drive Letter:                      F:
    Drive Type:                        Fixed Disk
    Volume Label:                      WINXP
    File System:                       NTFS
    Volume Serial Number:              90B8-E3D0
    Total Size:                        10.0 GB
    Free Space:                        8.9 GB (89.0%)
    Location:                          WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  G:[WIN7]
    Drive Letter:                      G:
    Drive Type:                        Fixed Disk
    Volume Label:                      WIN7
    File System:                       NTFS
    Volume Serial Number:              1C61-A5D1
    Total Size:                        250.0 GB
    Free Space:                        60.83 GB (24.3%)
    Location:                          Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
  H:[MUSIC]
    Drive Letter:                      H:
    Drive Type:                        Fixed Disk
    Volume Label:                      MUSIC
    File System:                       NTFS
    Volume Serial Number:              56C9-FD1A
    Total Size:                        891.51 GB
    Free Space:                        10.66 GB (1.2%)
    Location:                          WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  I:[GAMES]
    Drive Letter:                      I:
    Drive Type:                        Fixed Disk
    Volume Label:                      GAMES
    File System:                       NTFS
    Volume Serial Number:              E8D9-213C
    Total Size:                        619.52 GB
    Free Space:                        69.69 GB (11.2%)
    Location:                          Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
  J:[WIN11]
    Drive Letter:                      J:
    Drive Type:                        Fixed Disk
    Volume Label:                      WIN11
    File System:                       NTFS
    Volume Serial Number:              CC50-1EE0
    Total Size:                        30.0 GB
    Free Space:                        2.84 GB (9.5%)
    Location:                          Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
  K:[WIN10MAX]
    Drive Letter:                      K:
    Drive Type:                        Fixed Disk
    Volume Label:                      WIN10MAX
    File System:                       NTFS
    Volume Serial Number:              B8CC-3468
    Total Size:                        232.88 GB
    Free Space:                        58.87 GB (25.3%)
    Location:                          Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
  L:[MAXDATA]
    Drive Letter:                      L:
    Drive Type:                        Fixed Disk
    Volume Label:                      MAXDATA
    File System:                       NTFS
    Volume Serial Number:              DAE5-7313
    Total Size:                        931.51 GB
    Free Space:                        487.26 GB (52.3%)
    Location:                          HGST HTS541010A9E680 (JDA0001V16XKSH)
  M:
    Drive Letter:                      M:
    Drive Type:                        Optical Drive
    Location:                          ATAPI   DVD W  DH16W1S
                                       
                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
  USB Device 1
    Vendor (320Fh):                    Evision
    Device (5000h):                    RGB Gaming Mechanical Keyboard
    Manufacturer:                      Evision
    Product:                           RGB Keyboard
    Serial Number:                     
    Device Version:                    1.06
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     
    USB Version:                       2.0
    Current Speed:                     12 Mbit/s
    Transfer Type:                     Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         400 mA Remote Wakeup
    Parent Device:                     AMD Matisse USB 3.0 Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0004.Hub_#0003
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_320F&PID_5000&REV_0106
    Compatible ID:                     USB\COMPAT_VID_320F&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_149C&SUBSYS_7A381462&REV_00
  Interface 1
    Class (03h):                       Human Interface Devices
    SubClass (01h):                    Boot Interface Subclass
    Protocol (01h):                    Keyboard
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   002b.0000.0003.004.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_320F&PID_5000&REV_0106&MI_00
    Compatible ID:                     USB\COMPAT_VID_320f&Class_03&SubClass_01&Prot_01
    Parent ID:                         USB\VID_320F&PID_5000&REV_0106
  Interface 2
    Class (03h):                       Human Interface Devices
    SubClass (01h):                    Boot Interface Subclass
    Protocol (02h):                    Mouse
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   002b.0000.0003.004.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_320F&PID_5000&REV_0106&MI_01
    Compatible ID:                     USB\COMPAT_VID_320f&Class_03&SubClass_01&Prot_02
    Parent ID:                         USB\VID_320F&PID_5000&REV_0106
                                       
  USB Device 2
    Vendor (046Dh):                    Logitech
    Device (C09Dh):                    G102 LIGHTSYNC Gaming Mouse
    Manufacturer:                      Logitech
    Product:                           G102 LIGHTSYNC Gaming Mouse
    Serial Number:                     205834584258
    Device Version:                    52.02
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     U152.02_B0017           
    USB Version:                       2.0
    Current Speed:                     12 Mbit/s
    Transfer Type:                     Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         300 mA Remote Wakeup
    Parent Device:                     AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Logitech
    Device Description:                G203 LIGHTSYNC
    Friendly Name:                     G102 LIGHTSYNC
    Device Class:                      USB
    Device Location:                   Port_#0007.Hub_#0001
    Driver Provider:                   Logitech
    Driver Version:                    1.1.55.3120
    Driver Date:                       4-15-2024
    Inf File:                          oem15.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_046D&PID_C09D&REV_5202
    Compatible ID:                     USB\COMPAT_VID_046D&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
  Interface 1
    Class (03h):                       Human Interface Devices
    SubClass (01h):                    Boot Interface Subclass
    Protocol (02h):                    Mouse
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   0003.0000.0000.007.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_046D&PID_C09D&REV_5202&MI_00
    Compatible ID:                     USB\COMPAT_VID_046d&Class_03&SubClass_01&Prot_02
    Parent ID:                         USB\VID_046D&PID_C09D&REV_5202
  Interface 2
    Class (03h):                       Human Interface Devices
    SubClass (00h):                    No Subclass
    Protocol (00h):                    None
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   0003.0000.0000.007.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_046D&PID_C09D&REV_5202&MI_01
    Compatible ID:                     USB\COMPAT_VID_046d&Class_03&SubClass_00&Prot_00
    Parent ID:                         USB\VID_046D&PID_C09D&REV_5202
                                       
  USB Device 3
    Vendor (3142h):                    FIFINE
    Device (0080h):                    PC Gaming Dynamic RGB Headset
    Manufacturer:                      
    Product:                           fifine Headset
    Serial Number:                     
    Device Version:                    1.0
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     
    USB Version:                       1.10
    Current Speed:                     12 Mbit/s
    Transfer Type:                     Isochronous/Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         100 mA
    Parent Device:                     AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0011.Hub_#0001
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_3142&PID_0080&REV_0100
    Compatible ID:                     USB\COMPAT_VID_3142&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
  Interface 1
    Class (01h):                       Audio
    SubClass (01h):                    Control Device
    Protocol (00h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Generic USB Audio)
    Device Description:                USB Audio Device
    Friendly Name:                     fifine Headset
    Device Class:                      MEDIA
    Device Location:                   0003.0000.0000.011.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3958
    Driver Date:                       7-19-2024
    Inf File:                          wdma_usb.inf
    Service Name:                      usbaudio
    Hardware ID:                       USB\VID_3142&PID_0080&REV_0100&MI_00
    Compatible ID:                     USB\COMPAT_VID_3142&Class_01&SubClass_01&Prot_00
    Parent ID:                         USB\VID_3142&PID_0080&REV_0100
  Interface 2
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 3
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 4
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   0003.0000.0000.011.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_3142&PID_0080&REV_0100&MI_03
    Compatible ID:                     USB\COMPAT_VID_3142&Class_03&SubClass_00&Prot_00
    Parent ID:                         USB\VID_3142&PID_0080&REV_0100
  Interface 5
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 6
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 7
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 8
    Class (03h):                       Human Interface Devices
    SubClass (00h):                    No Subclass
    Protocol (00h):                    None
    Interface:                         
                                       
  USB Device 4
    Vendor (3142h):                    FIFINE
    Device (5060h):                    Microphone
    Manufacturer:                      
    Product:                           Fifine Microphone
    Serial Number:                     
    Device Version:                    1.0
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     
    USB Version:                       1.10
    Current Speed:                     12 Mbit/s
    Transfer Type:                     Isochronous/Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         100 mA
    Parent Device:                     AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0012.Hub_#0001
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_3142&PID_5060&REV_0100
    Compatible ID:                     USB\COMPAT_VID_3142&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
  Interface 1
    Class (01h):                       Audio
    SubClass (01h):                    Control Device
    Protocol (00h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Generic USB Audio)
    Device Description:                USB Audio Device
    Friendly Name:                     Fifine Microphone
    Device Class:                      MEDIA
    Device Location:                   0003.0000.0000.012.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3958
    Driver Date:                       7-19-2024
    Inf File:                          wdma_usb.inf
    Service Name:                      usbaudio
    Hardware ID:                       USB\VID_3142&PID_5060&REV_0100&MI_00
    Compatible ID:                     USB\COMPAT_VID_3142&Class_01&SubClass_01&Prot_00
    Parent ID:                         USB\VID_3142&PID_5060&REV_0100
  Interface 2
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 3
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   0003.0000.0000.012.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_3142&PID_5060&REV_0100&MI_02
    Compatible ID:                     USB\COMPAT_VID_3142&Class_03&SubClass_00&Prot_00
    Parent ID:                         USB\VID_3142&PID_5060&REV_0100
  Interface 4
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (00h):                    Unknown
    Interface:                         
  Interface 5
    Class (03h):                       Human Interface Devices
    SubClass (00h):                    No Subclass
    Protocol (00h):                    None
    Interface:                         
                                       
  USB Device 5
    Vendor (04A9h):                    Canon
    Device (2660h):                    LaserBase MF3110 Scanner/Printer
    Manufacturer:                      Canon,Inc.
    Product:                           MF3110
    Serial Number:                     2363E2124558
    Device Version:                    0.0
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     
    USB Version:                       2.0
    Current Speed:                     480 Mbit/s
    Transfer Type:                     Bulk/Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         2 mA Self-Powered
    Parent Device:                     AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0014.Hub_#0001
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_04A9&PID_2660&REV_0000
    Compatible ID:                     USB\COMPAT_VID_04A9&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
  Interface 1
    Class (FFh):                       Vendor Specific Class
    SubClass (00h):                    Unknown
    Protocol (FFh):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The drivers for this device are not installed (28)
    Device Description:                MF3110
    Device Location:                   0003.0000.0000.014.000.000.000.000.000
    Hardware ID:                       USB\VID_04A9&PID_2660&REV_0000&MI_00
    Compatible ID:                     USB\COMPAT_VID_04a9&Class_ff&SubClass_00&Prot_ff
    Parent ID:                         USB\VID_04A9&PID_2660&REV_0000
  Interface 2
    Class (07h):                       Printer
    SubClass (01h):                    Printer
    Protocol (02h):                    Bidirectional
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                USB Printing Support
    Friendly Name:                     Canon MF3110
    Device Class:                      USB
    Device Location:                   0003.0000.0000.014.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4249
    Driver Date:                       6-21-2006
    Inf File:                          usbprint.inf
    Service Name:                      usbprint
    Hardware ID:                       USB\VID_04A9&PID_2660&REV_0000&MI_01
    Compatible ID:                     USB\COMPAT_VID_04a9&Class_07&SubClass_01&Prot_02
    Parent ID:                         USB\VID_04A9&PID_2660&REV_0000
                                       
  USB Device 6
    Vendor (0B05h):                    ASUSTek Computer
    Device (180Dh):                    ASUS XONAR SC150 AUDIO DEVICE
    Manufacturer:                      ASUSTeK
    Product:                           STRIX SOUND CARD
    Serial Number:                     
    Device Version:                    1.03
    Class (EFh):                       Miscellaneous Device
    SubClass (02h):                    Common Class
    Protocol (01h):                    Interface Association
    Configuration:                     
    USB Version:                       2.0
    Current Speed:                     480 Mbit/s
    Transfer Type:                     Isochronous/Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         500 mA
    Parent Device:                     ASMedia Technology Inc. ASM1042A USB 3.0 Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0003.Hub_#0002
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_0B05&PID_180D&REV_0103
    Compatible ID:                     USB\COMPAT_VID_0B05&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1B21&DEV_1142&SUBSYS_86A01043&REV_00
  Interface 1
    Class (01h):                       Audio
    SubClass (01h):                    Control Device
    Protocol (20h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                USB Audio 2.0
    Friendly Name:                     STRIX SOUND CARD
    Device Class:                      MEDIA
    Device Location:                   0027.0000.0000.003.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       5-6-2022
    Inf File:                          usbaudio2.inf
    Service Name:                      usbaudio2
    Hardware ID:                       USB\VID_0B05&PID_180D&REV_0103&MI_00
    Compatible ID:                     USB\COMPAT_VID_0b05&Class_01&SubClass_00&Prot_20
    Parent ID:                         USB\VID_0B05&PID_180D&REV_0103
  Interface 2
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         Speaker
  Interface 3
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 4
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 5
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                USB Input Device
    Device Class:                      HIDClass
    Device Location:                   0027.0000.0000.003.000.000.000.000.000
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4111
    Driver Date:                       6-21-2006
    Inf File:                          input.inf
    Service Name:                      HidUsb
    Hardware ID:                       USB\VID_0B05&PID_180D&REV_0103&MI_04
    Compatible ID:                     USB\COMPAT_VID_0b05&Class_03&SubClass_00&Prot_00
    Parent ID:                         USB\VID_0B05&PID_180D&REV_0103
  Interface 6
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 7
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 8
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 9
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 10
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 11
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         SPDIF Output
  Interface 12
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 13
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 14
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 15
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         Input
  Interface 16
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 17
    Class (01h):                       Audio
    SubClass (02h):                    Streaming
    Protocol (20h):                    Unknown
    Interface:                         
  Interface 18
    Class (03h):                       Human Interface Devices
    SubClass (00h):                    No Subclass
    Protocol (00h):                    None
    Interface:                         
                                       
                  +-----------------------------------------+
                  |              Plug and Play              |
                  +-----------------------------------------+
  Plug and Play
    PnP Version:                       1.0
    Number of PnP Devices:             25
                                       
  PnP Device 1
    Vendor:                            Generic System Device
    Device Name:                       AT Interrupt Controller
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0000
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Programmable interrupt controller
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0000
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 2
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 3
    Vendor:                            Generic System Device
    Device Name:                       Standard LPT printer port
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0400
    Class (07h):                       Communication
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
    I/O Port:                          378h-37Fh
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard port types)
    Device Description:                Printer Port
    Friendly Name:                     Ïîðò ïðèíòåðà (LPT1)
    Device Class:                      Ports
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          msports.inf
    Service Name:                      Parport
    Hardware ID:                       ACPI\VEN_PNP&DEV_0400
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 4
    Vendor:                            Advanced Micro Devices, Inc.
    Device Name:                       AMD GPIO Controller
    PnP Device ID:                     ACPI\VEN_AMDI&DEV_F030
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
    Memory Address:                    FEC30000h-FEC30FFFh
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices, Inc.
    Device Description:                AMD GPIO Controller
    Device Class:                      System
    Driver Provider:                   Advanced Micro Devices, Inc.
    Driver Version:                    2.0.1.0
    Driver Date:                       3-9-2020
    Inf File:                          oem6.inf
    Service Name:                      amdgpio3
    Hardware ID:                       ACPI\VEN_AMDI&DEV_F030
    Compatible ID:                     ACPI\AMDIF030
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 5
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
                                       
  PnP Device 6
    Vendor:                            Generic System Device
    Device Name:                       Intel High Precision Event Timer
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0103
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                High precision event timer
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0103
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 7
    Vendor:                            Generic System Device
    Device Name:                       AT DMA Controller
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0200
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Direct memory access controller
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0200
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 8
    Vendor:                            Advanced Micro Devices, Inc.
    Device Name:                       AMD GPIO Controller
    PnP Device ID:                     ACPI\VEN_AMDI&DEV_0030
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
    System IRQ:                        7
    Memory Address:                    FED81500h-FED818FFh
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Advanced Micro Devices, Inc
    Device Description:                AMD GPIO Controller
    Device Class:                      System
    Driver Provider:                   Advanced Micro Devices, Inc
    Driver Version:                    2.2.0.130
    Driver Date:                       3-11-2020
    Inf File:                          oem17.inf
    Service Name:                      amdgpio2
    Hardware ID:                       ACPI\VEN_AMDI&DEV_0030
    Compatible ID:                     ACPI\AMDI0030
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 9
    Vendor:                            Generic System Device
    Device Name:                       16550A-compatible COM port
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0501
    Class (07h):                       Communication
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
    I/O Port:                          3F8h-3FFh
    System IRQ:                        4
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard port types)
    Device Description:                Communications Port
    Friendly Name:                     Ïîñëåäîâàòåëüíûé ïîðò (COM1)
    Device Class:                      Ports
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          msports.inf
    Service Name:                      Serial
    Hardware ID:                       ACPI\VEN_PNP&DEV_0501
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 10
    Vendor:                            Generic System Device
    Device Name:                       AT standard speaker sound
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0800
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                System speaker
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0800
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 11
    Vendor:                            Generic System Device
    Device Name:                       ISA System Board
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C01
    Class (08h):                       System Peripheral
    Parent Device:                     PCI Bus Host Bridge
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                System board
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C01
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  PnP Device 12
    Vendor:                            Generic System Device
    Device Name:                       Microsoft Windows Management Interface for ACPI
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C14
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                Microsoft Windows Management Interface for ACPI
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3958
    Driver Date:                       6-21-2006
    Inf File:                          wmiacpi.inf
    Service Name:                      WmiAcpi
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C14
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 13
    Vendor:                            Generic System Device
    Device Name:                       Microsoft Windows Management Interface for ACPI
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C14
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                Microsoft Windows Management Interface for ACPI
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3958
    Driver Date:                       6-21-2006
    Inf File:                          wmiacpi.inf
    Service Name:                      WmiAcpi
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C14
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 14
    Vendor:                            Generic System Device
    Device Name:                       PCI Bus Host Bridge
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0A08
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Connected Devices
    Device 1:                          AMD Starship/Matisse Root Complex
    Device 2:                          AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 3:                          AMD Starship/Matisse GPP Bridge
    Device 4:                          AMD Starship/Matisse GPP Bridge
    Device 5:                          AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 6:                          AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 7:                          AMD Starship/Matisse GPP Bridge
    Device 8:                          AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 9:                          AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 10:                         AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 11:                         AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Device 12:                         AMD Starship/Matisse PCIe Dummy Host Bridge
    Device 13:                         AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Device 14:                         AMD Hudson SMBus Controller
    Device 15:                         AMD B450 Fusion Controller Hub (FCH)
    Device 16:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 0
    Device 17:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 1
    Device 18:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 2
    Device 19:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 3
    Device 20:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 4
    Device 21:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 5
    Device 22:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 6
    Device 23:                         AMD Matisse/Vermeer Data Fabric: Device 18h; Function 7
    Device 24:                         ISA System Board
    Device 25:                         Motherboard registers
    Device 26:                         Motherboard registers
  Device Resources
    I/O Port:                          00h-3AFh
    I/O Port:                          3E0h-CF7h
    I/O Port:                          3B0h-3DFh
    I/O Port:                          D00h-FFFFh
    Memory Address:                    000A0000h-000BFFFFh
    Memory Address:                    000C0000h-000DFFFFh
    Memory Address:                    C0000000h-FEC2FFFFh
    Memory Address:                    FEE00000h-FFFFFFFFh
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                PCI Express Root Complex
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.4317
    Driver Date:                       6-21-2006
    Inf File:                          pci.inf
    Service Name:                      pci
    Hardware ID:                       ACPI\VEN_PNP&DEV_0A08
    Compatible ID:                     *PNP0A03
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 15
    Vendor:                            Generic System Device
    Device Name:                       ACPI system board hardware
    PnP Device ID:                     ACPI_HAL\PNP0C08
    Class (08h):                       System Peripheral
  Connected Devices
    Device 1:                          Advanced Micro Devices, Inc. AMD GPIO Controller
    Device 2:                          Intel High Precision Event Timer
    Device 3:                          Advanced Micro Devices, Inc. AMD GPIO Controller
    Device 4:                          Microsoft Windows Management Interface for ACPI
    Device 5:                          Microsoft Windows Management Interface for ACPI
    Device 6:                          PCI Bus Host Bridge
    Device 7:                          Generic System Device Trusted Platform Module 2.0
    Device 8:                          Microsoft Windows Management Interface for ACPI
    Device 9:                          Motherboard registers
    Device 10:                         Motherboard registers
    Device 11:                         ACPI power button device
    Device 12:                          Software Component
  Device Resources
    System IRQ:                        55
    System IRQ:                        0-255
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                Microsoft ACPI-Compliant System
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3810
    Driver Date:                       6-21-2006
    Inf File:                          acpi.inf
    Service Name:                      ACPI
    Hardware ID:                       ACPI_HAL\PNP0C08
    Parent ID:                         acpiapic
                                       
  PnP Device 16
    Vendor:                            Generic System Device
    Device Name:                       AT Timer
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0100
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                System timer
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0100
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
  PnP Device 17
    Vendor:                            Generic System Device
    Device Name:                       Trusted Platform Module 2.0
    PnP Device ID:                     ACPI\VEN_MSFT&DEV_0101
    Parent Device:                     ACPI system board hardware
  Device Resources
    Memory Address:                    BB465000h-BB468FFFh
    Memory Address:                    BB469000h-BB46CFFFh
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard)
    Device Description:                Trusted Platform Module 2.0
    Device Class:                      SecurityDevices
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          tpm.inf
    Service Name:                      TPM
    Hardware ID:                       ACPI\VEN_MSFT&DEV_0101
    Compatible ID:                     ACPI\MSFT0101
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 18
    Vendor:                            Generic System Device
    Device Name:                       Microsoft Windows Management Interface for ACPI
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C14
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Microsoft
    Device Description:                Microsoft Windows Management Interface for ACPI
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3958
    Driver Date:                       6-21-2006
    Inf File:                          wmiacpi.inf
    Service Name:                      WmiAcpi
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C14
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 19
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     PCI Bus Host Bridge
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  PnP Device 20
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 21
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 22
    Vendor:                            Generic System Device
    Device Name:                       ACPI power button device
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C0C
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                ACPI Power Button
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C0C
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 23
    Vendor:                            
    Device Name:                       Software Component
    PnP Device ID:                     ACPI\VEN_MBAD&DEV_0001
    Class (08h):                       System Peripheral
    Parent Device:                     ACPI system board hardware
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      Micro-Star INT'L CO., LTD.
    Device Description:                MSI Software Component Interface
    Device Class:                      System
    Driver Provider:                   Micro-Star INT'L CO., LTD.
    Driver Version:                    1.0.0.14
    Driver Date:                       8-20-2024
    Inf File:                          oem2.inf
    Hardware ID:                       ACPI\VEN_MBAD&DEV_0001
    Parent ID:                         ACPI_HAL\PNP0C08
                                       
  PnP Device 24
    Vendor:                            Generic System Device
    Device Name:                       Motherboard registers
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0C02
    Class (08h):                       System Peripheral
    Parent Device:                     PCI Bus Host Bridge
  Device Resources
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                Motherboard resources
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0C02
    Parent ID:                         ACPI\VEN_PNP&DEV_0A08
                                       
  PnP Device 25
    Vendor:                            Generic System Device
    Device Name:                       AT Real-Time Clock
    PnP Device ID:                     ACPI\VEN_PNP&DEV_0B00
    Class (08h):                       System Peripheral
    Parent Device:                     AMD B450 Fusion Controller Hub (FCH)
  Device Resources
    I/O Port:                          70h-71h
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard system devices)
    Device Description:                System CMOS/real time clock
    Device Class:                      System
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.1
    Driver Date:                       6-21-2006
    Inf File:                          machine.inf
    Hardware ID:                       ACPI\VEN_PNP&DEV_0B00
    Parent ID:                         PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
                                       
                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
  USB Printer 1
    Vendor (04A9h):                    Canon
    Device (2660h):                    LaserBase MF3110 Scanner/Printer
    Manufacturer:                      Canon,Inc.
    Product:                           MF3110
    Serial Number:                     2363E2124558
    Device Version:                    0.0
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Protocol (00h):                    Unknown
    Configuration:                     
    USB Version:                       2.0
    Speed:                             480 Mbit/s
    Transfer Type:                     Bulk/Interrupt
    Data Packet Size:                  64 bytes
    Max Power:                         2 mA Self-Powered
    Parent Device:                     AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard USB Host Controller)
    Device Description:                USB Composite Device
    Device Class:                      USB
    Device Location:                   Port_#0014.Hub_#0001
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          usb.inf
    Service Name:                      usbccgp
    Hardware ID:                       USB\VID_04A9&PID_2660&REV_0000
    Compatible ID:                     USB\COMPAT_VID_04A9&DevClass_00&SubClass_00&Prot00
    Parent ID:                         PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
                                       
                  +-----------------------------------------+
                  |            Installed Printers           |
                  +-----------------------------------------+
  Local Printers
  Installed Printer 1
    Printer Name:                      Microsoft Print to PDF
    Printer Port:                      PORTPROMPT:
    Default Printer:                   No
    Printer Type:                      Local
    Print Processor:                   winprint
    Data Type:                         RAW
                                       
                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    16x or x16
    Slot Designation:                  J6B2
    Slot Length:                       Long Length
    Slot ID:                           0
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J6B1
    Slot Length:                       Short Length
    Slot ID:                           1
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J6D1
    Slot Length:                       Short Length
    Slot ID:                           2
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J7B1
    Slot Length:                       Short Length
    Slot ID:                           3
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J8B4
    Slot Length:                       Short Length
    Slot ID:                           4
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J8D1
    Slot Length:                       Short Length
    Slot ID:                           5
  Slot PCI
    Slot Type:                         PCI
    Current Usage:                     In Use
    Data Bus Width:                    32 bit
    Slot Designation:                  J8B3
    Slot Length:                       Short Length
    Slot ID:                           6
  Slot PCI Express x16
    Slot Type:                         PCI Express x16
    Current Usage:                     In Use
    Data Bus Width:                    16x or x16
    Slot Designation:                  J10
    Slot Length:                       Short Length
    Slot ID:                           12
  Slot PCI Express x8
    Slot Type:                         PCI Express x8
    Current Usage:                     Available
    Data Bus Width:                    8x or x8
    Slot Designation:                  J3600 Pcie x8 slot
    Slot Length:                       Short Length
    Slot ID:                           13
  Slot PCI Express x4
    Slot Type:                         PCI Express x4
    Current Usage:                     Other
    Data Bus Width:                    4x or x4
    Slot Designation:                  J3707 Pcie x4 slot
    Slot Length:                       Short Length
    Slot ID:                           32
  Slot PCI Express x4
    Slot Type:                         PCI Express x4
    Current Usage:                     In Use
    Data Bus Width:                    4x or x4
    Slot Designation:                  J3700 PCIE x4 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           2
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3702 PCIE x1 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           3
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3703 PCIE x1 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           4
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3701 M.2 WLAN/BT slot
    Slot Length:                       Short Length
    Slot ID:                           5
                                       
                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1500
    Ext. Designator:                   USB 3.0
  Port 2 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1501
    Ext. Designator:                   USB 3.0
  Port 3 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1502
    Ext. Designator:                   USB-C
  Port 4 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1503
    Ext. Designator:                   USB 3.0
  Port 5 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1504
    Ext. Designator:                   USB 3.1
  Port 6 Network Port
    Int. Connector Type:               None
    Ext. Connector Type:               RJ-45
    Port Type:                         Network Port
    Int. Designator:                   J1503
    Ext. Designator:                   Network
  Port 7 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1704
    Ext. Designator:                   Sata Express
  Port 8 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1705
    Ext. Designator:                   Sata Express
  Port 9 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1701
    Ext. Designator:                   iSATA
  Port 10 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1702
    Ext. Designator:                   iSATA
  Port 11 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1703
    Ext. Designator:                   iSATA
  Port 12 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1706
    Ext. Designator:                   iSATA
  Port 13 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1100
    Ext. Designator:                   HDMI
  Port 14 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1101
    Ext. Designator:                   HDMI
  Port 15 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1102
    Ext. Designator:                   DP
  Port 16 Audio Port
    Int. Connector Type:               None
    Ext. Connector Type:               Mini-jack (headphones)
    Port Type:                         Audio Port
    Int. Designator:                   J2100
    Ext. Designator:                   Front Audio
  Port 17 Audio Port
    Int. Connector Type:               None
    Ext. Connector Type:               Mini-jack (headphones)
    Port Type:                         Audio Port
    Int. Designator:                   J2101
    Ext. Designator:                   Audio Jack
  Port 18 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1700
    Ext. Designator:                   Sata Express
                                       
                  +-----------------------------------------+
                  |                  Power                  |
                  +-----------------------------------------+
  Power
    AC Power Status:                   Online
    Battery Status:                    No Battery
  Power Plan
    Power Plan:                        Balanced
    Sleep After:                       15 min
    Allow Hybrid Sleep:                On
    Fast Startup:                      No
    Hibernate:                         No
    Turn Off Disk After:               20 min
    Turn Off Display After:            5 min
    Power Button Action:               Shut Down
    Sleep Button Action:               Sleep
                                       
                  +-----------------------------------------+
                  |                 Network                 |
                  +-----------------------------------------+
  Network
    Network Name:                      DESKTOP-O18FSDF
    User Name:                         KKV1
    User Role:                         Administrator
    Logon Domain:                      DESKTOP-O18FSDF
  Interface 1
    Network Chip Vendor:               Realtek Semiconductor
    Network Chip:                      RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
    Subsys Vendor:                     Micro-Star International Co Ltd (MSI)
    Parent Device:                     AMD 400 Series Chipset PCIe Port
    Bus Type:                          PCI Express 1.0 x1 2.5 GT/s (Current: x1 2.5 GT/s)
    Bus Bandwidth:                     0.25 GB/sec (Current: 0.25 GB/sec)
    Description:                       Realtek PCIe GbE Family Controller
    Adapter Manufacturer:              Micro-Star INTL CO., LTD.
    MAC Address:                       2C-F0-5D-D2-A7-22
    Adapter Type:                      Ethernet
    Link Speed:                        1000.0 Mbps
    MTU Size:                          1500 byte
    Adapter Status:                    Enabled
    Operational Status:                Operational
    DHCP Enabled:                      Yes
    DHCP Server:                       192.168.1.1
    IP Address:                        192.168.1.15
    IP Address Subnet Mask:            255.255.255.0
    Gateway:                           192.168.1.1
    DNS Server:                        192.168.1.1
                                       
                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
    Monitor Vendor:                    AOC International (TPV Technology)
    Monitor Model:                     Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5
    Viewable Size:                     27.0" (68.5 sm)
    Serial Number:                     7393
    Manufacture Date:                  October 2023
    EDID Version:                      1.4
    Monitor ID:                        AOC2702
    Aspect Ratio:                      16:9
    Horizontal Size:                   597 mm
    Vertical Size:                     336 mm
    Gamma Factor:                      2.200
    Display Type:                      RGB Color
    Input Signal:                      Digital
    Internal Model:                    Q27G2SG4
    Internal Number:                   XFXPAHA007393
    Vertical Frequency:                48-155 Hz
    Horizontal Frequency:              230-230 kHz
    Current Resolution:                2560x1440 32bpp @ 155 Hz
    Parent Device:                     NVIDIA GeForce RTX 3060 Ti LHR [GA104]
  DPMS Features
    Active Off:                        [X]
    Suspend:                           [ ]
    Standby:                           [ ]
  Supported Modes
    Mode 1:                            640x480   @ 60 Hz (VGA)
    Mode 2:                            640x480   @ 67 Hz (Mac II)
    Mode 3:                            640x480   @ 72 Hz (VESA)
    Mode 4:                            640x480   @ 75 Hz (VESA)
    Mode 5:                            640x480   @ 100 Hz
    Mode 6:                            640x480   @ 120 Hz
    Mode 7:                            720x400   @ 70 Hz (VGA)
    Mode 8:                            800x600   @ 56 Hz (VESA)
    Mode 9:                            800x600   @ 60 Hz (VESA)
    Mode 10:                           800x600   @ 72 Hz (VESA)
    Mode 11:                           800x600   @ 75 Hz (VESA)
    Mode 12:                           800x600   @ 100 Hz
    Mode 13:                           800x600   @ 120 Hz
    Mode 14:                           832x624   @ 75 Hz (Mac II)
    Mode 15:                           1024x768  @ 60 Hz (VESA)
    Mode 16:                           1024x768  @ 70 Hz (VESA)
    Mode 17:                           1024x768  @ 75 Hz (VESA)
    Mode 18:                           1024x768  @ 100 Hz
    Mode 19:                           1024x768  @ 120 Hz
    Mode 20:                           1280x1024 @ 60 Hz
    Mode 21:                           1280x1024 @ 75 Hz (VESA)
    Mode 22:                           1920x1080 @ 60 Hz
    Mode 23:                           2560x1440 @ 60 Hz (Recommended)
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      (Standard monitor types)
    Device Description:                Generic PnP Monitor
    Friendly Name:                     Generic Monitor (Q27G2SG4)
    Device Class:                      Monitor
    Driver Provider:                   Microsoft
    Driver Version:                    10.0.22621.3672
    Driver Date:                       6-21-2006
    Inf File:                          monitor.inf
    Service Name:                      monitor
    Hardware ID:                       MONITOR\AOC2702
    Compatible ID:                     *PNP09FF
    Parent ID:                         PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
                                       
                  +-----------------------------------------+
                  |                Video Card               |
                  +-----------------------------------------+
  Video
    Video Chip Vendor:                 NVIDIA Corporation
    Video Chip:                        GeForce RTX 3060 Ti LHR [GA104]
    Subsystem Vendor:                  Micro-Star International Co Ltd (MSI)
    Subsystem ID:                      MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
    Hardware ID:                       VEN_10DE&DEV_2489
    Revision:                          A1h
    GPU Type:                          Desktop Discrete
  Memory
    Video Memory Size:                 8 GB
    Memory Type:                       GDDR6 (Hynix)
    Bus Width:                         256-bit
  Architecture
    Architecture:                      Ampere
    Code Name:                         GA104 A1h
    GPU Variant:                       GA104-202
    Unified Shaders:                   4864
    Texture Mapping Units (TPU):       152
    Render Output Units (ROPS):        64
    Streaming Multiprocessors:         38
    Tensor Cores:                      152
    RT Cores:                          38
    Level 1 Cache:                     4.75 MB
    Level 2 Cache:                     4 MB
    GPU Manufacturer:                  Samsung
    Manufacturing Process:             8 nm
    Transistor Count:                  17400 million
    Die Size:                          392 mm2
    Package Type:                      BGA-2713
    Max TDP:                           200.0 Wattes
    Launch Date:                       May, 2021
  Base Clocks
    Base Core Clock:                   1410 MHz
    Base Memory Clock:                 1750 MHz (Effective: 14000 MHz)
    Memory Bandwidth:                  448.0 GB/s
  Boost Clocks
    Boost Core Clock:                  1695 MHz
    Boost Memory Clock:                1750 MHz (Effective: 14000 MHz)
    Memory Bandwidth:                  448.0 GB/s
  Theoretical Performance
    Estimated Speed:                   35% of GeForce GTX 4090
    Pixel Fillrate:                    108.5 GPixel/s
    Texture Fillrate:                  257.6 GTexel/s
  BIOS
    Bootup Message:                    PG190 SKU 12 VGA BIOS  MSINV397MH.520
    Video BIOS Version:                Version 94.04.46.00.D2
    Video BIOS Date:                   05/19/21
    BIOS Copyright:                    Copyright (C) 1996-2021 NVIDIA Corp.
    Board Model:                       GPU Board
  API Supported
    DirectX Version:                   12 (12_2)
    OpenGL Version:                    4.6
    Shader Model:                      6.7
    Vulkan Version:                    1.3
    CUDA Version:                      8.6
    OpenCL Version:                    3.0
  Other
    Driver Version:                    R572.16
    Parent Device:                     AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x16 8.0 GT/s (Current: x16 5.0 GT/s)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    RAMDAC Type:                       Integrated RAMDAC
  Hardware Monitoring
    Core Temperature:                  49 °C (120 °F)
    Current Core Clock:                210.0 MHz
    Current Video Engine Clock:        555 MHz
    Current Memory Clock:              101.0 MHz (Effective: 808.0 MHz)
    Core Usage:                        1 %
    Memory Usage:                      5 %
    Memory Controller Usage:           55 %
    Video Engine Usage:                0 %
    Bus Interface Load:                0 %
  Performance Profile 0
    Core Clock:                        2100 MHz
    Memory Clock:                      7001 MHz
  Performance Profile 2
    Core Clock:                        6801 MHz
    Memory Clock:                      6801 MHz
  Performance Profile 3
    Core Clock:                        210 MHz
    Memory Clock:                      5001 MHz
  Performance Profile 5
    Core Clock:                        210 MHz
    Memory Clock:                      810 MHz
  Performance Profile 8
    Core Clock:                        210 MHz
    Memory Clock:                      405 MHz
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     15.8 GB/sec (Current: 8.0 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
  Driver
    Driver Status:                     The device is working properly
    Manufacturer:                      NVIDIA
    Device Description:                NVIDIA GeForce RTX 3060 Ti
    Device Class:                      Display
    Device Location:                   PCI bus 41, device 0, function 0
    Driver Provider:                   NVIDIA
    Driver Version:                    32.0.15.7216
    Driver Date:                       1-26-2025
    Inf File:                          oem13.inf
    Service Name:                      nvlddmkm
    Hardware ID:                       PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
    Compatible ID:                     PCI\VEN_10DE&DEV_2489&REV_A1
    Parent ID:                         PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
                                       
                  +-----------------------------------------+
                  |           Hardware Monitoring           |
                  +-----------------------------------------+
  Processor 
    Processor:                         AMD Ryzen 5 5600 3500 MHz
    Core Voltage:                      1.119 V
    Core Voltage (SVI2 TFN):           1.113 V
    SoC Voltage (SVI2 TFN):            1.075 V
    Package Temperature:               53 °C (127 °F)
    CCD1 Temperature:                  53 °C (127 °F)
    SoC Temperature:                   45 °C (113 °F)
    L3 Cache Temperature:              43 °C (109 °F)
    Package Power:                     26.6 Wattes
    Cores Power:                       2.8 Wattes
    SoC Power:                         12.1 Wattes
    VDDIO Mem Power:                   9.2 Wattes
    VDD18 Power:                       0.9 Wattes
    FSB Clock:                         100.0 MHz
  Core 1
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.3 Wattes
    Core Clock:                        3560.0 MHz (Original: 3500 MHz)
    Multiplier:                        35.6
  Core 2
    Temperature Core:                  44 °C (111 °F)
    Core Power:                        0.6 Wattes
    Core Clock:                        3560.0 MHz (Original: 3500 MHz)
    Multiplier:                        35.6
  Core 3
    Temperature Core:                  44 °C (111 °F)
    Core Power:                        0.6 Wattes
    Core Clock:                        4450.0 MHz (Original: 3500 MHz)
    Multiplier:                        44.5
  Core 4
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.0 Wattes
    Core Clock:                        3560.0 MHz (Original: 3500 MHz)
    Multiplier:                        35.6
  Core 5
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.0 Wattes
    Core Clock:                        3560.0 MHz (Original: 3500 MHz)
    Multiplier:                        35.6
  Core 6
    Temperature Core:                  42 °C (108 °F)
    Core Power:                        0.1 Wattes
    Core Clock:                        3560.0 MHz (Original: 3500 MHz)
    Multiplier:                        35.6
  Video Card 
    Video Chip:                        GeForce RTX 3060 Ti LHR [GA104]
    Core Temperature:                  49 °C (120 °F)
    Current Core Clock:                210.0 MHz (Original: 1410 MHz)
    Current Memory Clock:              101.0 MHz (Original: 1750 MHz)
    Core Usage:                        1 %
    Memory Usage:                      5 %
    Memory Controller Usage:           55 %
    Video Engine Usage:                0 %
    Bus Interface Load:                0 %
  Disk Drive 1 
    Disk Model:                        Samsung SSD 860 EVO 250GB
    Disk Temperature:                  37 °C (99 °F)
    Total Host Writes:                 63.98 TB
  Disk Drive 2 
    Disk Model:                        WDC WD1001FALS-00J7B0
    Disk Temperature:                  42 °C (108 °F)
  Disk Drive 3 
    Disk Model:                        HGST HTS541010A9E680
    Disk Temperature:                  30 °C (86 °F)
  Disk Drive 4 
    Disk Model:                        Samsung SSD 970 EVO Plus 1TB            
    Disk Temperature:                  47 °C (117 °F)
    Total Host Writes:                 9.18 TB
    Total Host Reads:                  15.06 TB
                                       
                  +-----------------------------------------+
                  |          Drivers Troubleshooter         |
                  +-----------------------------------------+
  List of Problem Devices
  Problem Device 1
    Device Type:                       PCI/AGP Device
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1481h):                    Starship/Matisse IOMMU
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (08h):                       System Peripheral
    SubClass (06h):                    IOMMU
    Hardware ID:                       VEN_1022&DEV_1481
    Revision:                          00h
    Driver Status:                     The drivers for this device are not installed
  Problem Device 2
    Device Type:                       USB Device
    Vendor (04A9h):                    Canon
    Device (2660h):                    LaserBase MF3110 Scanner/Printer
    Manufacturer:                      Canon,Inc.
    Product:                           MF3110
    Device Version:                    0.0
    Class (00h):                       Unknown
    SubClass (00h):                    Unknown
    Hardware ID:                       VID_04A9&PID_2660
    Protocol (00h):                    Unknown
  Interface 1
    Class (FFh):                       Vendor Specific Class
    SubClass (00h):                    Unknown
    Protocol (FFh):                    Unknown
    Interface:                         
  Driver
    Driver Status:                     The drivers for this device are not installed (28)
    Device Description:                MF3110
    Device Location:                   0003.0000.0000.014.000.000.000.000.000
    Hardware ID:                       USB\VID_04A9&PID_2660&REV_0000&MI_00
    Compatible ID:                     USB\COMPAT_VID_04a9&Class_ff&SubClass_00&Prot_ff
    Parent ID:                         USB\VID_04A9&PID_2660&REV_0000
                                       
                  +-----------------------------------------+
                  |            Disk Diagnostics             |
                  +-----------------------------------------+
  Disk 1 Status
    Disk Model:                        Samsung SSD 860 EVO 250GB
    Disk Size:                         238475 MB (232.89 GB)
    Interface Type:                    Serial ATA III (SATA/600)
    Serial Number:                     S3Y9NB0K275545B
    Controller Revision:               RVT01B6Q
    Disk Marketing Size:               250059 MB (250.06 GB)
    Buffer Size:                       Unknown
    Location:                          AMD 400 Series Chipset SATA Controller
    Disk Temperature:                  37 °C (99 °F)
    Reallocated Sectors:               0
    Disk Health Status:                Good
    SSD Remaining Life:                83 %
    Total Host Writes:                 63.98 TB
                                       
  Disk 2 Status
    Disk Model:                        WDC WD1001FALS-00J7B0
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    Serial ATA II (SATA/300)
    Serial Number:                     WD-WMATV0357962
    Controller Revision:               05.00K05
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Buffer Size:                       32767.5 kB
    Location:                          AMD 400 Series Chipset SATA Controller
    Disk Temperature:                  42 °C (108 °F)
    Reallocated Sectors:               2
    Disk Health Status:                Poor
                                       
  Disk 3 Status
    Disk Model:                        HGST HTS541010A9E680
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    Serial ATA III (SATA/600)
    Serial Number:                     JDA0001V16XKSH
    Controller Revision:               JA0OA560
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Buffer Size:                       8192.0 kB
    Location:                          AMD 400 Series Chipset SATA Controller
    Disk Temperature:                  30 °C (86 °F)
    Reallocated Sectors:               0
    Disk Health Status:                Poor
                                       
  Disk 4 Status
    Disk Model:                        Samsung SSD 970 EVO Plus 1TB            
    Disk Size:                         953869 MB (931.51 GB)
    Interface Type:                    NVMe 1.3.0
    Serial Number:                     S6P7NF0T435103B     
    Controller Revision:               4B2QEXM7
    Disk Marketing Size:               1000204 MB (1000.2 GB)
    Buffer Size:                       Unknown
    Location:                          Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
    Disk Temperature:                  47 °C (117 °F)
    Disk Health Status:                Good
    SSD Remaining Life:                100 %
    Total Host Writes:                 9.18 TB
    Total Host Reads:                  15.06 TB
                                       
                  +-----------------------------------------+
                  |                 Windows                 |
                  +-----------------------------------------+
  Windows
    Operating System:                  MS Windows 11 Professional x64 Edition
    OS Type:                           x64 (64-bit)
    Version:                           22H2
    Build Number:                      10.0.22621.4317
    OS Language:                       Russian (Russia)
    Windows Folder:                    J:\Windows
    Installation Date:                 03 February 2025
    Kernel Type:                       Multiprocessor Free
    Registered Owner:                  KKV1
    Registered Organization:           
    Product ID:                        00330-80000-00000-AA702
    Product Key:                       XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
    System UpTime:                     0 Hour(s) 12 Minutes 44 Seconds
    IE Version:                        9.11.22621.0
    DirectX Version:                   DirectX 12 (10.00.22621.1)
  Regional Settings
    Country:                           Russia
    Language:                          Russian
    Time Zone:                         Central America Standard Time (GMT-6)
    Currency Name:                     Russian Ruble
    Measurment System:                 Metric
    ANSI Code Page:                    1251
    OEM Code Page:                     866
                                       
                  +-----------------------------------------+
                  |            Installed Programs           |
                  +-----------------------------------------+
  Installed Programs
     Program Name                                       | Version        |                      Publisher|       Date|      Size| 
     ---------------------------------------------------+----------------+-------------------------------+-----------+----------+------
     ASTRA32 - Advanced System Information Tool         | 4.20           |                    Sysinfo Lab|           |          | 
                                       
                  +-----------------------------------------+
                  |            Installed Hotfixes           |
                  +-----------------------------------------+
  Installed Hotfixes
    Security Update for Microsoft Windows (KB5044285):
    Security Update for Microsoft Windows (KB5046247):
    Update for Microsoft Windows (KB5028756):
                                       
                                [End of Report]                               
