[ Dual Core Center ]
1. MSI hardware monitor & overclock & fan control Tool & Voltage control
2. Dynamic overclock I & Dynamic overclock II for motherboard & VGA

Support list: 
[DualCoreCenter]
	refer to below note

[Green Power Center]
	MS-7374,MS-7375,MS-7512,MS-7513,MS-7516,MS-7532

VGA:(full function support model)
	ati:	V044
	nvidia: V046,V060,V069
	v1.0.2.5 start to support all nVidia/ATI AGP/PCI-E VGA Card

OS : Windows XP32,Vista32/64 (not support XP64)
=========================================================================
	DCC version 2.0.5.5 (2009/04/15)
		a. support AM3 600e,605e,400e,405e (CPUID=0xF52)
		b. modify MS-7592 CPUID 0x6F2,0x6FD cpu temp.(minus 5 degrees)
=========================================================================
	DCC version 2.0.5.4 (2009/04/02)
		a. modify MS-7521 0x676 CPU temp.
		b. fix F71889 initial value
=========================================================================
	DCC version 2.0.5.3 (2009/03/20)
		a. new mainboard:
			MS-7597 v1.0 (nVidia MCP61P, F71889, A7597NMS.10A, overclock)
		b. modify MS-7592 some cpu temp. for CPUID=0x6F2,0x6FD,0x67A,0x677
		c. modify MS-7302 CPUID=0xFB2 cpu temp.
=========================================================================
	DCC version 2.0.5.2 (2009/03/18)
		a. support Phenom II X3 720 and X4 9850
		b. support MS-7549 v1.3 (RTM880N-793)
		c. modify MS-7549 cpu temp. (CPUID=0xFB2)
		d. add support AM2 CPUID=0xFB0~0xFBF
		e. fix MS-7376 v1.0 w/ 9LPRS477BKL FSB reading
=========================================================================
	DCC version 2.0.5.1 (2009/02/24)
		a. adjust MS-7574-03S v1.1, MS-7521 some cpu temperature
		b. adjust MS-7574-03S CPUID=0x67A,0x676 cpu temp.
		c. fix MS-7521 v1.2 +12V voltage
=========================================================================
	DCC version 2.0.5.0 (2009/01/06)
		a. support Athlon Orleans/Sparta,Sempron Manila serials(CPUID:0xFF2)
=========================================================================
	DCC version 2.0.4.9 (2008/12/29)
		a. modify MS-7592 0x6FD,0x6F2,0x676,0x677 cpu temperature
		b. modify MS-7514 v2.0 some cpu temperature
=========================================================================
	DCC version 2.0.4.8 (2008/12/19)
		a. support AM2+ CPU Ratio reading (CPUID: 0xF20~0xF2F,0xF40~0xF4F)
		b. add MS-7592 over-fsb items
		c. modify MS-7574,7592 some cpu temperature
=========================================================================
	DCC version 2.0.4.7 (2008/12/08)
		a. new mainboard:
			MS-7526 v2.0 (Intel G45+ICH10, 9LPRS113, F71882, watch-dog)
		b. modify MS-7529,7528,7549 some cpu temperature
		c. new mainboard:
			MS-7592 v0A (Intel G41+ICH7, RTM875T-605, F71889)
	GPC version 1.0.2.3 (2008/12/09)
		a. modify MS-7512 ddr/nb voltage items by A7512IMS.156
		b. update FlashSys64.sys(02/15)
=========================================================================
	DCC version 2.0.4.6 (2008/11/26)
		a. fix MS-7574 FSB800 CPU show wrong fsb issue
		b. fix DOT down failed issue
=========================================================================
	DCC version 2.0.4.5 (2008/11/14)
		a. add RTM875T-605 PLL3 over-pcie for overclock
		b. modify MS-7514 v3.0 some cpu temperature
		c. modify MS-7564 some cpu temperature
		d. support MS-7514 v3.0 cpu voltage(uP6262)
=========================================================================
	DCC version 2.0.4.4 (2008/11/07)
		a. fix MS-7563,7564 adjust voltage unstable issue
		b. support MS-7514 v3.0
		c. add MS-7563 RTM875T-605 overclocking
		d. new mainboard:
			MS-7574 v0A (Intel G41+ICH7, RTM875T-605, F71882FG)
		e. modify MS-7514 v3.0 DDR/NB Voltage items by A7514IMS.704
=========================================================================
	DCC version 2.0.4.3 (2008/10/20)
		a. new mainboard:
			MS-7515 v1.0 (Intel G45+ICH10, 9LPRS113, F71882FG, watch-dog, A7515IMS.10C)
			MS-7364 0vA (Intel G41+ICH7, 9LPRS113, F71882FG, watch-dog)
			MS-7563 v0A (Intel G41+ICH7, RTM875T-605, F71882FG)
			MS-7572 v0A (Intel P45+ICH10, 9LPRS113, F71882FG, watch-dog)
		b. modify MS-7519 v2.0 0x676,0x677,0x6FB,0x6F7 cpu temperature
=========================================================================
	DCC version 2.0.4.2 (2008/10/08)
		a. new mainboard:
			MS-7519 v2.0 (Intel P45+ICH10, 9LPRS113, F71882FG, A7519IMS.404, DDR3 module)
			MS-7560 v0B (nVidia MCP72P, ClockGen: memory, F71882FG, A7560NMS.105)
		b. modify MS-7383 0x6F6,0x6FB,0x677 cpu temperature
=========================================================================
	DCC version 2.0.4.1 (2008/09/24)
		a. support MS-7314 v2.0
		b. modify MS-7383 v1.0 (A7383IMS.120) nb voltage items
		c. support MS-7511 v1.3 (A7511IMS.304, not support over cpu voltage)
	GPC version 1.0.2.2 (2008/09/24)
		a. modify 9600GT DOT2 detection between DCC and GPC
=========================================================================
	DCC version 2.0.4.0 (2008/09/12)
		a. update VGADLL.dll(08/28) for 9600GT fan control
		b. fine tune OC button flag to fix cpu heavy usage
		c. fix greenpower vga initial, mode status pic
		d. remove dot button in VGA mode
		e. disable Overclock for MS-7530,MS-7533 (MCP7A)
		f. finally update VGADLL.dll(09/08) for 9600GT
=========================================================================
	DCC version 2.0.3.9 (2008/08/27)
		a. update VGADLL.dll(08/22) for 9600GT fan and temperature
		b. remove SetRegular() for DOT2 button
		c. Enable MS-7550 RTM880N-739 Byte0x1F Bit7
		d. fix MS-7552,MS-7550 3.3V,5V,12V abnormal
=========================================================================
	DCC version 2.0.3.8 (2008/08/21)
		a. fix MS-7551 v1.0 +12v voltage
		b. for 9600GT:
			- update VGADLL.dll(08/19) for fan (Init: 0, GPUTemp>70, Fan roll)
			- add warning message box for OC button
			- modify total power saving
			- add OC button flag to fix cpu heavy usage
			- disable pop-up dialog and sound warning when fan stop
			- modify total power saving unit from W/hr to W/5hr
		c. support MS-7550 v1.2 w/ v114 bios
		d. add RTM880N-793 watch-dog
=========================================================================
	DCC version 2.0.3.7 (2008/08/05)
		a. new mainboard:
			MS-7558 v0A (Intel P45+ICH10, 9LPRS113AKLF, F71882FG)
			MS-7514 v1.1(Intel P45+ICH10, 9LPRS113AKLF, F71882FG)
			MS-7549 v0A (ATI RS780V+SB750, 9LPES477CKL, F71882FG)
=========================================================================
	DCC version 2.0.3.6 (2008/08/01)
		a. support MS-7514 v2.0
		b. support VGA 9600GT OC button
		c. modify PowerSaving value for 9600GT
		d. new mainboard:
			MS-7388 v3.0 (ATI RX780+SB700, RTM880N-793, F71882FG)
=========================================================================
	DCC version 2.0.3.5 (2008/07/22)
		a. fix AM2 cpu show wrong fsb for MS-7552
		b. support MS-7532 v1.0 Combo DDR2/3
		c. modify MS-7532 v1.0 cpu/ddr/nb voltage items by v10D bios
		d. add Green Power button for VGA page
		e. remove MS-7532 Green Power support
	GPC version 1.0.2.1 (2008/07/22)
		a. remove MS-7532 v0A support
=========================================================================
	DCC version 2.0.3.4 (2008/07/08)
		a. support MS-7550,7551 cpu/nb voltage adjustment, and modify 5v,12v voltage
		b. new mainboard:
			MS-7552 (ATI RS780+SB700, ICS 9LPRS477CKL, F71882FG)
=========================================================================
	DCC version 2.0.3.3 (2008/07/02)
		a. new mainboard:
			MS-7550 (ATI RS780D+SB750, RTM880N-793, F71882FG)
			MS-7551 (ATI RS780/RX780+SB700, RTM880N-793, F71882FG)
	GPC version 1.0.2.0 (2008/06/30)-for MB version
		a. max power saving mode will not adjust north bridge voltage
		b. fixed optimize mode ratio error on vista		
=========================================================================
	DCC version 2.0.3.2 (2008/06/23)
		a. modify cpu temperature(0x6FD,0x6FB,0x10677) for MS-7528
		b. modify cpu temperature(0x6FD,0x6F6,0x10677) for MS-7529
		c. support MS-7376 v1.0 w/ 9LPRS477BKL/CKL
	GPC version 1.0.1.8 (2008/06/12)-for MB version
=========================================================================
	DCC version 2.0.3.1 (2008/06/12)
		a. fix MS-7353 v3.0/MS-7338 Combo DDR2/3 read error issue
		b. fix MS-7528 v1.0 overclock failed issue
		c. fix MS-7388 v1.0 w/ 9LPRS477BKL/CKL read fsb failed issue
	GPC version 1.0.1.8 (2008/06/12)-for MB version
=========================================================================
	DCC version 2.0.3.0 (2008/06/10)
		a. fix MS-7392(w/ v2.xx bios) show wrong FSB
		b. modify MS-7392 CPU/NB voltage items, cpu temperature
	GPC version 1.0.1.7 (2008/06/9)-for MB version
		a. check if CPU_FSB=400 , not to adjust MCH Voltage on 'MAX POWER SAVING' mode.
		b. fixed "OCZ3P1333"(DDR3) default voltage error.(1.9V)
=========================================================================
	DCC version 2.0.2.9 (2008/06/3)
	GPC version 1.0.1.6 (2008/06/3)-for MB version
		a. fixed access Smbus error on EFI Bios.
		b. restore CPU/MCH/ICH/DDR voltage value before restart system(to avoid 'ff' debug message).
=========================================================================
	DCC version 2.0.2.8 (2008/06/02)
		a. modify MS-7508 NB voltage items
	GPC version 1.0.1.5 (2008/06/02)
		a. support new VGA: V245
=========================================================================
	DCC version 2.0.2.7 (2008/05/30)
	GPC version 1.0.1.4 (2008/05/30)
		a. fixed detect system power monitor device error.
=========================================================================
	DCC version 2.0.2.6 (2008/05/30)
	GPC version 1.0.1.3 (2008/05/30)
		a. add driver to installation program
		b. fixed 2 core CPU redundant ratio access
=========================================================================
	DCC version 2.0.2.5 (2008/05/29)
	GPC version 1.0.1.2 (2008/05/29)
		a. Change ICH vol value table (2.15~2.27 warning value , remove 2.30~3.41)
		b. Detect CPU APIC ID for each core to ensure ratio is changed.(fixed 'MAX POWER SAVING' mode adjust 4 core CPU Vcore error)
=========================================================================
	DCC version 2.0.2.4 (2008/05/29)
	GPC version 1.0.1.1 (2008/05/29)
		a. fixed 'MAX POWER SAVING' mode adjust 4 core CPU Vcore error.
=========================================================================
	DCC version 2.0.2.3 (2008/05/28)
	GPC version 1.0.1.0 (2008/05/28)
		a. 'MAX POWER SAVING' mode adjust CPU Vcore under 1V , and MCH under 1V too.
		b. change 'High Performance Mode' to be 'Optimize Mode'
=========================================================================
	DCC version 2.0.2.2 (2008/05/26)
		a. new mainboard:
                        MS-7532 v0A  (Chipset: Intel P45+ICH10, ClockGen: ICS9LPRS113AKLF, F71882FG)
			MS-7314 v1.0 (Chipset: Intel 945G+ICH7, ClockGen: RTM876-665, F71882FG)
			MS-7533 v0B  (Chipset: nVidia MCP7A, F71882FG)
		b. modify MS-7314 sysfan1/2 location
	GPC version 1.0.0.8 (2008/05/26)
		a. changed DDR2 voltage table for MS-7512
		b. add 'load setting' and 'apply' button
		c. add message for CPU phase is changed by CPU loading
		d. fixed CPU ratio changed error (not AHCI mode)
=========================================================================
	DCC version 2.0.2.1 (2008/05/16)
		a. modify MS-7511 NB voltage item
	GPC version 1.0.0.5 (2008/05/16)
		a. changed button text color(blue -> deep green).
		b. Support OCZ3P1600EB2GK (DDR3. Default=1.9V)
		c. Max Power Saving/high performance mode adjust ratio = min ratio.
		d. CPU usage > 40% changed high performance mode ratio = max ratio
=========================================================================
	DCC version 2.0.2.0 (2008/05/15)
		a. support Intel Wolfdale/Yorkfield CPU(CPUID:0x670-0x67F)
	GPC version 1.0.0.4 (2008/05/14)
		a. offset low value warning for P45+DDR3
		b. if(MCH > VTT)set fake MCH or VTT
		c. add CPU smart fan
=========================================================================
	DCC version 2.0.1.9
	GPC version 1.0.0.3 (2008/05/13)
		a. changed disable mode to be default mode
		b. if (MCH > VTT + 0.2) set fake MCH or VTT
		c. add low value warning, and confirm dialog
=========================================================================
	DCC version 2.0.1.8 (2008/05/13)
		a. support Green Power Center for MS-7375 v1.1,MS-7516 v1.0,MS-7374,MS-7512
		b. modify cpu voltage format be +/- sign
		c. fix MS-7388 overclock issue for changing clock for 477b to 477c
		d. new mainboard:
                        MS-7530 v0A  (Chipset: MCP7A, F71882FG, A7530NMS.103)
		e. update VGADLL.dll(04/22)
		f. modify "NB" to be "MCH" string
		g. delay to show icon in taskbar
	GPC version 1.0.0.2 (2008/05/12)
		a. set max cpu phase when close GreenPowerCenter for MS-7512,7513,7516		
		b. update fan control of Green Power Center
		c. support disable/manual/'high performance'/'max power saving' mode
		d. fixed S1/S3/S4 failed
		e. fixed manual mode save function error 
		f. set adjust vcore & ddr voltage timer (100 ms per step)
		g. fixed VTT FSB voltage table error
		h. change ICH voltage table for MS-7513,MS-7516
=========================================================================
	version 2.0.1.7 (2008/03/27)
		a. new mainboard:
                        MS-7514 v0B  (Chipset: Intel Eaglelake+ICH10, ClockGen: ICS9LPRS113AKLF-T, F71882FG, A7514IMS.10D)
                        MS-7519 v0B  (Chipset: Intel Eaglelake+ICH10, ClockGen: ICS9LPRS113AKLF-T, F71882FG, A7519IMS.10B)
                        MS-7521 v0a  (Chipset: Intel Eaglelake+ICH10, ClockGen: ICS9LPRS110AKLF-T, F71882FG, A7521IMS.106)
			MS-7375 v1.0 (Chipset: nVidia MCP72, ClockGen: memory, F71882FG, A7375NMS.108, wattage monitor)
			MS-7513 v0B  (Chipset: P45+ICH9, ClockGen: 9LPRS110AKLF, F71882FG, watch-dog, wattage monitor)
			MS-7516 v0B  (Chipset: P45+ICH9, ClockGen: 9LPRS113AKLF, F71882FG, watch-dog)
                        MS-7533 v0A (Chipset:   MCP7A,   F71882FG, A7533NMS.103)
                b. fix MS-7501 show the wrong value issue for changing ClkGen.
		c. fix MS-7368 v1.0 read FSB wrong issue
		d. modify MS-7513 wattage monitor formula
		e. fix FlashSys64.sys digital sign issue
		f. support MS-7513 adjust cpu voltage
		g. update VGADLL.dll memory clock*2 for 9800GX2(Device id:0604),9800GTX
		h. fix MS-7523 FSB overclock issue
		i. add support Green Power Center for MS-7513
		j. support VGA function(power saving,total power saving), remove GPU temp field
                k. fix MS-7302 cpu temperature show low value issue
                l. fix 7392 shows wrong FSB when using 200 CPU because the clkgen was changed from 906 to 908(divider for 200 changed from 2 to 4)
=========================================================================
	version 2.0.1.6 (2008/1/29)
		a. new mainboard:
			MS-7527 v0a  (Chipset: Intel 945+ICH7, ClockGen: RTM876-665, F71882FG, A7527IMS.004)
			MS-7529 v0a  (Chipset: Intel 945+ICH7, ClockGen: RTM876-665, F71882FG, A7529IMS.005)
                        MS-7514 v0a  (Chipset: Intel Eaglelake+ICH10(actually use ICH9), ClockGen: ICS9LPRS110AKLF-T, F71882FG, A7514IMS.106)
                        MS-7519 v0a  (Chipset: Intel Eaglelake+ICH10(actually use ICH9), ClockGen: ICS9LPRS110AKLF-T, F71882FG, A7519IMS.106)
                        MS-7523 v0a  (Chipset: nVidia C73+MCP55, ClockGen: C73NVRAM, F71882FG, A7523NMS.106, No Watch-dog)  
                b. fix MS-7302 show the wrong value issue for changing ClkGen.
                c. add MS-7374 vcore adjust function.
		d. modify MS-7388 v1.0 9LPRS477BKL clockgen type
                e. modify K8 CPU and Conroe CPU OverClock FSB Limit.
                f. update VGADLL.dll(N9600GT,DID:0622) for VGA Device ID support memory clock*2
                g. fix MS-7529 and MS-7528 show cpu temperature low issue
                h. change vgadll.dll for ati vga overclock
                i. add MS-7376 cpu voltage adjust function.
                j. update VGADLL.dll memory clock*2 for
			N9600GT(DID:0622), V116(8400,DID:06E4), V088(8600GT,DID:0x0401)
=========================================================================
	version 2.0.1.5 (2008/1/3)
                a. disable VGA CLOCK for MS-7302
                b. fix MS-7250 v1.0 ddr voltage show wrong by correct smbus base adress
                c. fix MS-7302 5v voltage show wrong value and sys2 fan show wrong position
                d. add MS-7510 "ECO" function 
                e: new mainboard:
		        MS-7501 v0A  (Chipset: ATI RS780+SB700, ClockGen: ICS 9LPRS477, F71882FG, A7501AMS.104)
                        MS-7528 v0a  (Chipset: Intel 945+ICH7, ClockGen: RTM876-665, F71882FG, A7528IMS.005)
			MS-7380 v1.0 (Chipset: nVidia C72+MCP55, ClockGen: NVAPI, F71882FG, A7380NMS.10G, No Watch-dog)
                        MS-7509 v0A (Chipset: MCP78+MCP78, F71882FG, A7509NMS.103)
                        MS-7390 v0A (Chipset: nVidia MCP65, ClockGen: NVAPI, F71882FG, A7390NMS.103)
                f: update FlashSys.sys and FlashSys64.sys
                g: fix MS-7395 fsb show wrong value issue for changing clockgen.
                h: change vgadll.dll for ati vga overclock.
=========================================================================
	version 2.0.1.4 (2007/12/06)
		a. new mainboard:
			MS-7511 v0A (Chipset: MCP78+MCP78, F71882FG, A7511NMS.109)
			MS-7508 v0A (Chipset: MCP78+MCP78, F71882FG, A7508NMS.104)
                b. change NVidia fsb read from bios,not use rdtsc.
                c. fix MS-7366 show wrong FSB issue.
                d. update VGADLL.dll(8800GS-512,DID:0600,11/13) for VGA Device ID support memory clock*2
		e. new mainboard:
			MS-7327 v1.1 (Chipset: ATI RS690+SB600, F71882FG, ClockGen: RMT870T-691, no overclock/WD, A7327AMS.201)
                        MS-7313 v0A  (Chipset: Intel 945+ICH7, ClockGen: RTM876-665, F71882FG, A7313IMS.104)
                        MS-7302 v0A  (Chipset: ATI RS780/RS740+SB700, ClockGen: ICS 9LPRS477, F71882FG, A7302AMS.104)
                        MS-7510 V0B  (Chipset: nVidia MCP55,F71882FG)
                f. change NS-7313 not support fsb overclock and dot.
                g. update ntuneoem.dll(v5.5.14.0) to fix MS-7369 fsb show wrong and can not overlock issue
                f: fix MS-7518 FSB show wrong value issue.
=========================================================================
	version 2.0.1.3 (2007/10/31)
		a. new mainboard:
			MS-7507 v0A (Chipset: Intel 945+ICH7, ClockGen: RTM876-665, F71882FG, A7507IMS.108)
			MS-7518 v0B (Chipset: nVidia MCP73, F71882FG)
			MS-7506 v1.0 (Chipset: nVidia MCP63, F71882FG)
		b. update VGADLL.dll(8400GS,DID:0404) for VGA Device ID support memory clock*2
		c. fix MS-7366 FSB800(cpuid=0x6f2) show wrong clock issue
		d. modify MS-7349 cpu temperature
=========================================================================
	version 2.0.1.2 (2007/10/19)
		a. fix Conroe_D,CedarMill CPU divisor for MS-7353
		b. fix MS-7376 overclock failed under Vista
		c. fix MS-7376 fan location
=========================================================================
	version 2.0.1.1 (2007/10/15)
		a. update VGADLL.dll(07/25) for VGA Device ID support memory clock*2
		b. add new ACEBridge.dll and delete ACEAssembly.dll from package.
		c. support AMD AM2+ Phenom X4 CPU (CPUID=0xF20~0xF2F)
		d. new mainboard:
			MS-7505 v0A (Chipset: nVidia MCP73, F71882FG, A7505NMS.103)
			MS-7353 v1.0 (Chipset: Intel X38+ICH9R, ClockGen: ICS 9LPRS910, F71882FG, MS7 WD)
			MS-7398 v0A (Chipset: Intel 945+ICH7, ClockGen: RTM876-660, F71882FG)
		e. add MS-7366 v0B DDR Voltage and Sysfan2 show NA
		f. fix Conroe-L FSB800 (CPUID=0x660,0x661) display FSB error issue
		g. fix MS-7388 v1.0 display cpu clock error issue
		h. modify MS-7388 v1.0 DDR/NB Voltage items for A7388AMS.10J
		i. add MS-7353 v1.0 HW Monitor "Pout" efficiency function
		j. support nVidia 8800GT (DID:0x0611) memory clock*2
		k. fix MS-7398 v0A overclock failed under Vista32/64
=========================================================================
	version 2.0.1.0 (2007/09/13)
		a. update VGADLL.dll(07/25) for VGA Device ID support memory clock*2
		b. new mainboard:
			MS-7395 v0A (Chipset: Intel Bearlake+ICH9, ClockGen: ICS 9LPRS906, F71882FG)
			MS-7373 v0A (Chipset: ATI RS690C+SB600, ClockGen: RMT870T-691, F71882FG)
			MS-7366 v0A (Chipset: nVidia MCP73, no support overclock, F71882FG)
			MS-7388 v0A (Chipset: ATI RS780/RD780+SB600, ClockGen: ICS 9LPRS472, F71882FG, A7388AMS.108)
                        MS-7376 V0b (Chipset: ATI RS780/RD780+SB600, ClockGen: ICS 9LPRS477, F71882FG, A7376AMS.107)
		c. modify MS-7373 DOT max range be 7%, disable DDR voltage adjustment by PM request
		d. new mainboard:
			MS-7392 v2.0 (Chipset: Intel P31+ICH7, ClockGen: ICS 9LPRS906, F71882FG)
		e. support MS-7357 v1.0 EIST function
		f. fix get FSB from MN failed when MS-7392 v2.0 EIST option is disable
		g. temporarily use old VGADLL.dll for ATI MB
		h. new mainboard:
			MS-7388 v1.0 (Chipset: ATI RS780/RD780+SB600, ClockGen: ICS 9LPRS477, F71882FG, A7388AMS.10H)
                i. adjust maxclock read from dmi.         
=========================================================================
	version 2.0.0.9 (2007/07/24)
		a. new mainboard:
			MS-7387 v0A (Chipset: VIA P4M900+VT8237S, ClockGen: ICS 9LPR904AGLF, W83627DHG, MS7 WD)
			MS-7382 v0A (Chipset: ATI RS690+SB600, ClockGen: RMT870T-691, F71882FG)
			MS-7392 v0A (Chipset: Intel P31+ICH7, ClockGen: ICS 9LPRS514, F71882FG)
		b. add VT8237S ISA Bridge for MS-7387
		c. patch MS-7392 overclock failed(9LPRS514 Byte21)
		d. fix MS-7320 v1.0 show wrong voltages under Vista64
		e. new mainboard:
			MS-7359 v1.0 (Chipset: Intel Bearlake+ICH9, ClockGen: ICS 9LPRS906CGLF, E71882FG, MS7 WD)
			MS-7383 v2.0 (Chipset: Intel G31+ICH7, ClockGen: RTM876-660, W83627DHG)
		f. update VGADLL.dll,VBios.dll(07/19)
		   update ACEAssembly.dll, ACEBridge.dll(07/23) for ATI VGA Card
		   modify installed path to \program files\msi for ATI VGA Card
		g. fix MS-7346 bios v1.10 DMI check be "1.0"
		h. add warning message when apply CPU/GPU clock
=========================================================================
	version 2.0.0.8 (2007/05/31)
		a. new mainboard:
			MS-7349 v1.0 (Chipset: nVidia MCP68/78, ClockGen: NVAPI, F71882FG, A7349NMS.20B)
			MS-7358 v1.0 (Chipset: Intel Q35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG)
			MS-7383 v0A (Chipset: Intel G31+ICH7, ClockGen: RTM876-660, W83627DHG)
			MS-7379 v0A (Chipset: Intel G31+ICH7, ClockGen: RTM876-660, W83627DHG)
		b. extend MS-7356 manual Max FSB be 1.8 multiple
		c. disable MS-7349 overclock and fan control
=========================================================================
	version 2.0.0.7 (2007/05/18)
		a. fix cpu usage show 100% issue under Vista64
		b. modify DDR adjustment when DOT
		c. fix Conroe CPU show 200 for MS-7236 v2.5(not support FSB266)
		d. modify MS-7362 v1.0 cpu temp. register be bank1 0x50h		
		e. new mainboard:
			MS-7338 v1.0 (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7338IMS.109)
			MS-7356 v1.0 (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7356IMS.10D)
		f. fix overclock failed after resume from suspend with unsupported MB
		g. support MS-7338 v1.0 combo DDR2/DDR3
		h. remove MS-7362 v1.0 DOT/FSB Overclock function
		i. support Conroe FSB1333 (CPUID=0x6F9,0x6FB)
			   Conroe-L FSB800 (CPUID=0x660,0x661)
		j. new mainboard:
			MS-7345 v1.1 (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7345IMS.114)
		k. add ICS 9LPRS906 watch dog for MS-7338,MS-7345,MS-7356
=========================================================================
	version 2.0.0.6 (2007/04/26)
		a. disable MS-7367 overclock(DOT) function (bios not support)
		b. add MS-7317 v1.0 EIST register(A7317SMS.10B)
		c. add DDR adjustment when DOT
		d. modify MS-7337 v1.0 sys temp. from 0x74h to 0x76h
		e. add MS-7365 watch-dog(byte9)
		f. new mainboard:
			MS-7357 v0A (Chipset: Intel Bearlake+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7357IMS.103)
			MS-7364 v1.0 (Chipset: VIA P4M900+VT8237A, ClockGen: ICS 9LPR704AGLF, MS7 WD, W83627EHG, A7364VMS.304)
		g. fix CedarMill cpu divisor error issue for MS-7364 v1.0
		i. fix MS-7337 v1.0 FSB/clock error under Vista32/64
		j. modify FSB266 CPU show 200 for MS-7267(not support FSB266)
		k. new mainboard:
			MS-7369 v0A (Chipset: nVidia MCP65, ClockGen: NVAPI, W83627DHG, A7369NMS.105)
			MS-7236 v2.5 (Chipset: 945PL+ICH7, ClockGen: 954519BGLF, F71882FG, A7236IMS.B00)
		l. show -0%,-3% only for MS-7364 v1.0 down-clock
		m. fix CedarMill cpu divisor error issue for MS-7246 v2.1
=========================================================================
	version 2.0.0.5 (2007/03/22)
		a. new mainboard:
			MS-7267 v4.0 (Chipset: Intel 945+ICH7, ClockGen: ICS 954519BGLF, MS7 WD, F71882FG)
			MS-7331 v1.0 (Chipset: VIA P4M900+VT8237A, ClockGen: ICS 953002DFLF, not support DOT overclock)
			MS-7345 v0B (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7345IMS.105)
			MS-7338 v0B (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906BGLF, F71882FG, A7338IMS.102)
			MS-7362 v0A (Chipset: Intel Broadwater+ICH8, ClockGen: ICS 9LPRS514EGLF, W83627DHG, A7362IMS.104)
			MS-7360 v0A (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906AGLF, F71882FG, A7360IMS.108)
			MS-7365 (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS906AGLF, F71882FG, A7365IMS.107)
			MS-7320 v0A (Chipset: nVidia C55+MCP55, ClockGen: NVAPI, F71882FG, A7320IMS.103)
			MS-7317 v1.0 (Chipset: SiS 671+968, ClockGen: RTM876-660, MS7 WD, W83627DHG, A7317SMS.10A)
		b. fix auto-overclock failed issue
		c. support Intel 0xF60~0xF6F FSB200 CPU
		d. modify MS-7235 v2.1 DMI detection be "2.0"
		e. reset fan divisor 0x47h after resume from suspend
		f. new mainboard:
			MS-7364 v0A (Chipset: VIA P4M900+VT8237RPlus, ClockGen: ICS 9LPR700EGLF, MS7 WD, W83627EHG, A7364VMS.101)
			MS-7367 v0A (Chipset: ATi RS690C+SB600, ClockGen: RMT870T-691, no Watch-dog)
                        MS-7368 v0A (Chipset: ATi RS690C+SB600, ClockGen: RMT870T-691, no Watch-dog)
=========================================================================
	version 2.0.0.4 (2007/01/31)
		a. new mainboard:
			MS-7345 v0A (Chipset: Intel P35/G33+ICH9, ClockGen: ICS 9LPRS900AGLF)
		b. modify EIST registers based on A7238IMS.130
=========================================================================
	version 2.0.0.3 (2007/01/16)
		a. add vcore adjustment when DOT
		b. modify DOT fan icon and speed
		c. add support 4-core CPU
		d. add Flash64.sys for VGA 64bit OS
		e. new mainboard:
			MS-7235 v2.1 (Chipset: Intel P965+ICH8, ClockGen: ICS 9LPRS514EGLF, MS7 Watch-dog, A7235IMS.30B)
			MS-7346 (Chipset: nVidia C55+MCP51, ClockGen: NVAPI, no Watch-dog, A7346NMS.004)
		f. add sysfan1,sysfan2 bitmap for MS-7176v3.1 and MS-7346
		g. correct MS-7238 v1.1 voltage
		h. add overclock after resuming from suspend
		i. fix Intel MB with ICS 9LPRS514 cause suspend failed issue
		j. show -0%,-3% only for MS-7350 down-clock
=========================================================================
	version 2.0.0.2 (2007/01/03)
		a. fix ICS954519BGLF(MS-7246v2.1) writing registers when overclock
		b. add xml.manifest to run directly, without run as administrator
		c. modify smbus base reading in drivers for ICH7 and ICH8
		d. update VBios.dll,FlashSys.sys,VGADLL.dll(12/21)
		e. new mainboard:
			MS-7226 v2.0 (Chipset: nVidia C51XE+MCP55PXE, ClockGen: NVAPI, no Watch-dog, A7226NMS.30A)
		f. fix MS-7246 v2.2 CPUFANIN0 divisor error to cause fan speed wrong issue
		g. modify W83627EHG/DHG CPUFANIN0/CPUFANIN1 divisor reading to correct fan speed
		h. add 5 mode(av,game,..) overclock after resume from S3S4
		i. add MS-7226 v2.0 NB Fan and CPU Voltage(MCP55 GPIO)
		j. new mainboard:
			MS-7350 (Chipset: nVidia C55+MCP51, ClockGen: NVAPI, no Watch-dog, A7350NMS.102)
			MS-7337 (Chipset: ATi RS690C+SB600, ClockGen: RMT870T-691, no Watch-dog)
		k. add MS-7350 CPU Voltage(ISL6322)
		l. fix read MS-7280 cpu clock failed issue
=========================================================================
	version 2.0.0.1 (2006/12/05)
		a. change AP version be v2.0.0.1
		b. support Vista32/64
		c. support MS-7241 v1.1, MS-7267 v3.0, MS-7309 v1.2, MS-7173 v2.2
		d. new mainboard:
			MS-7255 v1.2(Chipset: VIA P4M890M+VT8237A, ClockGen: ICS903002DFLF, Watch-dog(MS7))
				- support FSB200 and Conroe FSB266 overclocking
			MS-7253 v1.1(Chipset: VIA K4M890M+VT8237A, ClockGen: RTM866-895, No Watch-dog)
			MS-7255 v2.0(Chipset: VIA P4M890M+VT8237A, ClockGen: RTM870T-580, No Watch-dog)
				- support FSB200 and Conroe FSB266 overclocking
		e. fix Intel fsb200/Conroe show fsb wrong when set bios fsb not be default fsb
		f. fix MS-7253 v1.1 underclock smoothly by M-f code
		g. new mainboard:
			MS-7176 v3.0 (Chipset: Intel LakePort+ ICH7, ClockGen: ICS 9LPRS914EGLF, Watch-dog(MS7), A7176IMS.706)
=========================================================================
	version 1.0.2.6 (2006/10/17)
		a. support Intel Conroe CPU serial
			- E6300 (FSB266,EIST,CPUID=0x6F6h)
			- E6700 (FSB266,EIST,CPUID=0x6F5h)					
		b. fix Intel Conroe CPU Ratio error issue under EIST mode
		c. support Intel EIST for MS-7238 v1.1 (A7238IMS.110)
		d. check EIST enable/disable register by cmos
=========================================================================
	version 1.0.2.5 (2006/10/05)
		update VBios.dll(10/3) to support all nVidia/ATI AGP/PCI-E VGA card
		add unload NTGlm7x/RushTop driver in registry whem close AP
		rebuild Glm7x.dll and NTGlm7x.sys(10/05)
=========================================================================
	version 1.0.0.0 (2006/05/16)
			new release
			smartly load saved or auto_overclock frequency & voltages
		new mainboard :
         		MS-7250v1(ati:8.24,nvidia:84.26(v046))

	version 1.0.0.1 (2006/05/19)
		new mainboard :
         		MS-7226(ati:8.24,nvidia:84.26(v046))

	version 1.0.0.2 (2006/05/22)
		show cpu clock instead of FSB
		change interval time (3"->2")
		if press silence button,do not play fan alarm sound 

	version 1.0.0.3 (2006/05/23)
		change CPU temperature mapping address to support A7250NMS.112(MS-7250)

	version 1.0.0.4 (2006/05/29)
		fix nvidia VGA card error for MS-7226

	version 1.0.0.5 (2006/06/05)
		show NB fan speed for MS-7226
		adjustable vcore for MS-7226
		change some UI image file
		support V060

	version 1.0.0.6 (2006/06/05)
		support V044(ATI)
		need to install DotNet frame work 2.0

	version 1.0.0.7 (2006/06/05)
		disable VCore adjustable for MS-7226
		add up/down rate for DOT

	version 1.0.0.8 (2006/06/09)
		new mainboard :
         		MS-7246v2(ati:8.26(v044),nvidia:84.26(v046,v060))

	version 1.0.0.9 (2006/06/16)
		new mainboard :
         		MS-7238(ati:8.26(v044),nvidia:84.26(v046,v060))
		add MS-7226 vcore adjustable
		change CPU temp source(Fintek -> winbond) for MS-7226
		add smooth and sharp mode for CPU overclocking
		change some UI image
		change VGA overclocking range

	version 1.0.1.0 (2006/06/21)
		for VGA dll changed

	version 1.0.1.1 (2006/06/22)
		new mainboard :
         		MS-7280(bios:A7280AMS.10C)ati:8.26(v044),nvidia:84.26(v046,v060))

	version 1.0.1.2 (2006/06/23)
		fix VGA restore defalut value error.

	version 1.0.1.3 (2006/06/26)
		change system temperature mapping register for MS-7226
		change vcore adjust method for MS-7226
		display FSB value in the history diagram(instead of clock)
		automatic hide program dialog when it first start

	version 1.0.1.4 (2006/06/27)
		change help files
		fix conroe CPU ratio error
		fix NB fan control for MS-7238
		fix NB fan button status error for MS-7238
		remove watchdog timer for auto overclock for MS-7238
		remove NB temperature for MS-7238
		
	version 1.0.1.5 (2006/06/28)
		change CPU temperature mapping register for MS-7250
		fix CPU fan control error for MS-7280
		adjust NB fan speed range for MS-7238
		add auto overclock restart function for MS-7238

	version 1.0.1.6 (2006/07/03)
		show NB fan speed for MS-7226
		fix auto overclock function error(CPU usage rise high)
		fix CPU fan adjustable error for MS-7238

	version 1.0.1.7 (2006/07/12)
		add share memory for VGA OSD function
		add NB/SYS fan warning
		auto select profile when user setting profile
		fix vga dialog error for v069,v045

	version 1.0.1.8 (2006/07/17)
		change system temperature register mapping for MS-7238

	version 1.0.1.9 (2006/07/25)
		detect VGA vendor for directory of installation 
		change VGA GPU temperature alert value (80->95) for v069

	version 1.0.2.1 (2006/08/04)
		fix MB fan speed register mapping for MS-7246v2

	version 1.0.2.2 (2006/08/28)
		add installation need restart 
		support OSD 

	version 1.0.2.3 (2006/08/30)
		support MS-7246 version '2.' and MS-7250 version '1.'
		support MS-7238 CPU fan control,remove NB fan control

	version 1.0.2.4 (2006/09/28)
		support MS-7325 v0A (show DDR voltage v1.80~2.10v, discard its part2 v2.15~2.45v)
		update VBios.dll,FlashSys.sys to support Vista32
		update VGADLL.dll(09/28) for Mem DateRate and check MSI VGA Driver installed or not
		