; POTS for EAGLE
; Number of CMV writes made in this file MUST not exceed 16
; Refer to Application Note "Eagle/EagleII, Pathfinder BOM change"
; for improved TR-048 performance with this version of firmware
;
CW cntl 0 1
CW optn 0 80020066
CW optn 1 00000994
CW optn 4 006C0000
CW mask 8 3fffffc0
CW diag 0 23870020
CW flag 0 00000820
CW info 28 00000001
CW cntl 0 2

