WAN - Configuration

1. The WAN configuration page allow user to set the configuration for the WAN/ADSL ports.

2. Encapsulation: Choose accordingly to your configuration.

3. ATM

- VPI:: Virtual Path Identifier. Enter the given value by your Internet Service Provider.
- VCI: Virtual Circuit Identifier. Enter the given value by your Internet Service Provider.
- Service Category: UBR and CBR are supported from the ATM.
- BandWidth: Bandwidth setting takes effect only when the CBR is selected. The maximum available bandwidth is from the upstream data rate of ADSL status page.

4. DHCP Client

- Enable DHCP Client: Select to enable DHCP Client.
- Host Name: Enter the Host here.

5. PPP

Note:If user chose RFC1483 or RFC 1577 configuration please ignore PPP entry.

- Service Name : The service name of PPP is required by some ISPs. If the ISP does not provide the Service Name, please leave it blank.
- Username: If PPP type of encapsulation is setup, you may need to enter the username given by your Internet Service Provider.
- Password: If PPP type of encapsulation is setup, you may need to enter the password given by your Internet Service Provider.
- Disconnect Timeout: The Disconnect Timeout allows users to set the specific period of time to disconnect from the ISP. The default is 0, which means never disconnect fro the ISP.
- Automatic Reconnect: When it is checked, it will automatically reconncet ppp session.
- Authentication: When Auto option is chosen, the PAP mode will run first then Chap.

6. DHCP Client

- Enable DHCP Client: Select to enable DHCP Client.
- Host Name: Enter the Host here.