LAN - Configuration

1. This page allow user to configure the LAN Configuration.

DCHP Server

- System Allocated: The DHCP addres pool is based on LAN port IP address plus 12 IP addresses. For example, the LAN IP address is 10.0.0.2; the DHCP address pool is at the range of 10.0.0.3 to 10.0.0.14.
- User Defined: The DHCP address pool is at the range of User Defined Start Address and User Defined End Address. The Maximum pool size can be 253 IP addresses: 255 total IP addresses - 1 broadcast address - 1 LAN port IP address.
- Lease Time: The Lease time is the amount of time of a network user will be allowed to connect with DHCP server. If all fields are 0, the alocated IP addresses will be effective forever.