Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| Chipset
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| Disk
| ATAPI
| Storage (ASPI)
| Logical Drives
| USB Devices
| Plug and Play
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Network
| Power
| Monitor
| Video
| Hardware Monitoring
| Diagnostics
| Software
Background
| Background
| Version | ASTRA32 - Advanced System Information Tool 4.22
| Home Page | www.astra32.com
| Network Name | DESKTOP-O18FSDF
| User Name | KKV1
| Report Date | 11-Dec-2025
| Report Time | 12:40:04
| OS Version | MS Windows 11 Professional x64 Edition (10.0.22621)
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
| Command Line | /LL lang\a32en.lng /RTJXHCE examples\astra32
| Disabled Tests | UDMA
System Summary
| Processor
| Processor | AMD Ryzen 5 5600 3500 MHz
| CPU Clock | 3500.0 MHz (35.0 x 100.0 MHz)
| Level 1 Cache | 6 x 32 kB + 6 x 32 kB (data+instr.)
| Level 2 Cache | 6 x 512 kB
| Level 3 Cache | 1 x 32 MB
| Motherboard
| System Name | Micro-Star International Co., Ltd. MS-7A38
| Motherboard Vendor | Micro-Star International Co., Ltd.
| Board Model | Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
| BIOS Version | American Megatrends International, LLC. B.L0
| BIOS Version | AMI BIOS 08.00.10
| Chipset Name | AMD B450 (Promontory)
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| DMI/SMBIOS Version | 2.8
| Memory
| Memory Size | 15.93 GB
| System Memory | 16310 MB
| Memory Module | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Memory Module | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Storage
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Disk Model | Samsung SSD 970 EVO Plus 1TB
| Disk Size | 953869 MB (931.51 GB)
| CD/DVD Model | ATAPI DVD W DH16W1S
| CD/DVD Speed | 48x (Write: 48x)
| Monitor
| Monitor Vendor | BenQ
| Monitor Model | BenQ GW2470 (23.8")
| Video Card
| Video Chip Vendor | NVIDIA Corporation
| Video Chip | GeForce RTX 3060 Ti LHR [GA104]
| Bus Type | PCI Express 3.0 x16
| Video Memory Size | 8 GB GDDR6 (Hynix)
| Sound
| Sound Chip Vendor | NVIDIA Corporation
| Sound Chip | GA104 High Definition Audio Controller
| Audio Codec Name | NVidia GPU GA104 HDMI/DP
| Sound 2
| Sound Chip Vendor | Advanced Micro Devices (AMD)
| Sound Chip | Starship/Matisse HD Audio Controller
| Audio Codec Name | Realtek ALC892
| Sound 3
| Sound Chip Vendor | ASUSTek Computer
| Sound Chip | ASUS XONAR SC150 AUDIO DEVICE
| Printer
| Printer Vendor | Canon
| Printer Model | LaserBase MF3110 Scanner/Printer
| Operating System
| Operating System | MS Windows 11 Professional x64 Edition (Version 22H2, 10.0.22621.4317)
| Windows Folder | J:\Windows
| Network
| Network Name | DESKTOP-O18FSDF
| Network Chip Vendor | Realtek Semiconductor
| Network Chip | RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Interface Description | Realtek PCIe GbE Family Controller
| MAC Address | 2C-F0-5D-D2-A7-22
| Ports
| LPT Ports | LPT1 (0378h)
| COM Ports | COM1 (03F8h)
Motherboard
| System
| System Vendor | Micro-Star International Co., Ltd.
| Product Name | MS-7A38
| Version | 8.0
| Serial Number | To be filled by O.E.M.
| UUID | 12983CA982A41496AAC82CF05DD2A722
| Wake-up Type | Power Switch
| SKU Number | To be filled by O.E.M.
| Family | To be filled by O.E.M.
| Motherboard
| Motherboard Vendor | Micro-Star International Co., Ltd.
| Vendor URL | www.msi.com
| Board Model | Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
| Motherboard ID | BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
| Version | 8.0
| Serial Number | 07A3880_KB1E018736
| Asset Tag | To be filled by O.E.M.
| Chipset Name | AMD B450 (Promontory)
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| BIOS Version | American Megatrends International, LLC. B.L0
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 10/26/2023
| Onboard Device 1
| Description | Broadcom 5762
| Device Type | Ethernet
| Status | Disabled
| Configuration Options
| To be filled by O.E.M.
| System Enclosure
| Manufacturer | Micro-Star International Co., Ltd.
| Type | Desktop
| Version | 8.0
| Serial Number | To be filled by O.E.M.
| Asset Tag | To be filled by O.E.M.
| Boot-up State | Safe
| Power Supply State | Safe
| Thermal State | Safe
| Security Status | None
| OEM-defined | 00000000h
| Height | 0.0 sm
| Power Cords | 1
| Contained Element | 0
CPU
| CPU
| Processor | AMD Ryzen 5 5600 3500 MHz
| Coprocessor | Internal
| CPU Clock | 3500.0 MHz
| Level 1 Cache | 6 x 32 kB + 6 x 32 kB (data+instr.)
| Level 2 Cache | 6 x 512 kB
| Level 3 Cache | 1 x 32 MB
| Code Name | Vermeer (Zen 3)
| Manufacturing Process | 7 nm
| FSB Clock | 100.0 MHz
| Multiplier | 35.0
| Expected Clock | 3500 MHz
| Overclocking Support | Unlocked Multiplier
| AMD Core Performance Boost | Supported (Enabled)
| Max Turbo Clock | 4450.0 MHz
| Processor Topology | Nodes: 1, CPU Complexes (CCX): 1, Cores: 6, Threads: 12
| Socket Type | Socket AM4
| Instruction Set | IA-32, AMD64, MMX, AMDMMX, SSE, SSE2, SSE3, SSSE3
| Instruction Set | SSE4.1, SSE4.2, SSE4A, AVX, AVX2, AES, FMA, SHA
| Maximum Temperature (Tjmax) | 95 °C (203 °F)
| Core Voltage | 1.113 V
| Infinity Fabric Clock (FCLK) | 1800.0 MHz
| Vendor | AuthenticAMD
| Processor Name | AMD Ryzen 5 5600 6-Core Processor
| Processor Type | Original OEM Processor
| CPUID | Family: 15, Model: 1, Stepping: 2
| Ext. Family/Model | Family: 10, Model: 2
| CPU Signature | 00A20F12h
| Number of Cores | 6
| Logical Cores Count | 12
| Core Stepping | VMR-B2
| OPN Code | 100-000000927, 100-100000927BOX
| Microcode Revision | A20120Eh
| SMU Firmware Version | 56.76.00
| Power Table Version | 380905h
| Max TDP | 65 Wattes
| Power Limit | 76 Wattes
| Thermal Design Current (TDC) | 60 Amps
| Electrical Design Current (EDC) | 90 Amps
| Transistor Count | 6240 million
| Die Size | 81 mm2 + I/O 122 mm2
| Launch Date | April, 2022
| Recommended Price (USD) | $199
| Hardware Monitoring
| Core Voltage | 1.113 V
| Core Voltage (SVI2 TFN) | 1.119 V
| SoC Voltage (SVI2 TFN) | 1.075 V
| Package Temperature | 48 °C (118 °F)
| CCD1 Temperature | 48 °C (118 °F)
| SoC Temperature | 40 °C (104 °F)
| L3 Cache Temperature | 38 °C (100 °F)
| Package Power | 27.1 Wattes
| Cores Power | 3.0 Wattes
| SoC Power | 12.4 Wattes
| VDDIO Mem Power | 9.2 Wattes
| VDD18 Power | 0.9 Wattes
| FSB Clock | 100.0 MHz
| Core 1
| Temperature Core | 38 °C (100 °F)
| Core Power | 0.5 Wattes
| Core Clock | 3560.0 MHz
| Multiplier | 35.6
| Core 2
| Temperature Core | 39 °C (102 °F)
| Core Power | 0.5 Wattes
| Core Clock | 4450.1 MHz
| Multiplier | 44.5
| Core 3
| Temperature Core | 39 °C (102 °F)
| Core Power | 0.7 Wattes
| Core Clock | 4450.1 MHz
| Multiplier | 44.5
| Core 4
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.0 Wattes
| Core Clock | 3560.0 MHz
| Multiplier | 35.6
| Core 5
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.0 Wattes
| Core Clock | 3560.0 MHz
| Multiplier | 35.6
| Core 6
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.1 Wattes
| Core Clock | 3560.0 MHz
| Multiplier | 35.6
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Supported
| SSE4.1 Instruction Set | Supported
| SSE4.2 Instruction Set | Supported
| Advanced Vector Extensions (AVX) | Supported
| Advanced Vector Extensions 2 (AVX2) | Supported
| AVX-512 Foundation Instructions | Not Supported
| AVX-512 Prefetch Instructions | Not Supported
| AVX-512 Exponential and Reciprocal | Not Supported
| AVX-512 Conflict Detection | Not Supported
| AVX-512 Byte and Word Instructions | Not Supported
| AVX-512 Doubleword and Quadword | Not Supported
| AVX-512 Vector Length Extensions | Not Supported
| AVX-512 Integer Fused Multiply-Add | Not Supported
| AVX-512 Vector Bit Manipulation | Not Supported
| AVX-512 QVNNI Instructions | Not Supported
| AVX-512 QFMA Instructions | Not Supported
| AVX-512 VBMI2 Instructions | Not Supported
| AVX-512 VNNI Instructions | Not Supported
| AVX-512 BITALG Instructions | Not Supported
| Galois Field NI/Affine Transformation | Not Supported
| VEX-encoded AES-NI (VAES) | Supported
| VEX-encoded PCLMUL (VPCL) | Supported
| PCOMMIT Instruction | Not Supported
| CLWB Instruction | Supported
| PREFETCHWT1 Instruction | Not Supported
| Software Guard Extensions (SGX) | Not Supported
| SGX Launch Configuration | Not Supported
| FMA Instructions Set | Supported
| AES Instructions Set | Supported
| Intel Extended Memory 64 Tech. | Not Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Supported
| AMD 3DNow! Instructions | Not Supported
| AMD 3DNow! Extensions | Not Supported
| AMD 3DNow! Prefetch | Supported
| AMD SSE4A Extensions | Supported
| AMD eXtended OPeration (XOP) | Not Supported
| AMD Misaligned SSE | Supported
| AMD64 Architecture | Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Supported
| OS Supports XSAVE Instructions | Supported
| PCLMULQDQ Instruction Supported | Supported
| MOVBE Insruction Supported | Supported
| F16C Insruction Supported | Supported
| RDTSCP Insruction Supported | Supported
| RDRAND Insruction Supported | Supported
| (RD/WR)(FS/GS) BASE Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Enhanced REP MOVSB/STOSB | Supported
| INVPCID Instruction | Supported
| XSAVEOPT Instruction | Supported
| RDSEED Instruction | Supported
| ADCX/ADOX Instructions | Supported
| CLAC/STAC Instructions | Supported
| SCLFLUSHOPT Instruction | Supported
| RDPID Instruction | Supported
| VPOPCNT[D/Q] Instructions | Not Supported
| Fast Short REP MOV Instruction | Supported
| PCONFIG Instruction | Not Supported
| WBNOINVD Instruction | Supported
| WaitPKG Instructions | Not Supported
| CLDEMOTE Instruction | Not Supported
| MOVDIRI Instruction | Not Supported
| MOVDIRI64B Instruction | Not Supported
| RDPRU Instruction | Supported
| MCOMMIT Instruction | Not Supported
| AMD Fast Save and Restore | Supported
| AMD SKINIT, STGI, DEV Supported | Not Supported
| AMD Light Weight Profiling (LWP) | Not Supported
| AMD FMA4 Insruction Supported | Not Supported
| AMD TBM Insruction Supported | Not Supported
| AMD MONITORX/MWAITX Instructions | Supported
| AMD CLZERO Instruction | Supported
| Processor Features
| Hypervisor Present | Supported
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Not Supported
| 64-bit Debug Store | Not Supported
| Self-Snoop | Not Supported
| Hyper-Threading Technology | Supported
| Pending Break Enable | Not Supported
| CPL-Qualified Debug Store | Not Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Not Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Not Supported
| x2APIC Architecture | Not Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Supported
| Instruction Based Sampling | Not Supported
| 1-GB Large Page | Supported
| Process Context Identifiers | Not Supported
| Time Stamp Counter Deadline | Not Supported
| Time Stamp Counter Adjust | Not Supported
| Intel Virtualization Technology | Not Supported
| Intel Trusted Execution Technology | Not Supported
| Supervisor Mode Execution Protection | Supported
| Hardware Lock Elision | Not Supported
| Restricted Transactional Memory | Not Supported
| Quality of Service Monitoring | Supported
| Quality of Service Enforcement | Supported
| Deprecated FPU CS and FPU DS | Not Supported
| Memory Protection Extensions (MPX) | Not Supported
| Processor Trace (PT) | Not Supported
| Secure Hash Algorithm Ext. (SHA) | Supported
| Debug Interface MSR | Not Supported
| User-Mode Instruction Prevention | Supported
| Protection Keys for User-Mode Pages | Not Supported
| 5 Level Page Table | Not Supported
| Total Memory Encryption (TME) | Not Supported
| Speculation Control (IBRS and IBPB) | Not Supported
| Single Thread Indirect Branch Predictors | Not Supported
| L1 Data Cache (L1D) Flush | Not Supported
| ARCH_CAPABILITIES MSR | Not Supported
| Speculative Store Bypass Disable (SSBD) | Not Supported
| AMD Core Performance Boost | Supported, Enabled
| Intel Turbo Boost Max Technology 3.0 | Not Supported
| AMD No-execute Page Protection | Supported
| Hybrid Processor | Not Supported
| AMD Secure Virtual Machine | Not Supported
| AMD Model-Specific Registers | Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Supported
| AMD CR8 in Legacy Mode | Supported
| AMD Ext. APIC Register Space | Not Supported
| AMD Watchdog Timer | Supported
| AMD Translation Cache Extension | Not Supported
| AMD NodeID MSR | Not Supported
| AMD Topology Extensions | Supported
| AMD Core Performance Counter Ext. | Supported
| AMD NB Performance Counter Ext. | Not Supported
| AMD Streaming Performance Monitor | Not Supported
| AMD Data Breakpoint Extension | Not Supported
| AMD Performance TSC | Not Supported
| AMD L2I Performance Counter Ext. | Not Supported
| AMD IRPERF Performance Counter | Not Supported
| AMD Always Save/Restore FP Error Pointers | Supported
| AMD Indirect Branch Prediction Barrier | Supported
| AMD Indirect Branch Restricted Speculation | Supported
| AMD IBRS Always On Mode | Not Supported
| AMD IBRS Preferred | Not Supported
| AMD Single Thread Indirect Branch Predictor | Supported
| AMD STIBP Always On Mode | Not Supported
| AMD Speculative Store Bypass Disable (SSBD) | Supported
| AMD SSBD Not Needed | Not Supported
| AMD VIRT_SPEC_CTRL MSR | Not Supported
| Power Management
| ACPI Supported | Not Supported
| Thermal Monitor Supported | Not Supported
| Thermal Monitor 2 | Not Supported
| Enhanced SpeedStep Technology | Not Supported
| Digital Thermal Sensor | Not Supported
| Always Running APIC Timer | Not Supported
| Invariant TSC | Supported
| Power Limit Notification | Not Supported
| Extended Clock Modulation Duty | Not Supported
| Package Thermal Management | Not Supported
| Hardware Coordination Feedback | Supported
| ACNT2 Capability | Not Supported
| Performance-Energy Bias | Not Supported
| Hardware-Managed P-State Base Support | Not Supported
| Hardware Duty Cycle Programming (HDC) | Not Supported
| AMD Temperature Sensor | Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Supported
| AMD Thermal Monitoring | Not Supported
| AMD Software Thermal Control | Not Supported
| AMD 100MHz Multiplier Steps | Not Supported
| AMD Hardware P-State Control | Supported
| AMD Effective Frequency Interface | Supported
| AMD Processor Feedback Interface | Not Supported
| AMD Processor Accumulator | Not Supported
| AMD Connected Standby | Not Supported
| AMD Running Average Power Limit | Supported
| AMD MCA Overflow Recovery | Supported
| AMD Software Uncorr. Error Containment/Recovery | Supported
| AMD Hardware Assert (HWA) | Not Supported
| AMD Scalable MCA | Supported
CPU Cache
| Level 1 Data Cache
| Size | 6 x 32 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 64
| Associativity | full
| Level 1 Instruction Cache
| Size | 6 x 32 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 64
| Associativity | full
| Level 2 Cache
| Size | 6 x 512 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| Data TLB 4K Pages |
| Number of Entries | 2048
| Associativity | 8-way
| Instr. TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Data TLB 2/4M Pages |
| Number of Entries | 2048
| Associativity | 4-way
| Instr. TLB 2/4M Pages |
| Number of Entries | 512
| Associativity | 2-way
| Level 3 Cache
| Size | 1 x 32 MB
| Associativity | 16-way
| Lines per Tag | 1
| Line Size | 64 byte
CPU (SMBIOS)
| Processor
| Processor Vendor | Advanced Micro Devices, Inc.
| Processor Version | AMD Ryzen 5 5600 6-Core Processor
| Current Speed | 3500 MHz
| External Clock | 100 MHz
| Voltage | 1.1 V
| Processor Upgrade | Socket AM4
| Processor Status | CPU Enabled
| Socket Designation | AM4
| Processor Type | Central Processor
| Processor Family | AMD Zen
| Processor ID1 | 00A20F12h
| Processor ID2 | 178BFBFFh
| Max Speed | 4450 MHz
| Socket Status | CPU Socket Populated
| Serial Number | Unknown
| Asset Tag | Unknown
| Part Number | Unknown
| CPU Core Count | 6 (Enabled: 6)
| CPU Thread Count | 12
| Structure Length | 30h
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 384 kB
| Operational Mode | Write-Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L1 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 384 kB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 3 MB
| Operational Mode | Write-Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L2 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 3 MB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 32 MB
| Operational Mode | Write-Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L3 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 32 MB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 16-way Set-Associative
| Structure Length | 13h
Chipset
| Chipset
| Chipset Name | AMD B450
| Code Name | Promontory
| Chipset Type | Single Chip: Southbridge-only
| Manufacturing Process | 55 nm
| Max TDP | 5.8 Wattes
| Launch Date | March, 2018
| Northbridge
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Code Name | Vermeer (Zen 3)
| Location | CPU Integrated
| Infinity Fabric Clock (FCLK) | 1800.0 MHz
| Manufacturing Process | 7 nm
| Hardware ID | VEN_1022&DEV_1480
| Revision | 00h
| Stepping | VMR-B2
| Memory Controller
| Current Memory Type | DDR4-3600
| Supported Memory Types | DDR4-2667, DDR4-2933, DDR4-3200
| Maximum Memory Amount | 128 GB
| Current Controller Mode | Dual-channel (128-bit)
| Supported Controller Mode | Dual-channel (128-bit)
| Channel 0 DIMM A | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Channel 1 DIMM A | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Current Memory Clock | 1800.0 MHz (Effective: 3600.0 MHz)
| FSB:DRAM Ratio | 1:18
| Memory Bandwidth | 56.3 GB/s
| Memory Controller Clock (UCLK) | 1800.0 MHz
| ECC | Supported, Disabled
| ECC Scrubbing | Not Supported
| Mirroring Mode (RAID) | Not Supported
| ECC Chipkill | Not Supported
| Timings
| CAS Latency (CL) | 16.0
| RAS to CAS Delay (tRCD) | 20
| RAS Precharge Time (tRP) | 20
| RAS Active Time (tRAS) | 39
| Row Cycle Time (tRC) | 83
| Row Refresh Cycle Time (tRFC) | 631
| Command Rate (CR) | 1T
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Connected Device | Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x8 8.0 GT/s (Current: x4 8.0 GT/s)
| Bus Bandwidth | 7.9 GB/sec (Current: 3.9 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Connected Device 1 | AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Connected Device 2 | AMD 400 Series Chipset SATA Controller
| Connected Device 3 | AMD 400 Series Chipset PCIe Bridge
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x16 8.0 GT/s (Current: x16 8.0 GT/s)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Connected Device 1 | NVIDIA GeForce RTX 3060 Ti LHR [GA104]
| Connected Device 2 | NVIDIA GA104 High Definition Audio Controller
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Bus Type | PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Connected Device | AMD Starship/Matisse PCIe Dummy Function
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Bus Type | PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Connected Device 1 | AMD Starship/Matisse Reserved SPP
| Connected Device 2 | AMD Starship/Matisse Cryptographic Coprocessor PSPCPP
| Connected Device 3 | AMD Matisse USB 3.0 Host Controller
| Connected Device 4 | AMD Starship/Matisse HD Audio Controller
| Connected Device 5 | Motherboard registers
| Southbridge
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| Bus Type | PCI Express
| Manufacturing Process | 55 nm
| Max TDP | 5.8 Wattes
| Hardware ID | VEN_1022&DEV_790E
| Revision | 51h
| Top Marking | 218-0891011
| Package Type | LFBGA-583
| Connected Device 1 | AT Interrupt Controller
| Connected Device 2 | Motherboard registers
| Connected Device 3 | Standard LPT printer port
| Connected Device 4 | AT DMA Controller
| Connected Device 5 | 16550A-compatible COM port
| Connected Device 6 | AT standard speaker sound
| Connected Device 7 | AT Timer
| Connected Device 8 | AT Real-Time Clock
| Integrated Sound
| Audio Controller | AMD Starship/Matisse HD Audio Controller
| Audio Codec Name | Realtek ALC892
| Controller Type | High Definition Audio
| Hardware ID | VEN_1022&DEV_1487
| Revision | 00h
| Integrated Storage
| Storage Controller | AMD 400 Series Chipset SATA Controller
| Controller Type | Serial ATA
| Hardware ID | VEN_1022&DEV_43C8
| Revision | 01h
BIOS
| BIOS
| Motherboard Vendor | Micro-Star International Co., Ltd.
| Vendor URL | www.msi.com
| BIOS Version | AMI BIOS 08.00.10
| BIOS Type | AMIBIOS 8 (BigBIOS)
| BIOS Type | UEFI (CSM Mode)
| BIOS Date | 12/24/18
| BIOS Copyright | 12/24/18(C)2010 American Megatrends, Inc. All Rights Reserved
| Motherboard ID | BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
| BIOS ID | 63-0100-000001-00101111-122418-Chipset-H
| AMI BIOS Tag | 0AAAA000
| BIOS Size | 512 kB
| Processor | 686
| Chipset ID | Chipset
| BIOS Revision | 0100
| Keyboard Controller Revision | H
| PnP Version | 1.0
| MCFG Address | F0000000h
| DMI/SMBIOS Version | 2.8
| DMI/SMBIOS Structures | 62
| SMBIOS
| BIOS Vendor | American Megatrends International, LLC.
| BIOS Version | B.L0
| BIOS Date | 10/26/2023
| BIOS ROM Size | 16 MB
| System BIOS Version | 5.17
| Starting Segment | F000h
| Structure Length | 1Ah
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Not Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Not Supported
| LS-120 Boot | Not Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Not Supported
| PnP is Supported | Not Supported
| APM is Supported | Not Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| UEFI Specification is Supported | Supported
| Virtual Machine | Not Supported
| Int 13h - 5.25"/360kB Floppy | Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Supported
| Int 13h - Floppy for NEC 9800 | Supported
| Int 13h - Floppy for Toshiba | Supported
| NEC PC-98 | Not Supported
| ROM Extension
| Adapter Vendor | Intel Corporation
| Adapter Name | Realtek PXE B25 D00
| BIOS Version | PXE-EC6: UNDI driver image is invalid.
| BIOS Copyright | Copyright (C) 1997-2000 Intel Corporation
| Device Class | Network
| ROM Address | CF80h
| BIOS ROM Size | 4 kB
| ROM Extension
| Device Name | NVIDIA GeForce RTX 3060 Ti LHR [GA104]
| BIOS Version | Version 94.04.46.00.D2
| BIOS Copyright | Copyright (C) 1996-2021 NVIDIA Corp.
| Device Class | Display
| ROM Address | C000h
| BIOS ROM Size | 61 kB
| OEM SMBIOS Strings
| To be filled by O.E.M.
| Other SMBIOS Structures
| System Boot Information (32)
| Unknown (44)
| TPM Device (43)
| 32-bit Memory Error Information (18)
| Memory Array Mapped Address (19)
| Memory Array Mapped Address (19)
| 32-bit Memory Error Information (18)
| 32-bit Memory Error Information (18)
| Memory Device Mapped Address (20)
| 32-bit Memory Error Information (18)
| 32-bit Memory Error Information (18)
| Memory Device Mapped Address (20)
| Unknown (143)
PCI/AGP Devices
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1480h) | Starship/Matisse Root Complex
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1480
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1480&SUBSYS_7A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1480&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 01h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 1, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 01h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device | Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FC800000h - FC8FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 1
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Port
| Device Class | System
| Device Location | PCI bus 0, device 1, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1483&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 01h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device 1 | AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Device 2 | AMD 400 Series Chipset SATA Controller
| Device 3 | AMD 400 Series Chipset PCIe Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC500000h - FC7FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x8 (Current: x4)
| Bus Bandwidth | 7.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Port
| Device Class | System
| Device Location | PCI bus 0, device 1, function 3
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1483&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 02h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 2, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 03h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 3, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 03h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device 1 | NVIDIA GeForce RTX 3060 Ti LHR [GA104]
| Device 2 | NVIDIA GA104 High Definition Audio Controller
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | FB000000h - FC0FFFFFh
| Memory Address | D0000000h - E1FFFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Port
| Device Class | System
| Device Location | PCI bus 0, device 3, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1483&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 04h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 4, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 05h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 5, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 07h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 7, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 07h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1484h) | Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device | AMD Starship/Matisse PCIe Dummy Function
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Port
| Device Class | System
| Device Location | PCI bus 0, device 7, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1484&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 08h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 8, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1482&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 08h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1484h) | Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device 1 | AMD Starship/Matisse Reserved SPP
| Device 2 | AMD Starship/Matisse Cryptographic Coprocessor PSPCPP
| Device 3 | AMD Matisse USB 3.0 Host Controller
| Device 4 | AMD Starship/Matisse HD Audio Controller
| Device 5 | Motherboard registers
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FC200000h - FC4FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Port
| Device Class | System
| Device Location | PCI bus 0, device 8, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1484&REV_00
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (790Bh) | Hudson SMBus Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Hardware ID | VEN_1022&DEV_790B
| Revision | 61h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| SMBus Port | 0B00h
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc
| Device Description | AMD SMBus
| Device Class | System
| Device Location | PCI bus 0, device 20, function 0
| Driver Provider | Advanced Micro Devices, Inc
| Driver Version | 5.12.0.38
| Driver Date | 9-15-2022
| Inf File | oem3.inf
| Hardware ID | PCI\VEN_1022&DEV_790B&SUBSYS_7A381462&REV_61
| Compatible ID | PCI\VEN_1022&DEV_790B&REV_61
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 14h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (790Eh) | B450 Fusion Controller Hub (FCH)
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Hardware ID | VEN_1022&DEV_790E
| Revision | 51h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Connected Devices
| Device 1 | AT Interrupt Controller
| Device 2 | Motherboard registers
| Device 3 | Standard LPT printer port
| Device 4 | AT DMA Controller
| Device 5 | 16550A-compatible COM port
| Device 6 | AT standard speaker sound
| Device 7 | AT Timer
| Device 8 | AT Real-Time Clock
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard ISA bridge
| Device Class | System
| Device Location | PCI bus 0, device 20, function 3
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | msisadrv
| Hardware ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| Compatible ID | PCI\VEN_1022&DEV_790E&REV_51
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1440h) | Matisse/Vermeer Data Fabric: Device 18h; Function 0
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1440
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1440&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1441h) | Matisse/Vermeer Data Fabric: Device 18h; Function 1
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1441
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1441&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1442h) | Matisse/Vermeer Data Fabric: Device 18h; Function 2
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1442
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 2
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1442&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1443h) | Matisse/Vermeer Data Fabric: Device 18h; Function 3
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1443
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 3
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1443&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1444h) | Matisse/Vermeer Data Fabric: Device 18h; Function 4
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1444
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 4
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1444&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 05h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1445h) | Matisse/Vermeer Data Fabric: Device 18h; Function 5
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1445
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 5
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1445&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 06h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1446h) | Matisse/Vermeer Data Fabric: Device 18h; Function 6
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1446
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 6
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1446&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 00h, Device: 18h, Function: 07h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1447h) | Matisse/Vermeer Data Fabric: Device 18h; Function 7
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1447
| Revision | 00h
| Interface | 00h
| Parent Device | PCI Bus Host Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 7
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1447&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (144Dh) | Samsung Electronics Co Ltd
| Device (A808h) | NVMe SSD Controller SM981/PM981/PM983
| Subsys Vendor (144Dh) | Samsung Electronics Co Ltd
| Subsystem ID (A801h) | SSD 970 EVO/PRO
| Class (01h) | Storage
| SubClass (08h) | Non-Volatile memory controller
| Hardware ID | VEN_144D&DEV_A808
| Revision | 00h
| Interface | 02h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Connected Devices
| Device | Samsung SSD 970 EVO Plus 1TB
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC800000h - FC803FFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Standard NVM Express Controller
| Device Description | Standard NVM Express Controller
| Device Class | SCSIAdapter
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | stornvme.inf
| Service Name | stornvme
| Hardware ID | PCI\VEN_144D&DEV_A808&SUBSYS_A801144D&REV_00
| Compatible ID | PCI\VEN_144D&DEV_A808&REV_00
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 03h, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43D5h) | 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Subsys Vendor (1B21h) | ASMedia Technology Inc.
| Subsystem ID (1142h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1022&DEV_43D5
| Revision | 01h
| Interface | 30h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Connected Devices
| Device | Canon LaserBase MF3110 Scanner/Printer
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC7A0000h - FC7A7FFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Generic USB xHCI Host Controller
| Device Description | USB xHCI Compliant Host Controller
| Friendly Name | AMD USB 3.10 eXtensible Host Controller - 1.10 (Microsoft)
| Device Class | USB
| Device Location | PCI bus 3, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 5-21-2024
| Inf File | usbxhci.inf
| Service Name | USBXHCI
| Hardware ID | PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43D5&REV_01
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 03h, Device: 00h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C8h) | 400 Series Chipset SATA Controller
| Subsys Vendor (1B21h) | ASMedia Technology Inc.
| Subsystem ID (1062h) | Unknown
| Class (01h) | Storage
| SubClass (06h) | Serial ATA
| Hardware ID | VEN_1022&DEV_43C8
| Revision | 01h
| Interface | 01h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Connected Devices
| Device 1 | WDC WD1001FALS-00J7B0
| Device 2 | ATAPI DVD W DH16W1S
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC780000h - FC79FFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Standard SATA AHCI Controller
| Device Description | Standard SATA AHCI Controller
| Device Class | HDC
| Device Location | PCI bus 3, device 0, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.2506
| Driver Date | 6-21-2006
| Inf File | mshdc.inf
| Service Name | storahci
| Hardware ID | PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C8&REV_01
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 03h, Device: 00h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C6h) | 400 Series Chipset PCIe Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C6
| Revision | 01h
| Interface | 00h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Connected Devices
| Device 1 | AMD 400 Series Chipset PCIe Port
| Device 2 | AMD 400 Series Chipset PCIe Port
| Device 3 | AMD 400 Series Chipset PCIe Port
| Device 4 | AMD 400 Series Chipset PCIe Port
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC500000h - FC6FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTC#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Upstream Port of PCI-E Switch
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Upstream Switch Port
| Device Class | System
| Device Location | PCI bus 3, device 0, function 2
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C6&REV_01
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 20h, Device: 04h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Parent Device | AMD 400 Series Chipset PCIe Bridge
| Connected Devices
| Device | Realtek Semiconductor RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC600000h - FC6FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 4
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Downstream Switch Port
| Device Class | System
| Device Location | PCI bus 32, device 4, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C7&REV_01
| Parent ID | PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
| Bus: 20h, Device: 05h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Parent Device | AMD 400 Series Chipset PCIe Bridge
| Connected Devices
| Device | ASMedia Technology Inc. ASM1042A USB 3.0 Host Controller
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 5
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Downstream Switch Port
| Device Class | System
| Device Location | PCI bus 32, device 6, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C7&REV_01
| Parent ID | PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
| Bus: 20h, Device: 06h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Parent Device | AMD 400 Series Chipset PCIe Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FC500000h - FC5FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 5.0 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.5 GB/sec)
| Link Port Number | 6
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Downstream Switch Port
| Device Class | System
| Device Location | PCI bus 32, device 5, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C7&REV_01
| Parent ID | PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
| Bus: 20h, Device: 07h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Parent Device | AMD 400 Series Chipset PCIe Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 7
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Downstream Switch Port
| Device Class | System
| Device Location | PCI bus 32, device 7, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Compatible ID | PCI\VEN_1022&DEV_43C7&REV_01
| Parent ID | PCI\VEN_1022&DEV_43C6&SUBSYS_02011B21&REV_01
| Bus: 25h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Hardware ID | VEN_10EC&DEV_8168
| Revision | 15h
| Interface | 00h
| Parent Device | AMD 400 Series Chipset PCIe Port
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC604000h - FC604FFFh
| Memory Address | FC600000h - FC603FFFh
| PCI-E Capabilities
| PCI Express Version | 1.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 2.5 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.25 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Realtek
| Device Description | Realtek PCIe GbE Family Controller
| Friendly Name | Realtek PCIe GbE Family Controller
| Device Class | Net
| Device Location | PCI bus 37, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 1.0.0.14
| Driver Date | 2-1-2021
| Inf File | rtcx21x64.inf
| Service Name | rtcx21
| Hardware ID | PCI\VEN_10EC&DEV_8168&SUBSYS_7A381462&REV_15
| Compatible ID | PCI\VEN_10EC&DEV_8168&REV_15
| Parent ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Bus: 27h, Device: 00h, Function: 00h
| Vendor (1B21h) | ASMedia Technology Inc.
| Device (1142h) | ASM1042A USB 3.0 Host Controller
| Subsys Vendor (1043h) | ASUSTeK Computer Inc
| Subsystem ID (86A0h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1B21&DEV_1142
| Revision | 00h
| Interface | 30h
| Parent Device | AMD 400 Series Chipset PCIe Port
| Connected Devices
| Device | ASUSTek Computer ASUS XONAR SC150 AUDIO DEVICE
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC500000h - FC507FFFh
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 5.0 GT/s (Current: 5.0 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.5 GB/sec)
| Link Port Number | 1
| Driver
| Driver Status | The device is working properly
| Manufacturer | Generic USB xHCI Host Controller
| Device Description | USB xHCI Compliant Host Controller
| Friendly Name | ASMedia USB 3.0 eXtensible Host Controller - 1.0 (Microsoft)
| Device Class | USB
| Device Location | PCI bus 39, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 5-21-2024
| Inf File | usbxhci.inf
| Service Name | USBXHCI
| Hardware ID | PCI\VEN_1B21&DEV_1142&SUBSYS_86A01043&REV_00
| Compatible ID | PCI\VEN_1B21&DEV_1142&REV_00
| Parent ID | PCI\VEN_1022&DEV_43C7&SUBSYS_33061B21&REV_01
| Bus: 29h, Device: 00h, Function: 00h
| Vendor (10DEh) | NVIDIA Corporation
| Device (2489h) | GeForce RTX 3060 Ti LHR [GA104]
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (3972h) | MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
| Class (03h) | Display
| SubClass (00h) | VGA
| Hardware ID | VEN_10DE&DEV_2489
| Revision | A1h
| Interface | 00h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Connected Devices
| Device | BenQ GW2470
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FB000000h - FBFFFFFFh
| Memory Address | D0000000h - DFFFFFFFh
| Memory Address | E0000000h - E1FFFFFFh
| Base I/O Port | 0000E000h - 0000E07Fh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | NVIDIA
| Device Description | NVIDIA GeForce RTX 3060 Ti
| Device Class | Display
| Device Location | PCI bus 41, device 0, function 0
| Driver Provider | NVIDIA
| Driver Version | 32.0.15.7216
| Driver Date | 1-26-2025
| Inf File | oem13.inf
| Service Name | nvlddmkm
| Hardware ID | PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_2489&REV_A1
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 29h, Device: 00h, Function: 01h
| Vendor (10DEh) | NVIDIA Corporation
| Device (228Bh) | GA104 High Definition Audio Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (3972h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | High Definition Audio
| Hardware ID | VEN_10DE&DEV_228B
| Revision | A1h
| Interface | 00h
| Parent Device | AMD Starship/Matisse GPP Bridge
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC080000h - FC083FFFh
| Sound
| Audio Codec Name | NVidia GPU GA104 HDMI/DP
| Controller Type | High Definition Audio
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 41, device 0, function 1
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3810
| Driver Date | 6-18-2024
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_10DE&DEV_228B&SUBSYS_39721462&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_228B&REV_A1
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
| Bus: 2Ah, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (148Ah) | Starship/Matisse PCIe Dummy Function
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (13h) | Non-Essential Instrumentation
| SubClass (00h) | Unknown
| Hardware ID | VEN_1022&DEV_148A
| Revision | 00h
| Interface | 00h
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices
| Device Description | AMD PCI
| Device Class | System
| Device Location | PCI bus 42, device 0, function 0
| Driver Provider | Advanced Micro Devices
| Driver Version | 1.0.0.90
| Driver Date | 3-26-2024
| Inf File | oem20.inf
| Service Name | AMDPCIDev
| Hardware ID | PCI\VEN_1022&DEV_148A&SUBSYS_7A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_148A&REV_00
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Bus: 2Bh, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1485h) | Starship/Matisse Reserved SPP
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (13h) | Non-Essential Instrumentation
| SubClass (00h) | Unknown
| Hardware ID | VEN_1022&DEV_1485
| Revision | 00h
| Interface | 00h
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices
| Device Description | AMD PCI
| Device Class | System
| Device Location | PCI bus 43, device 0, function 0
| Driver Provider | Advanced Micro Devices
| Driver Version | 1.0.0.90
| Driver Date | 3-26-2024
| Inf File | oem20.inf
| Service Name | AMDPCIDev
| Hardware ID | PCI\VEN_1022&DEV_1485&SUBSYS_7A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1485&REV_00
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Bus: 2Bh, Device: 00h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1486h) | Starship/Matisse Cryptographic Coprocessor PSPCPP
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (10h) | En/Decryption
| SubClass (80h) | Other
| Hardware ID | VEN_1022&DEV_1486
| Revision | 00h
| Interface | 00h
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC300000h - FC3FFFFFh
| Memory Address | FC408000h - FC409FFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices Inc.
| Device Description | AMD PSP 11.0 Device
| Device Class | SecurityDevices
| Device Location | PCI bus 43, device 0, function 1
| Driver Provider | Advanced Micro Devices Inc.
| Driver Version | 4.13.0.0
| Driver Date | 3-6-2020
| Inf File | oem16.inf
| Service Name | amdpsp
| Hardware ID | PCI\VEN_1022&DEV_1486&SUBSYS_7A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1486&REV_00
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Bus: 2Bh, Device: 00h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (149Ch) | Matisse USB 3.0 Host Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1022&DEV_149C
| Revision | 00h
| Interface | 30h
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Connected Devices
| Device 1 | Evision RGB Gaming Mechanical Keyboard
| Device 2 | Logitech G102 LIGHTSYNC Gaming Mouse
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC200000h - FC2FFFFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Generic USB xHCI Host Controller
| Device Description | USB xHCI Compliant Host Controller
| Friendly Name | AMD USB 3.10 eXtensible Host Controller - 1.10 (Microsoft)
| Device Class | USB
| Device Location | PCI bus 43, device 0, function 3
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 5-21-2024
| Inf File | usbxhci.inf
| Service Name | USBXHCI
| Hardware ID | PCI\VEN_1022&DEV_149C&SUBSYS_7A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_149C&REV_00
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| Bus: 2Bh, Device: 00h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1487h) | Starship/Matisse HD Audio Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (9A38h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | High Definition Audio
| Hardware ID | VEN_1022&DEV_1487
| Revision | 00h
| Interface | 00h
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC400000h - FC407FFFh
| Sound
| Audio Codec Name | Realtek ALC892
| Controller Type | High Definition Audio
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 43, device 0, function 4
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3810
| Driver Date | 6-18-2024
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_1022&DEV_1487&SUBSYS_9A381462&REV_00
| Compatible ID | PCI\VEN_1022&DEV_1487&REV_00
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
Memory Modules
| Memory Slot 3
| Memory Type | 8 GB DDR4-3602 (1801 MHz) SDRAM
| Manufacturer | Kingston
| DRAM Manufacturer | SK Hynix
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 16 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
| JEDEC Profile @ 1200 MHz | 18.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1200 MHz | 17.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1163 MHz | 16.0-16-16-38-54-408-303-187
| JEDEC Profile @ 1090 MHz | 15.0-15-15-35-50-382-284-175
| JEDEC Profile @ 1018 MHz | 14.0-14-14-33-47-357-265-163
| JEDEC Profile @ 945 MHz | 13.0-13-13-31-44-331-246-152
| JEDEC Profile @ 872 MHz | 12.0-12-12-28-40-306-227-140
| JEDEC Profile @ 799 MHz | 11.0-11-11-26-37-280-208-128
| JEDEC Profile @ 727 MHz | 10.0-10-10-24-34-255-190-117
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.20 V
| SPD Revision | 1.1
| Part Number | KF3600C16D4/8GX
| Manufacturing Location | 7
| Manufacture Date | September 2023 (2338h)
| Serial Number | 211C9E38h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Supported
| XMP Revision | 2.0
| XMP Profile 1
| Profile Name | XMP-3602 (1801 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1801 MHz | 18.0-20-20-39-85
| XMP Profile @ 1801 MHz | 17.0-20-20-39-85
| XMP Profile @ 1801 MHz | 16.0-20-20-39-85 (Active)
| XMP Profile @ 1689 MHz | 15.0-19-19-37-80
| XMP Profile @ 1576 MHz | 14.0-18-18-35-75
| XMP Profile @ 1463 MHz | 13.0-17-17-32-69
| XMP Profile @ 1351 MHz | 12.0-15-15-30-64
| XMP Profile @ 1238 MHz | 11.0-14-14-27-59
| XMP Profile @ 1126 MHz | 10.0-13-13-25-53
| XMP Profile 2
| Profile Name | XMP-2998 (1499 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1499 MHz | 17.0-17-17-36-64
| XMP Profile @ 1499 MHz | 16.0-17-17-36-64
| XMP Profile @ 1499 MHz | 15.0-17-17-36-64
| XMP Profile @ 1399 MHz | 14.0-16-16-34-60
| XMP Profile @ 1299 MHz | 13.0-15-15-32-56
| XMP Profile @ 1199 MHz | 12.0-14-14-29-52
| XMP Profile @ 1099 MHz | 11.0-13-13-27-47
| XMP Profile @ 899 MHz | 9.0-11-11-22-39
| Memory Slot 4
| Memory Type | 8 GB DDR4-3602 (1801 MHz) SDRAM
| Manufacturer | Kingston
| DRAM Manufacturer | SK Hynix
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 16 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
| JEDEC Profile @ 1200 MHz | 18.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1200 MHz | 17.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1163 MHz | 16.0-16-16-38-54-408-303-187
| JEDEC Profile @ 1090 MHz | 15.0-15-15-35-50-382-284-175
| JEDEC Profile @ 1018 MHz | 14.0-14-14-33-47-357-265-163
| JEDEC Profile @ 945 MHz | 13.0-13-13-31-44-331-246-152
| JEDEC Profile @ 872 MHz | 12.0-12-12-28-40-306-227-140
| JEDEC Profile @ 799 MHz | 11.0-11-11-26-37-280-208-128
| JEDEC Profile @ 727 MHz | 10.0-10-10-24-34-255-190-117
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.20 V
| SPD Revision | 1.1
| Part Number | KF3600C16D4/8GX
| Manufacturing Location | 7
| Manufacture Date | November 2023 (2346h)
| Serial Number | 804C34DDh
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Supported
| XMP Revision | 2.0
| XMP Profile 1
| Profile Name | XMP-3602 (1801 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1801 MHz | 18.0-20-20-39-85
| XMP Profile @ 1801 MHz | 17.0-20-20-39-85
| XMP Profile @ 1801 MHz | 16.0-20-20-39-85 (Active)
| XMP Profile @ 1689 MHz | 15.0-19-19-37-80
| XMP Profile @ 1576 MHz | 14.0-18-18-35-75
| XMP Profile @ 1463 MHz | 13.0-17-17-32-69
| XMP Profile @ 1351 MHz | 12.0-15-15-30-64
| XMP Profile @ 1238 MHz | 11.0-14-14-27-59
| XMP Profile @ 1126 MHz | 10.0-13-13-25-53
| XMP Profile 2
| Profile Name | XMP-2998 (1499 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1499 MHz | 17.0-17-17-36-64
| XMP Profile @ 1499 MHz | 16.0-17-17-36-64
| XMP Profile @ 1499 MHz | 15.0-17-17-36-64
| XMP Profile @ 1399 MHz | 14.0-16-16-34-60
| XMP Profile @ 1299 MHz | 13.0-15-15-32-56
| XMP Profile @ 1199 MHz | 12.0-14-14-29-52
| XMP Profile @ 1099 MHz | 11.0-13-13-27-47
| XMP Profile @ 899 MHz | 9.0-11-11-22-39
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 131072 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 4
| Structure Length | 17h
| Memory Device 1
| Size | Not Installed
| Form Factor | Unknown
| Memory Type | Unknown
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | Unknown
| Maximum Voltage | Unknown
| Minimum Voltage | Unknown
| Device Locator | DIMM 0
| Bank Locator | P0 CHANNEL A
| Total Width | Unknown
| Data Width | Unknown
| Device Set | 00h
| Type Detail | Unknown
| Manufacturer | Unknown
| Serial Number | Unknown
| Asset Tag |
| Part Number | Unknown
| Structure Length | 28h
| Memory Device 2
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR4
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | 1.2 V
| Maximum Voltage | 1.2 V
| Minimum Voltage | 1.2 V
| Device Locator | DIMM 1
| Bank Locator | P0 CHANNEL A
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous, Unbuffered (Unregistered)
| Manufacturer | Kingston
| Serial Number | 211C9E38
| Asset Tag |
| Part Number | KF3600C16D4/8GX
| Structure Length | 28h
| Memory Device 3
| Size | Not Installed
| Form Factor | Unknown
| Memory Type | Unknown
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | Unknown
| Maximum Voltage | Unknown
| Minimum Voltage | Unknown
| Device Locator | DIMM 0
| Bank Locator | P0 CHANNEL B
| Total Width | Unknown
| Data Width | Unknown
| Device Set | 00h
| Type Detail | Unknown
| Manufacturer | Unknown
| Serial Number | Unknown
| Asset Tag |
| Part Number | Unknown
| Structure Length | 28h
| Memory Device 4
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR4
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | 1.2 V
| Maximum Voltage | 1.2 V
| Minimum Voltage | 1.2 V
| Device Locator | DIMM 1
| Bank Locator | P0 CHANNEL B
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous, Unbuffered (Unregistered)
| Manufacturer | Kingston
| Serial Number | 804C34DD
| Asset Tag |
| Part Number | KF3600C16D4/8GX
| Structure Length | 28h
Disk
| Disk
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA8-ACS
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Buffer Size | 32 MB
| Buffer Type | Not Specified
| Disk Temperature | 39 °C (102 °F)
| Reallocated Sectors | 3
| Disk Health Status | Poor
| Power On Hours Count | 15666 Hour(s)
| Drive Power Cycle Count | 7459
| Logical Drives | E:, F:, H:
| ECC bytes | 50
| Security Erase Time | 194 min
| Enh. Security Erase | 194 min
| Current APM Value | None
| Acoustic Management | 80h (80h Recommended) - Enabled
| Location | AMD 400 Series Chipset SATA Controller
| Transfer Modes
| SATA Speed | 300 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
| Sectors per Interrupt | 16, Active: 16
| Disk Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Not Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Enabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Enabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 51 | 190 | 200 | 42
| 3 | Spin-up Time | 21 | 253 | 253 | 6266
| 4 | Start/Stop Count | 0 | 83 | 83 | 17599
| 5 | Reallocated Sectors Count | 140 | 199 | 199 | 3
| 7 | Seek Error Rate | 51 | 253 | 100 | 0
| 9 | Power On Hours Count | 0 | 79 | 79 | 15666
| 10 | Spin-up Retry Count | 51 | 100 | 100 | 0
| 11 | Recalibration Retries | 51 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 0 | 93 | 93 | 7459
| 192 | Power-Off Retract Count | 0 | 199 | 199 | 1317
| 193 | Load/Unload Cycle Count | 0 | 195 | 195 | 17585
| 194 | Drive Temperature | 0 | 97 | 111 | 39
| 196 | Reallocation Event Count | 0 | 198 | 200 | 0
| 197 | Current Pending Sectors | 0 | 200 | 200 | 1
| 198 | Uncorrectable Sectors | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 0
| 200 | Write Error Rate | 51 | 197 | 200 | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | WDC WD1001FALS-00J7B0
| Device Class | DiskDrive
| Device Location | Bus Number 1, Target Id 0, LUN 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | SCSI\DiskWDC_____WD1001FALS-00J7B05.0
| Compatible ID | SCSI\Disk
| Parent ID | PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
| Disk
| Disk Model | Samsung SSD 970 EVO Plus 1TB
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | NVMe 1.3.0
| Serial Number | S6P7NF0T435103B
| Controller Revision | 4B2QEXM7
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Disk Temperature | 41 °C (106 °F)
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Power On Hours Count | 7481 Hour(s)
| Drive Power Cycle Count | 4621
| Total Host Writes | 10.77 TB
| Total Host Reads | 18.87 TB
| Logical Drives | C:, D:, G:, I:, J:
| Controller Manufacturer | Samsung Electronics Co., Ltd., Memory Division
| IEEE OUI Identifier | 00-25-38
| Controller ID | 6
| Number of Namespaces | 1
| Power Consumption | 0.005-7.5 Wattes
| Number of Power States | 5
| Warning Temperature Threshold | 82 °C (180 °F)
| Critical Temperature Threshold | 85 °C (185 °F)
| Max Data Transfer Size | 128 Pages
| Abort Command Limit | 8
| Asynchronous Event Request Limit | 4
| Firmware Slots | 3
| Time for Firmware Activation | 0 sec
| Max Error Log Page Entries | 64
| Host Memory Buffer Preferred Size | 0 kB
| Host Memory Buffer Minimum Size | 0 kB
| Extended Self-Test Time | 35 min
| Submission Queue Entry Size | Minimum: 64 bytes, Maximum: 64 bytes
| Completion Queue Entry Size | Minimum: 16 bytes, Maximum: 16 bytes
| Subsystem Name | nqn.1994-11.com.samsung:nvme:980PRO:M.2:S6P7NF0T435103B
| Location | Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
| Transfer Modes
| Bus Type | PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| NVMe Commands
| Security Send/Receive | Supported
| Format NVM | Supported
| Firmware Commit | Supported
| Firmware Image Download | Supported
| Namespace Management | Not Supported
| Device Self-test | Supported
| Directive Send/Receive | Not Supported
| NVMe-MI Send/Receive | Not Supported
| Virtualization Management | Not Supported
| Doorbell Buffer Config | Not Supported
| Compare | Supported
| Write Uncorrectable | Supported
| Dataset Management | Supported
| Write Zeroes | Not Supported
| Reservations | Not Supported
| Verify | Not Supported
| NVMe Features
| Volatile Write Cache | Supported
| Get LBA Status | Not Supported
| SMART Info Per Namespace | Supported
| Command Effects Log Page | Supported
| Get Log Page Extended Data | Supported
| Telemetry Host-Initiated | Supported
| Telemetry Controller-Initiated | Supported
| Persistent Event Log | Not Supported
| Autonomous Power State Transition | Supported
| Keep Alive Support | Not Supported
| Thermal Management | Supported
| Crypto Erase Support | Supported
| Block Erase Support | Supported
| Overwrite Support | Not Supported
| Save Select Field | Supported
| Timestamp Feature | Supported
| Compare/Write Fused Operation | Not Supported
| NVM Sets | Not Supported
| Endurance Groups | Supported
| S.M.A.R.T.
| ID | Attribute Name | Raw Value
| 0 | Critical Warning | 0
| 1 | Composite Temperature | 314
| 3 | Available Spare | 100
| 4 | Available Spare Threshold | 10
| 5 | Percentage Used | 0
| 6 | Endurance Group Critical Warning | 0
| 32 | Data Units Read | 40513127
| 48 | Data Units Written | 23138422
| 64 | Host Read Commands | 701768617
| 80 | Host Write Commands | 396723296
| 96 | Controller Busy Time | 4155
| 112 | Drive Power Cycle Count | 4621
| 128 | Power On Hours Count | 7481
| 144 | Unsafe Shutdown Count | 1286
| 160 | Media and Data Integrity Errors | 0
| 176 | Error Information Log Entries | 0
| 192 | Warning Composite Temperature Time | 0
| 196 | Critical Composite Temperature Time | 0
| 200 | Temperature Sensor 1 | 314
| 202 | Temperature Sensor 2 | 320
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Samsung SSD 970 EVO Plus 1TB
| Device Class | DiskDrive
| Device Location | Bus Number 0, Target Id 0, LUN 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | SCSI\DiskNVMe________________Samsung_SSD_970_EVO_Plus_1TB4B2QEXM7
| Compatible ID | SCSI\Disk
| Parent ID | PCI\VEN_144D&DEV_A808&SUBSYS_A801144D&REV_00
ATAPI
| ATAPI
| ATAPI Model | ATAPI DVD W DH16W1S
| ATAPI Type | DVD+-RW DL/CD-RW
| Interface Type | Serial ATA I
| Physical Interface | Serial ATAPI
| ATAPI Name | ATAPI DVD W DH16W1S
| Vendor Specific | 2006/10/27 19:00
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 48x (Current: 48x)
| DVD Read Speed | Current: 5x
| DVD Write Speed | Current: 5x
| Buffer Size | 2 MB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 48
| Write Retry Count | 0
| Compatibility | ATA/ATAPI-7
| Serial Number |
| Controller Revision | 2A11
| Logical Drives | M:
| Command DRQ Type | Accelerated DRQ
| Command Packet Size | 12 bytes
| Location | AMD 400 Series Chipset SATA Controller
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | 7, Active: 2
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 5 (UltraDMA/100), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Supported
| DVD-R DL Disk Read | Supported
| DVD-RW Disk Read | Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Supported
| DVD+R DL Disk Read | Supported
| DVD+RW Disk Read | Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Supported
| DVD-R DL Disk Write | Not Supported
| DVD-RW Disk Write | Supported
| DVD+R Disk Write | Supported
| DVD+R DL Disk Write | Supported
| DVD+RW Disk Write | Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Not Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| S.M.A.R.T. | Not Supported
| S.M.A.R.T. Self-test | Not Supported
| S.M.A.R.T. Error Logging | Not Supported
| Security Mode Feature Set | Not Supported
| Removable Media | Not Supported
| Power Management | Not Supported
| PACKET Command | Supported, Enabled
| Write Cache | Not Supported
| Look-ahead | Not Supported
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Supported, Enabled
| Host Protected Area | Not Supported
| Write Verify Command | Not Supported
| Write Buffer Command | Not Supported
| Read Buffer Command | Not Supported
| NOP Command | Not Supported
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Not Supported
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Not Supported
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Not Supported
| Device Configuration Overlay | Not Supported
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Not Supported
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Not Supported
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard CD-ROM drives)
| Device Description | CD-ROM Drive
| Friendly Name | ATAPI DVD W DH16W1S
| Device Class | CDROM
| Device Location | Bus Number 5, Target Id 0, LUN 0
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | cdrom.inf
| Service Name | cdrom
| Hardware ID | SCSI\CdRomATAPI___DVD_W__DH16W1S__2A11
| Compatible ID | SCSI\CdRom
| Parent ID | PCI\VEN_1022&DEV_43C8&SUBSYS_10621B21&REV_01
Storage (ASPI)
| ASPI devices not found
Logical Drives
| Local Drives
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT
| Volume Serial Number | 0805-FB80
| Total Size | 1.99 GB
| Free Space | 478.25 MB (23.4%)
| Location | Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT32
| Volume Serial Number | 089E-9200
| Total Size | 29.99 GB
| Free Space | 7.15 GB (23.9%)
| Location | Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
| E:[WIN2K]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | WIN2K
| File System | NTFS
| Volume Serial Number | A4B5-2192
| Total Size | 30.0 GB
| Free Space | 20.35 GB (67.8%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| F:[WINXP]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | WINXP
| File System | NTFS
| Volume Serial Number | 90B8-E3D0
| Total Size | 10.0 GB
| Free Space | 8.91 GB (89.1%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| G:[WIN7]
| Drive Letter | G:
| Drive Type | Fixed Disk
| Volume Label | WIN7
| File System | NTFS
| Volume Serial Number | 1C61-A5D1
| Total Size | 250.0 GB
| Free Space | 45.34 GB (18.1%)
| Location | Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
| H:[MUSIC]
| Drive Letter | H:
| Drive Type | Fixed Disk
| Volume Label | MUSIC
| File System | NTFS
| Volume Serial Number | 56C9-FD1A
| Total Size | 891.51 GB
| Free Space | 16.43 GB (1.8%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| I:[GAMES]
| Drive Letter | I:
| Drive Type | Fixed Disk
| Volume Label | GAMES
| File System | NTFS
| Volume Serial Number | E8D9-213C
| Total Size | 619.52 GB
| Free Space | 202.73 GB (32.7%)
| Location | Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
| J:[WIN11]
| Drive Letter | J:
| Drive Type | Fixed Disk
| Volume Label | WIN11
| File System | NTFS
| Volume Serial Number | CC50-1EE0
| Total Size | 30.0 GB
| Free Space | 1.51 GB (5.0%)
| Location | Samsung SSD 970 EVO Plus 1TB (S6P7NF0T435103B)
| M:
| Drive Letter | M:
| Drive Type | Optical Drive
| Location | ATAPI DVD W DH16W1S
USB Devices
| USB Device 1
| Vendor (320Fh) | Evision
| Device (5000h) | RGB Gaming Mechanical Keyboard
| Manufacturer | Evision
| Product | RGB Keyboard
| Serial Number |
| Device Version | 1.06
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.0
| Current Speed | 12 Mbit/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | 400 mA Remote Wakeup
| Parent Device | AMD Matisse USB 3.0 Host Controller
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0003.Hub_#0003
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_320F&PID_5000&REV_0106
| Compatible ID | USB\COMPAT_VID_320F&DevClass_00&SubClass_00&Prot00
| Parent ID | PCI\VEN_1022&DEV_149C&SUBSYS_7A381462&REV_00
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (01h) | Keyboard
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 002b.0000.0003.003.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_320F&PID_5000&REV_0106&MI_00
| Compatible ID | USB\COMPAT_VID_320f&Class_03&SubClass_01&Prot_01
| Parent ID | USB\VID_320F&PID_5000&REV_0106
| Interface 2
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 002b.0000.0003.003.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_320F&PID_5000&REV_0106&MI_01
| Compatible ID | USB\COMPAT_VID_320f&Class_03&SubClass_01&Prot_02
| Parent ID | USB\VID_320F&PID_5000&REV_0106
| USB Device 2
| Vendor (046Dh) | Logitech
| Device (C09Dh) | G102 LIGHTSYNC Gaming Mouse
| Manufacturer | Logitech
| Product | G102 LIGHTSYNC Gaming Mouse
| Serial Number | 205834584258
| Device Version | 52.02
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration | U152.02_B0017
| USB Version | 2.0
| Current Speed | 12 Mbit/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | 300 mA Remote Wakeup
| Parent Device | AMD Matisse USB 3.0 Host Controller
| Driver
| Driver Status | The device is working properly
| Manufacturer | Logitech
| Device Description | G203 LIGHTSYNC
| Friendly Name | G102 LIGHTSYNC
| Device Class | USB
| Device Location | Port_#0004.Hub_#0003
| Driver Provider | Logitech
| Driver Version | 1.1.55.3120
| Driver Date | 4-15-2024
| Inf File | oem15.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_046D&PID_C09D&REV_5202
| Compatible ID | USB\COMPAT_VID_046D&DevClass_00&SubClass_00&Prot00
| Parent ID | PCI\VEN_1022&DEV_149C&SUBSYS_7A381462&REV_00
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 002b.0000.0003.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_046D&PID_C09D&REV_5202&MI_00
| Compatible ID | USB\COMPAT_VID_046d&Class_03&SubClass_01&Prot_02
| Parent ID | USB\VID_046D&PID_C09D&REV_5202
| Interface 2
| Class (03h) | Human Interface Devices
| SubClass (00h) | No Subclass
| Protocol (00h) | None
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 002b.0000.0003.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_046D&PID_C09D&REV_5202&MI_01
| Compatible ID | USB\COMPAT_VID_046d&Class_03&SubClass_00&Prot_00
| Parent ID | USB\VID_046D&PID_C09D&REV_5202
| USB Device 3
| Vendor (04A9h) | Canon
| Device (2660h) | LaserBase MF3110 Scanner/Printer
| Manufacturer | Canon,Inc.
| Product | MF3110
| Serial Number | 2363E2124558
| Device Version | 0.0
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.0
| Current Speed | 480 Mbit/s
| Transfer Type | Bulk/Interrupt
| Data Packet Size | 64 bytes
| Max Power | 2 mA Self-Powered
| Parent Device | AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0011.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000
| Compatible ID | USB\COMPAT_VID_04A9&DevClass_00&SubClass_00&Prot00
| Parent ID | PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
| Interface 1
| Class (FFh) | Vendor Specific Class
| SubClass (00h) | Unknown
| Protocol (FFh) | Unknown
| Interface |
| Driver
| Driver Status | The drivers for this device are not installed (28)
| Device Description | MF3110
| Device Location | 0003.0000.0000.011.000.000.000.000.000
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000&MI_00
| Compatible ID | USB\COMPAT_VID_04a9&Class_ff&SubClass_00&Prot_ff
| Parent ID | USB\VID_04A9&PID_2660&REV_0000
| Interface 2
| Class (07h) | Printer
| SubClass (01h) | Printer
| Protocol (02h) | Bidirectional
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | USB Printing Support
| Friendly Name | Canon MF3110
| Device Class | USB
| Device Location | 0003.0000.0000.011.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4249
| Driver Date | 6-21-2006
| Inf File | usbprint.inf
| Service Name | usbprint
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000&MI_01
| Compatible ID | USB\COMPAT_VID_04a9&Class_07&SubClass_01&Prot_02
| Parent ID | USB\VID_04A9&PID_2660&REV_0000
| USB Device 4
| Vendor (0B05h) | ASUSTek Computer
| Device (180Dh) | ASUS XONAR SC150 AUDIO DEVICE
| Manufacturer | ASUSTeK
| Product | STRIX SOUND CARD
| Serial Number |
| Device Version | 1.03
| Class (EFh) | Miscellaneous Device
| SubClass (02h) | Common Class
| Protocol (01h) | Interface Association
| Configuration |
| USB Version | 2.0
| Current Speed | 480 Mbit/s
| Transfer Type | Isochronous/Interrupt
| Data Packet Size | 64 bytes
| Max Power | 500 mA
| Parent Device | ASMedia Technology Inc. ASM1042A USB 3.0 Host Controller
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0003.Hub_#0002
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_0B05&PID_180D&REV_0103
| Compatible ID | USB\COMPAT_VID_0B05&DevClass_00&SubClass_00&Prot00
| Parent ID | PCI\VEN_1B21&DEV_1142&SUBSYS_86A01043&REV_00
| Interface 1
| Class (01h) | Audio
| SubClass (01h) | Control Device
| Protocol (20h) | Unknown
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | USB Audio 2.0
| Friendly Name | STRIX SOUND CARD
| Device Class | MEDIA
| Device Location | 0027.0000.0000.003.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 5-6-2022
| Inf File | usbaudio2.inf
| Service Name | usbaudio2
| Hardware ID | USB\VID_0B05&PID_180D&REV_0103&MI_00
| Compatible ID | USB\COMPAT_VID_0b05&Class_01&SubClass_00&Prot_20
| Parent ID | USB\VID_0B05&PID_180D&REV_0103
| Interface 2
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface | Speaker
| Interface 3
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 4
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 5
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 0027.0000.0000.003.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4111
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_0B05&PID_180D&REV_0103&MI_04
| Compatible ID | USB\COMPAT_VID_0b05&Class_03&SubClass_00&Prot_00
| Parent ID | USB\VID_0B05&PID_180D&REV_0103
| Interface 6
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 7
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 8
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 9
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 10
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 11
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface | SPDIF Output
| Interface 12
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 13
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 14
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 15
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface | Input
| Interface 16
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 17
| Class (01h) | Audio
| SubClass (02h) | Streaming
| Protocol (20h) | Unknown
| Interface |
| Interface 18
| Class (03h) | Human Interface Devices
| SubClass (00h) | No Subclass
| Protocol (00h) | None
| Interface |
Plug and Play
| Plug and Play
| PnP Version | 1.0
| Number of PnP Devices | 25
| PnP Device 1
| Vendor | Generic System Device
| Device Name | AT Interrupt Controller
| PnP Device ID | ACPI\VEN_PNP&DEV_0000
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Programmable interrupt controller
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0000
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 2
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 3
| Vendor | Generic System Device
| Device Name | Standard LPT printer port
| PnP Device ID | ACPI\VEN_PNP&DEV_0400
| Class (07h) | Communication
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| I/O Port | 378h-37Fh
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard port types)
| Device Description | Printer Port
| Friendly Name | Ïîðò ïðèíòåðà (LPT1)
| Device Class | Ports
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | msports.inf
| Service Name | Parport
| Hardware ID | ACPI\VEN_PNP&DEV_0400
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 4
| Vendor | Advanced Micro Devices, Inc.
| Device Name | AMD GPIO Controller
| PnP Device ID | ACPI\VEN_AMDI&DEV_F030
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Memory Address | FEC30000h-FEC30FFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc.
| Device Description | AMD GPIO Controller
| Device Class | System
| Driver Provider | Advanced Micro Devices, Inc.
| Driver Version | 2.0.1.0
| Driver Date | 3-9-2020
| Inf File | oem6.inf
| Service Name | amdgpio3
| Hardware ID | ACPI\VEN_AMDI&DEV_F030
| Compatible ID | ACPI\AMDIF030
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 5
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | PCI\VEN_1022&DEV_1484&SUBSYS_14627A38&REV_00
| PnP Device 6
| Vendor | Generic System Device
| Device Name | Intel High Precision Event Timer
| PnP Device ID | ACPI\VEN_PNP&DEV_0103
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | High precision event timer
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0103
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 7
| Vendor | Generic System Device
| Device Name | AT DMA Controller
| PnP Device ID | ACPI\VEN_PNP&DEV_0200
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Direct memory access controller
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0200
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 8
| Vendor | Advanced Micro Devices, Inc.
| Device Name | AMD GPIO Controller
| PnP Device ID | ACPI\VEN_AMDI&DEV_0030
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| System IRQ | 7
| Memory Address | FED81500h-FED818FFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc
| Device Description | AMD GPIO Controller
| Device Class | System
| Driver Provider | Advanced Micro Devices, Inc
| Driver Version | 2.2.0.130
| Driver Date | 3-11-2020
| Inf File | oem17.inf
| Service Name | amdgpio2
| Hardware ID | ACPI\VEN_AMDI&DEV_0030
| Compatible ID | ACPI\AMDI0030
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 9
| Vendor | Generic System Device
| Device Name | 16550A-compatible COM port
| PnP Device ID | ACPI\VEN_PNP&DEV_0501
| Class (07h) | Communication
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| I/O Port | 3F8h-3FFh
| System IRQ | 4
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard port types)
| Device Description | Communications Port
| Friendly Name | Ïîñëåäîâàòåëüíûé ïîðò (COM1)
| Device Class | Ports
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | msports.inf
| Service Name | Serial
| Hardware ID | ACPI\VEN_PNP&DEV_0501
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 10
| Vendor | Generic System Device
| Device Name | AT standard speaker sound
| PnP Device ID | ACPI\VEN_PNP&DEV_0800
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | System speaker
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0800
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 11
| Vendor | Generic System Device
| Device Name | ISA System Board
| PnP Device ID | ACPI\VEN_PNP&DEV_0C01
| Class (08h) | System Peripheral
| Parent Device | PCI Bus Host Bridge
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | System board
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C01
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| PnP Device 12
| Vendor | Generic System Device
| Device Name | Microsoft Windows Management Interface for ACPI
| PnP Device ID | ACPI\VEN_PNP&DEV_0C14
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | Microsoft Windows Management Interface for ACPI
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3958
| Driver Date | 6-21-2006
| Inf File | wmiacpi.inf
| Service Name | WmiAcpi
| Hardware ID | ACPI\VEN_PNP&DEV_0C14
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 13
| Vendor | Generic System Device
| Device Name | Microsoft Windows Management Interface for ACPI
| PnP Device ID | ACPI\VEN_PNP&DEV_0C14
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | Microsoft Windows Management Interface for ACPI
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3958
| Driver Date | 6-21-2006
| Inf File | wmiacpi.inf
| Service Name | WmiAcpi
| Hardware ID | ACPI\VEN_PNP&DEV_0C14
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 14
| Vendor | Generic System Device
| Device Name | PCI Bus Host Bridge
| PnP Device ID | ACPI\VEN_PNP&DEV_0A08
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Connected Devices
| Device 1 | AMD Starship/Matisse Root Complex
| Device 2 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 3 | AMD Starship/Matisse GPP Bridge
| Device 4 | AMD Starship/Matisse GPP Bridge
| Device 5 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 6 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 7 | AMD Starship/Matisse GPP Bridge
| Device 8 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 9 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 10 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 11 | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device 12 | AMD Starship/Matisse PCIe Dummy Host Bridge
| Device 13 | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Device 14 | AMD Hudson SMBus Controller
| Device 15 | AMD B450 Fusion Controller Hub (FCH)
| Device 16 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 0
| Device 17 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 1
| Device 18 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 2
| Device 19 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 3
| Device 20 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 4
| Device 21 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 5
| Device 22 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 6
| Device 23 | AMD Matisse/Vermeer Data Fabric: Device 18h; Function 7
| Device 24 | ISA System Board
| Device 25 | Motherboard registers
| Device 26 | Motherboard registers
| Device Resources
| I/O Port | 00h-3AFh
| I/O Port | 3E0h-CF7h
| I/O Port | 3B0h-3DFh
| I/O Port | D00h-FFFFh
| Memory Address | 000A0000h-000BFFFFh
| Memory Address | 000C0000h-000DFFFFh
| Memory Address | C0000000h-FEC2FFFFh
| Memory Address | FEE00000h-FFFFFFFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI Express Root Complex
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.4317
| Driver Date | 6-21-2006
| Inf File | pci.inf
| Service Name | pci
| Hardware ID | ACPI\VEN_PNP&DEV_0A08
| Compatible ID | *PNP0A03
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 15
| Vendor | Generic System Device
| Device Name | ACPI system board hardware
| PnP Device ID | ACPI_HAL\PNP0C08
| Class (08h) | System Peripheral
| Connected Devices
| Device 1 | Advanced Micro Devices, Inc. AMD GPIO Controller
| Device 2 | Intel High Precision Event Timer
| Device 3 | Advanced Micro Devices, Inc. AMD GPIO Controller
| Device 4 | Microsoft Windows Management Interface for ACPI
| Device 5 | Microsoft Windows Management Interface for ACPI
| Device 6 | PCI Bus Host Bridge
| Device 7 | Generic System Device Trusted Platform Module 2.0
| Device 8 | Microsoft Windows Management Interface for ACPI
| Device 9 | Motherboard registers
| Device 10 | Motherboard registers
| Device 11 | ACPI power button device
| Device 12 | MSI Software Component Interface
| Device Resources
| System IRQ | 55
| System IRQ | 0-255
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | Microsoft ACPI-Compliant System
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3810
| Driver Date | 6-21-2006
| Inf File | acpi.inf
| Service Name | ACPI
| Hardware ID | ACPI_HAL\PNP0C08
| Parent ID | acpiapic
| PnP Device 16
| Vendor | Generic System Device
| Device Name | AT Timer
| PnP Device ID | ACPI\VEN_PNP&DEV_0100
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | System timer
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0100
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
| PnP Device 17
| Vendor | Generic System Device
| Device Name | Trusted Platform Module 2.0
| PnP Device ID | ACPI\VEN_MSFT&DEV_0101
| Parent Device | ACPI system board hardware
| Device Resources
| Memory Address | BB465000h-BB468FFFh
| Memory Address | BB469000h-BB46CFFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard)
| Device Description | Trusted Platform Module 2.0
| Device Class | SecurityDevices
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | tpm.inf
| Service Name | TPM
| Hardware ID | ACPI\VEN_MSFT&DEV_0101
| Compatible ID | ACPI\MSFT0101
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 18
| Vendor | Generic System Device
| Device Name | Microsoft Windows Management Interface for ACPI
| PnP Device ID | ACPI\VEN_PNP&DEV_0C14
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | Microsoft Windows Management Interface for ACPI
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3958
| Driver Date | 6-21-2006
| Inf File | wmiacpi.inf
| Service Name | WmiAcpi
| Hardware ID | ACPI\VEN_PNP&DEV_0C14
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 19
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | PCI Bus Host Bridge
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| PnP Device 20
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 21
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 22
| Vendor | Generic System Device
| Device Name | ACPI power button device
| PnP Device ID | ACPI\VEN_PNP&DEV_0C0C
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | ACPI Power Button
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C0C
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 23
| Vendor | MSI
| Device Name | Software Component Interface
| PnP Device ID | ACPI\VEN_MBAD&DEV_0001
| Class (08h) | System Peripheral
| Parent Device | ACPI system board hardware
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | Micro-Star INT'L CO., LTD.
| Device Description | MSI Software Component Interface
| Device Class | System
| Driver Provider | Micro-Star INT'L CO., LTD.
| Driver Version | 1.0.0.14
| Driver Date | 8-20-2024
| Inf File | oem2.inf
| Hardware ID | ACPI\VEN_MBAD&DEV_0001
| Parent ID | ACPI_HAL\PNP0C08
| PnP Device 24
| Vendor | Generic System Device
| Device Name | Motherboard registers
| PnP Device ID | ACPI\VEN_PNP&DEV_0C02
| Class (08h) | System Peripheral
| Parent Device | PCI Bus Host Bridge
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Motherboard resources
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0C02
| Parent ID | ACPI\VEN_PNP&DEV_0A08
| PnP Device 25
| Vendor | Generic System Device
| Device Name | AT Real-Time Clock
| PnP Device ID | ACPI\VEN_PNP&DEV_0B00
| Class (08h) | System Peripheral
| Parent Device | AMD B450 Fusion Controller Hub (FCH)
| Device Resources
| I/O Port | 70h-71h
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | System CMOS/real time clock
| Device Class | System
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.1
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | ACPI\VEN_PNP&DEV_0B00
| Parent ID | PCI\VEN_1022&DEV_790E&SUBSYS_7A381462&REV_51
Physical Printers
| USB Printer 1
| Vendor (04A9h) | Canon
| Device (2660h) | LaserBase MF3110 Scanner/Printer
| Manufacturer | Canon,Inc.
| Product | MF3110
| Serial Number | 2363E2124558
| Device Version | 0.0
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.0
| Speed | 480 Mbit/s
| Transfer Type | Bulk/Interrupt
| Data Packet Size | 64 bytes
| Max Power | 2 mA Self-Powered
| Parent Device | AMD 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0011.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000
| Compatible ID | USB\COMPAT_VID_04A9&DevClass_00&SubClass_00&Prot00
| Parent ID | PCI\VEN_1022&DEV_43D5&SUBSYS_11421B21&REV_01
Installed Printers
| Local Printers
| Installed Printer 1
| Printer Name | Microsoft Print to PDF
| Printer Port | PORTPROMPT:
| Default Printer | Yes
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
Slots (SMBIOS)
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J6B2
| Slot Length | Long Length
| Slot ID | 0
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6B1
| Slot Length | Short Length
| Slot ID | 1
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6D1
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J7B1
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8B4
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8D1
| Slot Length | Short Length
| Slot ID | 5
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | J8B3
| Slot Length | Short Length
| Slot ID | 6
| Slot PCI Express x16
| Slot Type | PCI Express x16
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J10
| Slot Length | Short Length
| Slot ID | 12
| Slot PCI Express x8
| Slot Type | PCI Express x8
| Current Usage | Available
| Data Bus Width | 8x or x8
| Slot Designation | J3600 Pcie x8 slot
| Slot Length | Short Length
| Slot ID | 13
| Slot PCI Express x4
| Slot Type | PCI Express x4
| Current Usage | Other
| Data Bus Width | 4x or x4
| Slot Designation | J3707 Pcie x4 slot
| Slot Length | Short Length
| Slot ID | 32
| Slot PCI Express x4
| Slot Type | PCI Express x4
| Current Usage | In Use
| Data Bus Width | 4x or x4
| Slot Designation | J3700 PCIE x4 slot from Promontory
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3702 PCIE x1 slot from Promontory
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3703 PCIE x1 slot from Promontory
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3701 M.2 WLAN/BT slot
| Slot Length | Short Length
| Slot ID | 5
Ports (SMBIOS)
| Port 1 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1500
| Ext. Designator | USB 3.0
| Port 2 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1501
| Ext. Designator | USB 3.0
| Port 3 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1502
| Ext. Designator | USB-C
| Port 4 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1503
| Ext. Designator | USB 3.0
| Port 5 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1504
| Ext. Designator | USB 3.1
| Port 6 Network Port
| Int. Connector Type | None
| Ext. Connector Type | RJ-45
| Port Type | Network Port
| Int. Designator | J1503
| Ext. Designator | Network
| Port 7 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1704
| Ext. Designator | Sata Express
| Port 8 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1705
| Ext. Designator | Sata Express
| Port 9 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1701
| Ext. Designator | iSATA
| Port 10 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1702
| Ext. Designator | iSATA
| Port 11 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1703
| Ext. Designator | iSATA
| Port 12 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1706
| Ext. Designator | iSATA
| Port 13 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1100
| Ext. Designator | HDMI
| Port 14 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1101
| Ext. Designator | HDMI
| Port 15 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1102
| Ext. Designator | DP
| Port 16 Audio Port
| Int. Connector Type | None
| Ext. Connector Type | Mini-jack (headphones)
| Port Type | Audio Port
| Int. Designator | J2100
| Ext. Designator | Front Audio
| Port 17 Audio Port
| Int. Connector Type | None
| Ext. Connector Type | Mini-jack (headphones)
| Port Type | Audio Port
| Int. Designator | J2101
| Ext. Designator | Audio Jack
| Port 18 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1700
| Ext. Designator | Sata Express
Power
| Power
| AC Power Status | Online
| Battery Status | No Battery
| Power Plan
| Power Plan | Balanced
| Sleep After | 15 min
| Allow Hybrid Sleep | On
| Fast Startup | No
| Hibernate | No
| Turn Off Disk After | 20 min
| Turn Off Display After | 5 min
| Power Button Action | Shut Down
| Sleep Button Action | Sleep
Network
| Network
| Network Name | DESKTOP-O18FSDF
| User Name | KKV1
| User Role | Administrator
| Logon Domain | DESKTOP-O18FSDF
| Interface 1
| Network Chip Vendor | Realtek Semiconductor
| Network Chip | RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor | Micro-Star International Co Ltd (MSI)
| Parent Device | AMD 400 Series Chipset PCIe Port
| Bus Type | PCI Express 1.0 x1 2.5 GT/s (Current: x1 2.5 GT/s)
| Bus Bandwidth | 0.25 GB/sec (Current: 0.25 GB/sec)
| Description | Realtek PCIe GbE Family Controller
| Adapter Manufacturer | Micro-Star INTL CO., LTD.
| MAC Address | 2C-F0-5D-D2-A7-22
| Adapter Type | Ethernet
| Link Speed | 1000.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Enabled | Yes
| DHCP Server | 192.168.1.1
| IP Address | 192.168.1.15
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 192.168.1.1
| DNS Server | 192.168.1.1
Monitor
| Monitor
| Monitor Vendor | BenQ
| Monitor Model | BenQ GW2470
| Viewable Size | 23.8" (60.4 sm)
| Serial Number | 21573
| Manufacture Date | August 2016
| EDID Version | 1.3
| Monitor ID | BNQ78D9
| Aspect Ratio | 16:9
| Horizontal Size | 527 mm
| Vertical Size | 296 mm
| Gamma Factor | 2.200
| Display Type | RGB Color
| Input Signal | Digital
| Internal Model | BenQ GW2470
| Internal Number | K8G00916019
| Vertical Frequency | 50-76 Hz
| Horizontal Frequency | 30-83 kHz
| Current Resolution | 1920x1080 32bpp @ 60 Hz
| Recommended Resolution | 1920x1080 @ 60 Hz
| Parent Device | NVIDIA GeForce RTX 3060 Ti LHR [GA104]
| DPMS Features
| Active Off | Supported
| Suspend | Not Supported
| Standby | Not Supported
| Supported Modes
| Mode 1 | 640x480 @ 60 Hz (VGA)
| Mode 2 | 640x480 @ 75 Hz (VESA)
| Mode 3 | 720x400 @ 70 Hz (VGA)
| Mode 4 | 800x600 @ 60 Hz (VESA)
| Mode 5 | 800x600 @ 75 Hz (VESA)
| Mode 6 | 832x624 @ 75 Hz (Mac II)
| Mode 7 | 1024x768 @ 60 Hz (VESA)
| Mode 8 | 1024x768 @ 75 Hz (VESA)
| Mode 9 | 1152x870 @ 75 Hz (Mac II)
| Mode 10 | 1280x720 @ 60 Hz
| Mode 11 | 1280x800 @ 60 Hz
| Mode 12 | 1280x1024 @ 60 Hz
| Mode 13 | 1280x1024 @ 75 Hz (VESA)
| Mode 14 | 1600x900 @ 60 Hz
| Mode 15 | 1680x1050 @ 60 Hz
| Mode 16 | 1920x1080 @ 60 Hz (Recommended)
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard monitor types)
| Device Description | Generic PnP Monitor
| Friendly Name | Generic Monitor (BenQ GW2470)
| Device Class | Monitor
| Driver Provider | Microsoft
| Driver Version | 10.0.22621.3672
| Driver Date | 6-21-2006
| Inf File | monitor.inf
| Service Name | monitor
| Hardware ID | MONITOR\BNQ78D9
| Compatible ID | *PNP09FF
| Parent ID | PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
Video Card
| Video
| Video Chip Vendor | NVIDIA Corporation
| Video Chip | GeForce RTX 3060 Ti LHR [GA104]
| Subsystem Vendor | Micro-Star International Co Ltd (MSI)
| Subsystem ID | MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
| Hardware ID | VEN_10DE&DEV_2489
| Revision | A1h
| GPU Type | Desktop Discrete
| Memory
| Video Memory Size | 8 GB
| Memory Type | GDDR6 (Hynix)
| Bus Width | 256-bit
| Architecture
| Architecture | Ampere
| Code Name | GA104 A1h
| GPU Variant | GA104-202
| Unified Shaders | 4864
| Texture Mapping Units (TPU) | 152
| Render Output Units (ROPS) | 64
| Streaming Multiprocessors | 38
| Tensor Cores | 152
| RT Cores | 38
| Level 1 Cache | 4.75 MB
| Level 2 Cache | 4 MB
| GPU Manufacturer | Samsung
| Manufacturing Process | 8 nm
| Transistor Count | 17400 million
| Die Size | 392 mm2
| Package Type | BGA-2713
| Max TDP | 200.0 Wattes
| Launch Date | May, 2021
| Base Clocks
| Base Core Clock | 1410 MHz
| Base Memory Clock | 1750 MHz (Effective: 14000 MHz)
| Memory Bandwidth | 448.0 GB/s
| Boost Clocks
| Boost Core Clock | 1695 MHz
| Boost Memory Clock | 1750 MHz (Effective: 14000 MHz)
| Memory Bandwidth | 448.0 GB/s
| Theoretical Performance
| Estimated Speed | 35% of GeForce GTX 4090
| Pixel Fillrate | 108.5 GPixel/s
| Texture Fillrate | 257.6 GTexel/s
| BIOS
| Bootup Message | PG190 SKU 12 VGA BIOS MSINV397MH.520
| Video BIOS Version | Version 94.04.46.00.D2
| Video BIOS Date | 05/19/21
| BIOS Copyright | Copyright (C) 1996-2021 NVIDIA Corp.
| Board Model | GPU Board
| API Supported
| DirectX Version | 12 (12_2)
| OpenGL Version | 4.6
| Shader Model | 6.7
| Vulkan Version | 1.3
| CUDA Version | 8.6
| OpenCL Version | 3.0
| Other
| Driver Version | R572.16
| Parent Device | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x16 8.0 GT/s (Current: x16 8.0 GT/s)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| RAMDAC Type | Integrated RAMDAC
| Hardware Monitoring
| Core Temperature | 40 °C (104 °F)
| Current Core Clock | 210.0 MHz
| Current Video Engine Clock | 555 MHz
| Current Memory Clock | 101.0 MHz (Effective: 808.0 MHz)
| Core Usage | 0 %
| Memory Usage | 5 %
| Memory Controller Usage | 34 %
| Video Engine Usage | 0 %
| Bus Interface Load | 0 %
| Performance Profile 0
| Core Clock | 2100 MHz
| Memory Clock | 7001 MHz
| Performance Profile 2
| Core Clock | 6801 MHz
| Memory Clock | 6801 MHz
| Performance Profile 3
| Core Clock | 210 MHz
| Memory Clock | 5001 MHz
| Performance Profile 5
| Core Clock | 210 MHz
| Memory Clock | 810 MHz
| Performance Profile 8
| Core Clock | 210 MHz
| Memory Clock | 405 MHz
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | NVIDIA
| Device Description | NVIDIA GeForce RTX 3060 Ti
| Device Class | Display
| Device Location | PCI bus 41, device 0, function 0
| Driver Provider | NVIDIA
| Driver Version | 32.0.15.7216
| Driver Date | 1-26-2025
| Inf File | oem13.inf
| Service Name | nvlddmkm
| Hardware ID | PCI\VEN_10DE&DEV_2489&SUBSYS_39721462&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_2489&REV_A1
| Parent ID | PCI\VEN_1022&DEV_1483&SUBSYS_12341022&REV_00
Hardware Monitoring
| Processor
| Processor | AMD Ryzen 5 5600 3500 MHz
| Core Voltage | 1.113 V
| Core Voltage (SVI2 TFN) | 1.119 V
| SoC Voltage (SVI2 TFN) | 1.075 V
| Package Temperature | 48 °C (118 °F)
| CCD1 Temperature | 48 °C (118 °F)
| SoC Temperature | 40 °C (104 °F)
| L3 Cache Temperature | 38 °C (100 °F)
| Package Power | 27.1 Wattes
| Cores Power | 3.0 Wattes
| SoC Power | 12.4 Wattes
| VDDIO Mem Power | 9.2 Wattes
| VDD18 Power | 0.9 Wattes
| FSB Clock | 100.0 MHz
| Core 1
| Temperature Core | 38 °C (100 °F)
| Core Power | 0.5 Wattes
| Core Clock | 3560.0 MHz (Original: 3500 MHz)
| Multiplier | 35.6
| Core 2
| Temperature Core | 39 °C (102 °F)
| Core Power | 0.5 Wattes
| Core Clock | 4450.1 MHz (Original: 3500 MHz)
| Multiplier | 44.5
| Core 3
| Temperature Core | 39 °C (102 °F)
| Core Power | 0.7 Wattes
| Core Clock | 4450.1 MHz (Original: 3500 MHz)
| Multiplier | 44.5
| Core 4
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.0 Wattes
| Core Clock | 3560.0 MHz (Original: 3500 MHz)
| Multiplier | 35.6
| Core 5
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.0 Wattes
| Core Clock | 3560.0 MHz (Original: 3500 MHz)
| Multiplier | 35.6
| Core 6
| Temperature Core | 37 °C (99 °F)
| Core Power | 0.1 Wattes
| Core Clock | 3560.0 MHz (Original: 3500 MHz)
| Multiplier | 35.6
| Video Card
| Video Chip | GeForce RTX 3060 Ti LHR [GA104]
| Core Temperature | 40 °C (104 °F)
| Current Core Clock | 210.0 MHz (Original: 1410 MHz)
| Current Memory Clock | 101.0 MHz (Original: 1750 MHz)
| Core Usage | 0 %
| Memory Usage | 5 %
| Memory Controller Usage | 34 %
| Video Engine Usage | 0 %
| Bus Interface Load | 0 %
| Disk Drive 1
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Temperature | 39 °C (102 °F)
| Disk Drive 2
| Disk Model | Samsung SSD 970 EVO Plus 1TB
| Disk Temperature | 41 °C (106 °F)
| Total Host Writes | 10.77 TB
| Total Host Reads | 18.87 TB
Drivers Troubleshooter
| List of Problem Devices
| Problem Device 1
| Device Type | USB Device
| Vendor (04A9h) | Canon
| Device (2660h) | LaserBase MF3110 Scanner/Printer
| Manufacturer | Canon,Inc.
| Product | MF3110
| Device Version | 0.0
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Hardware ID | VID_04A9&PID_2660
| Protocol (00h) | Unknown
| Interface 1
| Class (FFh) | Vendor Specific Class
| SubClass (00h) | Unknown
| Protocol (FFh) | Unknown
| Interface |
| Driver
| Driver Status | The drivers for this device are not installed (28)
| Device Description | MF3110
| Device Location | 0003.0000.0000.011.000.000.000.000.000
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000&MI_00
| Compatible ID | USB\COMPAT_VID_04a9&Class_ff&SubClass_00&Prot_ff
| Parent ID | USB\VID_04A9&PID_2660&REV_0000
Disk Diagnostics
| Disk 1 Status
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Buffer Size | 32767.5 kB
| Location | AMD 400 Series Chipset SATA Controller
| Disk Temperature | 39 °C (102 °F)
| Reallocated Sectors | 3
| Disk Health Status | Poor
| Disk 2 Status
| Disk Model | Samsung SSD 970 EVO Plus 1TB
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | NVMe 1.3.0
| Serial Number | S6P7NF0T435103B
| Controller Revision | 4B2QEXM7
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Buffer Size | Unknown
| Location | Samsung Electronics Co Ltd NVMe SSD Controller SM981/PM981/PM983
| Disk Temperature | 41 °C (106 °F)
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 10.77 TB
| Total Host Reads | 18.87 TB
Windows
| Windows
| Operating System | MS Windows 11 Professional x64 Edition
| OS Type | x64 (64-bit)
| Version | 22H2
| Build Number | 10.0.22621.4317
| OS Language | Russian (Russia)
| Windows Folder | J:\Windows
| Installation Date | 03 February 2025
| Kernel Type | Multiprocessor Free
| Registered Owner | KKV1
| Registered Organization |
| Product ID | 00330-80000-00000-AA702
| Product Key | XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
| System UpTime | 0 Hour(s) 32 Minutes 41 Seconds
| IE Version | 9.11.22621.0
| DirectX Version | DirectX 12 (10.00.22621.1)
| Regional Settings
| Country | Russia
| Language | Russian
| Time Zone | Central America Standard Time (GMT-6)
| Currency Name | Russian Ruble
| Measurment System | Metric
| ANSI Code Page | 1251
| OEM Code Page | 866
Installed Programs
| Installed Programs
| Program Name | Version | Publisher | Date | Size |
| ASTRA32 - Advanced System Information Tool | 4.22 | Sysinfo Lab |  |  |
Installed Hotfixes
| Installed Hotfixes
| Definition Update for Microsoft Office 2013 (KB2760587) 64-Bit Edition |
| Security Update for Microsoft Windows (KB5044285) |
| Security Update for Microsoft Windows (KB5046247) |