************************************************************
** ENU *************************************************** 
************************************************************
*
*  Intel (R) SMBus Driver
*  Version: 6.8.1.2
*  Installation Readme
*
*  This document makes references to unannounced products
*  being developed by Intel.  There are some restrictions 
*  on how these products may be used and what information 
*  may be disclosed to others.  Please read the Disclaimer 
*  section at the bottom of this document, and contact your 
*  Intel field representative if you would like additional 
*  information.
*
************************************************************
************************************************************

************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************

This document contains the following sections:

1.  System Requirements
2.  Localized Language Abbreviations
3.  Installing and Executing the Software
4.  Verifying Installation of the Software
5.  Identifying the Software Version Number
6.  Installation Switches Available

************************************************************
* 1.  SYSTEM REQUIREMENTS
************************************************************

1. The system must contain an Intel Chipset with an
integrated SMBus Controller.

2. One of the following operating systems must be installed
    on the system:
    
    Windows* XP
    Windows* Server 2003
    Windows* Vista*
    Windows* 7

To verify which operating system has been installed onto the 
target system, follow the steps below:
  a. Click on Start.
  b. Select Settings.
  c. Select Control Panel.
  d. Double-click on the System icon.
  e. Click on the General tab in the System Properties window.
  f. Verify which OS has been installed by reading the System information.

3. It is recommended that the kit software be installed on systems
   with at least 32 MB of system memory.

4. It is recommended that there be sufficient hard disk 
   space in the <TEMP> directory (typically C:\WINDOWS\TEMP)
   on the system, in order to install this software.

Please check with your system provider to determine the 
operating system and Intel chipset used in your system.
This driver will not be supported with any other hardware or 
software that is not listed above.  


************************************************************
* 2.  LOCALIZED LANGUAGE ABBREVIATIONS
************************************************************

Not available.


************************************************************
* 3.  INSTALLING AND EXECUTING THE SOFTWARE
************************************************************

"Have Disk" Install (Windows XP, Windows Server 2003 and Windows Vista):

1.  Locate the device in the device manager.  The device will usually
    be listed as an Other PCI Device, or under the System Devices.  If the
    device does not exist, this may be due to the controller being disabled 
    in the BIOS.  In this case an installer will be needed to start the 
    driver as a service or through registry modifications.  Support for 
    these modes of installation are currently not supported.  

2.  Enter the device properties and select update or reinstall driver.

3.  Specify the path to the SMBus driver and INF file.  Care must be taken to
    ensure that the new driver is actually installed.  Since the SMBus 2.0 
    driver is not signed, the OS will usually attempt to install the 
    chipset INF driver.  On Win2000 there is a check box indicating install 
    another driver.  This should be set and the proper driver selected. 

4.  If the driver installed properly the device manager should indicate 
    an SMBus2.0 driver.  

Automated Install:

1. Check the System Requirements. A supported operating 
    system must be fully installed and running on the system before
    running this software.

2. Close any running applications. Otherwise, you may
    experience difficulties.

3.  Run the installation program:
	Setup.EXE

4.  Follow the on-screen instructions.

5.  Select OK to restart if required.

6.  Follow the on-screen instructions and use the default
    settings to complete the setup, once the operating
    system has rebooted.

Note:  It is recommended that any earlier versions of the installer
       be uninstalled prior to installing the new driver package.


************************************************************
* 4.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************

Windows XP, Windows Server 2003 and Windows vista:
	To determine if the driver is loaded and working properly,
	enter the device manager and locate the SMBus Controller under
 	the System Devices.  If "Intel(R) SMBus 2.0 Driver" is specified
	at the end of the line and there are no yellow bangs, then
	the driver is loaded.

Silent Mode Install:
	To determine whether the install was successful, verify the 
	'install' value in the registry key HKLM\Software\Intel\SMBus

	The following table describes the various parameter values:

	Value		Type		Data		Description
	--------	------		------		---------------
	"install"	String		"success"	Successful installation
					"failure"	Unsuccessful installation

	"reboot"	String		"Yes"		A reboot is required to 
							complete installation.
					"No"		No reboot is required to 
							complete installation.

	"version"	String		<varies>	Current version number of 
							the Intel(R) SMBus
							Installer Software.
	

************************************************************
* 5.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************

The software version of each application file can be 
obtained by querying the corresponding file's properties
under Explorer

1. Run the Windows Explorer application.

2. Open the application directory (i.e., the directory 
    selected during the installation).  The default
    installation directory for the driver is C:\Windows\System32\Drivers.

3. Click on "intelsmb.sys" 

4. Select the Properties item.

5. Select the Version tab.

6. The software version should be listed in the Product Version
    area of the dialog and/or the top of the dialog.


************************************************************
* 6.  INSTALLATION SWITCHES AVAILABLE
************************************************************

The switches in the .EXE file have the following syntax.
Switches are not case sensitive and may be specified
in any order (except for the  -s  switch).  Switches must
be separated by spaces.

setup.exe -silent -b -overwrite -nolog -nolic

-b         - When a reboot is necessary, this switch forces a system
             reboot after the installation completes.  In verbose 
             mode, the absence of this switch will prompt the user 
             to reboot.  In silent mode, the absence of this switch 
             forces the Setup.exe installer to complete without rebooting 
             (the user must manually reboot to conclude the
             installation process).
-nolic	   - In verbose mode, suppresses the display of the license 
             agreement screen.
-nolog	   - Suppresses the creation of the install log file (SMBusIns.log).
-overwrite - Installs the SMBus driver regardless of the version of 
             the currently installed driver.   In verbose mode, the absence 
             of this switch will prompt the user to confirm overwrite of
             a newer driver.  In silent mode, the absence of this switch 
             means that the installation will abort any attempts to 
             regress the revision of the SMBus driver.
-silent	   - Run in silent mode. The absence of this switch causes the 
             install to be performed in verbose mode.

EXAMPLES:

SETUP EXECUTABLE

setup.exe -silent      - Silent Mode Install
setup.exe -overwrite   - Verbose Mode Install. Overwrites current driver version


************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, including 
liability or warranties relating to fitness for a particular 
purpose, merchantability or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  Intel 
reserves the right to make changes to this document at any 
time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-2010


