# Ejecutando TestDisk

### From CGSecurity

## Inicio de TestDisk

Cuando TestDisk es ejecutado, puede ver la frase `Please wait...` en su pantalla hasta que se han juntado datos suficientes del BIOS ó el SO para obtener la lista de discos rígidos.

    TestDisk 6.6-WIP, Data Recovery Utility, Febrero de 2007
    Christophe GRENIER <grenier@cgsecurity.org>
    http://www.cgsecurity.org

    TestDisk is a data recovery designed to help recover lost partitions
    and/or make non-booting disks bootable again when these symptoms
    are caused by faulty software, certain types of viruses or human error.
    It can also be used to repair some filesystem errors.

    Information gathered during TestDisk use can be recorded for later
    review. If you choose to create the text file, testdisk.log , it
    will contain TestDisk options, technical information and various
    outputs; including any folder/file names TestDisk was used to find and
    list onscreen.

    Use arrow keys to select, then press Enter key:
    [ Create ]  Create a new log file
    [ Append ]  Append information to log file
    [ No Log ]  Don't record anything

    TestDisk 6.5-WIP, Data Recovery Utility, October 2006
    Christophe GRENIER <grenier@cgsecurity.org>
    http://www.cgsecurity.org

      TestDisk is free software, and
    comes with ABSOLUTELY NO WARRANTY.

    Select a media (use Arrow keys, then press Enter):
    Disk /dev/sda - 120 GB / 111 GiB
    Disk /dev/sdb - 120 GB / 111 GiB

    [Proceed ]  [  Quit  ]

    Note: Disk capacity must be correctly detected for a successful recovery.
    If a disk listed above has incorrect size, check HD jumper settings, BIOS
    detection, and install the latest OS patches and disk drivers.

Si el tamaño reportado no es igual al tamaño del disco, ejemplo, un disco de 120 GB es reconocido como solamente uno de 32 GB, revise los seteos del BIOS de su disco y los jumpers en el disco. En la mayoría de los discos grandes, hay jumpers que limitan el tamaño a sólo 32 u 8 GB. Si su HD es detectado como de 130 GB solamente, puede no estar disponible el soporte para LBA48 en su sistema operativo, lea Notas de SO para más información.

El próximo paso es seleccionar el tipo de tabla de partición

    TestDisk 6.5-WIP, Data Recovery Utility, November 2005
    Christophe GRENIER <grenier@cgsecurity.org>
    http://www.cgsecurity.org

    Disk /dev/sda - 120 GB / 111 GiB

    Please select the partition table type, press ENTER when done.
    [ Intel ]  Intel/PC partition
    [ Mac   ]  Apple partition map
    [ None  ]  Non partitioned media
    [ Sun   ]  Sun Solaris partition
    [ XBox  ]  XBox partition

    Note: Do NOT select 'None' for media with only a single partition. It's very
    rare for a drive to be 'Non-partitioned'.

## Items de Menú de TestDisk

- Analize Analiza la estructura de la partición actual y busca particiones perdidas
- Utilidades avanzadas de Sistemas de Archivos
  - FAT: Reparación de sector de Boot y FAT
  - NTFS: Reparación de sector de Boot y MFT
  - EXT2/EXT3: Busca el Backup SuperBlock
- Geometry Cambiar geometría del disco
- Options Modificar opciones
- MBR Code Escribir el código MBR de TestDisk al primer sector
- Delete Borrar todos los datos en la tabla de partición

Volver a la página principal de TestDisk (Castellano)

Category: Data Recovery

##### Data Recovery

- TestDisk
- PhotoRec
- download